# Non-Referenced Macros for: leds_autoprog.h

Return to Index

## Non-Referenced Macros:

- Active [1145]: `ADDR_MSK` `ADDR_OFFSET` `ALL_CHANNELS` `AND` `APATTERNT10_T` `APATTERNT11_T` `APATTERNT12_T` `APATTERNT13_T` `APATTERNT14_T` `APATTERNT15_T` `APATTERNT16_T` `APATTERNT17_T` `APATTERNT18_T` `APATTERNT19_T` `APATTERNT20_T` `APATTERNT21_T` `APATTERNT22_T` `APATTERNT23_T` `APATTERNT24_T` `APATTERNT25_T` `APATTERNT26_T` `APATTERNT27_T` `APATTERNT28_T` `APATTERNT29_T` `APATTERNT30_T` `APATTERNT31_T` `APATTERNT32_T` `APATTERNT33_T` `APATTERNT34_T` `APATTERNT35_T` `APATTERNT36_T` `APATTERNT37_T` `APATTERNT38_T` `APATTERNT39_T` `APATTERNT3_T` `APATTERNT40_T` `APATTERNT41_T` `APATTERNT42_T` `APATTERNT43_T` `APATTERNT44_T` `APATTERNT45_T` `APATTERNT46_T` `APATTERNT47_T` `APATTERNT48_T` `APATTERNT49_T` `APATTERNT4_T` `APATTERNT50_T` `APATTERNT51_T` `APATTERNT52_T` `APATTERNT53_T` `APATTERNT54_T` `APATTERNT55_T` `APATTERNT56_T` `APATTERNT57_T` `APATTERNT58_T` `APATTERNT59_T` `APATTERNT5_T` `APATTERNT60_T` `APATTERNT61_T` `APATTERNT62_T` `APATTERNT63_T` `APATTERNT64_T` `APATTERNT6_T` `APATTERNT7_T` `APATTERNT8_T` `APATTERNT9_T` `APatternT10(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,...)` `APatternT11(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,...)` `APatternT12(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,...)` `APatternT13(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,...)` `APatternT14(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,...)` `APatternT15(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,...)` `APatternT16(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,...)` `APatternT17(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,...)` `APatternT18(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,...)` `APatternT19(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,...)` `APatternT20(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,...)` `APatternT21(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,...)` `APatternT22(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,...)` `APatternT23(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,...)` `APatternT24(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,...)` `APatternT25(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,...)` `APatternT26(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,...)` `APatternT27(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,...)` `APatternT28(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,...)` `APatternT29(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,...)` `APatternT3(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,...)` `APatternT30(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,...)` `APatternT31(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,...)` `APatternT32(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,...)` `APatternT33(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,...)` `APatternT34(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,...)` `APatternT35(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,...)` `APatternT36(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,...)` `APatternT37(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,...)` `APatternT38(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,...)` `APatternT39(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,...)` `APatternT4(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,...)` `APatternT40(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,...)` `APatternT41(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,...)` `APatternT42(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,...)` `APatternT43(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,...)` `APatternT44(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,...)` `APatternT45(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,...)` `APatternT46(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,...)` `APatternT47(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,...)` `APatternT48(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,...)` `APatternT49(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,...)` `APatternT5(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,...)` `APatternT50(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,...)` `APatternT51(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,...)` `APatternT52(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,...)` `APatternT53(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,...)` `APatternT54(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,...)` `APatternT55(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,...)` `APatternT56(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,...)` `APatternT57(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,...)` `APatternT58(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,...)` `APatternT59(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,...)` `APatternT6(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,...)` `APatternT60(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,...)` `APatternT61(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,...)` `APatternT62(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,...)` `APatternT63(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,T63,...)` `APatternT64(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,T63,T64,...)` `APatternT7(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,...)` `APatternT8(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,...)` `APatternT9(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,...)` `APatternTE1(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,...)` `APatternTE10(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,...)` `APatternTE11(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,...)` `APatternTE12(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,...)` `APatternTE13(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,...)` `APatternTE14(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,...)` `APatternTE15(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,...)` `APatternTE16(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,...)` `APatternTE17(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,...)` `APatternTE18(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,...)` `APatternTE19(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,...)` `APatternTE2(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,...)` `APatternTE20(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,...)` `APatternTE21(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,...)` `APatternTE22(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,...)` `APatternTE23(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,...)` `APatternTE24(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,...)` `APatternTE25(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,...)` `APatternTE26(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,...)` `APatternTE27(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,...)` `APatternTE28(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,...)` `APatternTE29(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,...)` `APatternTE3(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,...)` `APatternTE30(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,...)` `APatternTE31(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,...)` `APatternTE32(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,...)` `APatternTE33(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,...)` `APatternTE34(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,...)` `APatternTE35(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,...)` `APatternTE36(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,...)` `APatternTE37(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,...)` `APatternTE38(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,...)` `APatternTE39(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,...)` `APatternTE4(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,...)` `APatternTE40(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,...)` `APatternTE41(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,...)` `APatternTE42(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,...)` `APatternTE43(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,...)` `APatternTE44(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,...)` `APatternTE45(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,...)` `APatternTE46(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,...)` `APatternTE47(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,...)` `APatternTE48(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,...)` `APatternTE49(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,...)` `APatternTE5(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,...)` `APatternTE50(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,...)` `APatternTE51(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,...)` `APatternTE52(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,...)` `APatternTE53(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,...)` `APatternTE54(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,...)` `APatternTE55(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,...)` `APatternTE56(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,...)` `APatternTE57(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,...)` `APatternTE58(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,...)` `APatternTE59(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,...)` `APatternTE6(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,...)` `APatternTE60(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,...)` `APatternTE61(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,...)` `APatternTE62(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,...)` `APatternTE63(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,T63,...)` `APatternTE64(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,T63,T64,...)` `APatternTE7(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,...)` `APatternTE8(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,...)` `APatternTE9(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,...)` `AmpelX(LED,InCh)` `AndreaskrLT(LED,Single_Cx,InCh,MaxBrightness,LT_Time,FadeTime,OnTime)` `AndreaskrLT3(LED,Single_Cx,InCh,MaxBrightness,LT_Time,FadeTime,OnTime)` `AndreaskrLT3_RGB(LED,InCh,MaxBrightness,LT_Time,FadeTime,OnTime)` `AndreaskrLT_RGB(LED,InCh,MaxBrightness,LT_Time,FadeTime,OnTime)` `AndreaskrRGB(LED,InCh)` `Andreaskreuz(LED,Cx,InCh)` `BIN_INCH_TO_TMPVAR1_T` `B_GREEN` `B_RED` `B_TAST` `Bin_InCh_to_TmpVar1(FirstInCh,InCh_Cnt)` `Blink2(LED,Cx,InCh,Pause,Act,Val0,Val1)` `Blink3(LED,Cx,InCh,Pause,Act,Val0,Val1,Off)` `Blinker(LED,Cx,InCh,Period)` `BlinkerHD(LED,Cx,InCh,Period)` `BlinkerInvInp(LED,Cx,InCh,Period)` `BlueLight1(LED,Cx,InCh)` `BlueLight2(LED,Cx,InCh)` `Button(LED,Cx,InCh,Duration,Val0,Val1)` `ButtonFunc(DstVar,InCh,Duration)` `ButtonNOff(LED,Cx,InCh,Duration,Val0,Val1)` `C12` `C23` `CALCULATE_t10` `CALCULATE_t4` `CALCULATE_t4w` `CANDLE1` `CANDLE2` `CANDLE3` `CF_BINARY` `CF_INV_ENABLE` `CF_INV_INPUT` `CF_LOCAL_VAR` `CF_ONLY_LOCALVAR` `CF_PINGPONG` `CF_RANDOM` `CF_RESET_LONG` `CF_ROTATE` `CF_SKIP0` `CF_UP_DOWN` `CM_NORMAL` `COLOR0` `COLOR1` `COLOR2` `COLOR3` `COLOR4` `COLOR5` `COLOR_GASL_B` `COLOR_GASL_D` `COLOR_NEON_B` `COLOR_NEON_D` `COLOR_NEON_M` `COLOR_SINGLE` `COLOR_SINGLE_D` `COLOR_TV0_A` `COLOR_TV0_B` `COLOR_TV1_A` `COLOR_TV1_B` `CONST_T` `COPYLED_OFF` `COPYLED_OFF_ONCE` `COPYLED_T` `COUNTER_ID` `COUNTER_T` `CPX_ANALOG_INPUT` `CPX_ANALOG_LIMMITS` `CPX_LED_ASSIGNEMENT` `C_ALL` `C_BLUE` `C_CYAN` `C_GREEN` `C_RED` `C_WHITE` `C_YELLOW` `Charlie_Binary(LED,InCh,BinStates)` `Charlie_Buttons(LED,InCh,States)` `ConstrWarnLight10(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitE)` `ConstrWarnLight11(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitE)` `ConstrWarnLight12(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitE)` `ConstrWarnLight13(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitE)` `ConstrWarnLight14(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitE)` `ConstrWarnLight15(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitE)` `ConstrWarnLight3(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitE)` `ConstrWarnLight4(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitE)` `ConstrWarnLight5(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitE)` `ConstrWarnLight6(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitE)` `ConstrWarnLight7(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitE)` `ConstrWarnLight8(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitE)` `ConstrWarnLight9(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitE)` `ConstrWarnLightFlash10(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitT,WaitE)` `ConstrWarnLightFlash11(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitT,WaitE)` `ConstrWarnLightFlash12(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitT,WaitE)` `ConstrWarnLightFlash13(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitT,WaitE)` `ConstrWarnLightFlash14(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitT,WaitE)` `ConstrWarnLightFlash15(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitT,WaitE)` `ConstrWarnLightFlash3(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitT,WaitE)` `ConstrWarnLightFlash4(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitT,WaitE)` `ConstrWarnLightFlash5(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitT,WaitE)` `ConstrWarnLightFlash6(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitT,WaitE)` `ConstrWarnLightFlash7(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitT,WaitE)` `ConstrWarnLightFlash8(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitT,WaitE)` `ConstrWarnLightFlash9(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitT,WaitE)` `ConstrWarnLightRGB6(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitT,WaitE)` `CopyLED(LED,InCh,SrcLED)` `Counter(Mode,InCh,Enable,TimeOut,...)` `DISABLE` `Def_Neon_Misha(LED,InCh,Var,Min_Delay,Max_Delay)` `DepSignal4(LED,InCh,MaxB128)` `DepSignal4Bin(LED,InCh,MaxB128)` `DepSignal4Bin_RGB(LED,InCh,MaxB128)` `DepSignal4_RGB(LED,InCh,MaxB128)` `ENABLE` `EXT_PROC_BASE_T` `EntrySignal3(LED,InCh,MaxB128)` `EntrySignal3Bin(LED,InCh,MaxB128)` `EntrySignal3Bin_RGB(LED,InCh,MaxB128)` `EntrySignal3_RGB(LED,InCh)` `EntrySignal3_RGB_B(LED,InCh,MaxBrightness)` `EntrySignal3_RGB_BT(LED,InCh,MaxBrightness,FadeTime)` `EntrySignal3_RGB_T(LED,InCh,FadeTime)` `FASTLED_INTERNAL` `FIRE_T` `Fire(LED,InCh,LedCnt,Brightness)` `Flash(LED,Cx,InCh,Var,MinTime,MaxTime)` `GAS_LIGHT` `GAS_LIGHT1` `GAS_LIGHT1D` `GAS_LIGHT2D` `GAS_LIGHT3` `GAS_LIGHT3D` `GAS_LIGHTD` `GEN_BUTTON_RELEASE` `GEN_BUTTON_RELEASE_COM` `GasLights(LED,InCh,...)` `GasLights_Inv(LED,InCh,...)` `GleissperrsignalBin_RGB(LED,InCh,MaxB32)` `Gleissperrsignal_RGB(LED,InCh,MaxB32)` `HP_2_2Bin_RGB(LED,InCh,MaxB16)` `HP_2_2_RGB(LED,InCh,MaxB16)` `HS_5_PlusBin_RGB(LED,InCh,MaxB64)` `HS_5_Plus_RGB(LED,InCh,MaxB64)` `HS_5lBin_RGB(LED,InCh,MaxB64)` `HS_5l_RGB(LED,InCh,MaxB64)` `HS_5rBin_RGB(LED,InCh,MaxB64)` `HS_5r_RGB(LED,InCh,MaxB64)` `HS_EinfachBin_RGB(LED,InCh,MaxB32)` `HS_Einfach_RGB(LED,InCh,MaxB32)` `Herz_2MoRelais(LED,InCh,Single_Cx,DelayHerz2)` `Herz_2MoRelais_I(LED,InCh,Single_Cx,DelayHerz2)` `Herz_BiRelais(LED,InCh,Single_Cx,DelayHerz1)` `Herz_BiRelais_I(LED,InCh,Single_Cx,DelayHerz1)` `Herz_BiRelais_I_V1_AB(LED,InCh,DelayHerz1)` `Herz_BiRelais_I_V1_CD(LED,InCh,DelayHerz1)` `Herz_BiRelais_I_V1_EF(LED,InCh,DelayHerz1)` `Herz_BiRelais_V1_AB(LED,InCh,DelayHerz1)` `Herz_BiRelais_V1_CD(LED,InCh,DelayHerz1)` `Herz_BiRelais_V1_EF(LED,InCh,DelayHerz1)` `Herz_MoRelais(LED,InCh,Single_Cx,DelayHerz1,TmpNr)` `Herz_MoRelais_I(LED,InCh,Single_Cx,DelayHerz1,TmpNr)` `House(LED,InCh,On_Min,On_Limit,...)` `HouseT_Inv(LED,InCh,On_Min,On_Limit,Min_T,Max_T,...)` `House_Inv(LED,InCh,On_Min,On_Limit,...)` `INCH_TO_TMPVAR1_T` `INCH_TO_TMPVAR_T` `INP_OFF` `IS_COUNTER` `IS_PULSE` `InCh_to_TmpVar(FirstInCh,InCh_Cnt)` `InCh_to_TmpVar1(FirstInCh,InCh_Cnt)` `InCnt_MSK` `KS_Hauptsignal_Zs3_Zs1(LED,InCh,MaxB128)` `KS_Hauptsignal_Zs3_Zs1Bin(LED,InCh,MaxB128)` `KS_Hauptsignal_Zs3_Zs1Bin_RGB(LED,InCh,MaxB128)` `KS_Hauptsignal_Zs3_Zs1_RGB(LED,InCh,MaxB128)` `KS_Hauptsignal_Zs3_Zs6_Zs1(LED,InCh,MaxB128)` `KS_Hauptsignal_Zs3_Zs6_Zs1Bin(LED,InCh,MaxB128)` `KS_Hauptsignal_Zs3_Zs6_Zs1Bin_RGB(LED,InCh,MaxB128)` `KS_Hauptsignal_Zs3_Zs6_Zs1_RGB(LED,InCh,MaxB128)` `KS_Vorsignal_Zs3V(LED,InCh,MaxB128)` `KS_Vorsignal_Zs3VBin(LED,InCh,MaxB128)` `KS_Vorsignal_Zs3VBin_RGB(LED,InCh,MaxB128)` `KS_Vorsignal_Zs3V_RGB(LED,InCh,MaxB128)` `LAST_APATTERN_T` `LAST_PATTERN_T` `LEDS_PER_CHANNEL` `LOGIC_T` `Leuchtfeuer(LED,Cx,InCh)` `LeuchtfeuerALL(LED,InCh)` `Logic(DstVar,...)` `Min` `MobaLedLibPtr_Create(leds)` `MobaLedLib_Copy_to_InpStruct(Src,ByteCnt,ChannelNr)` `MobaLedLib_Create(leds)` `MobaLedLib_Prepare()` `MobaLedLib_Ver` `MonoFlop(DstVar,InCh,Duration)` `MonoFlop2(DstVar0,DstVar1,InCh,Duration)` `MonoFlop2LongReset(DstVar0,DstVar1,InCh,Duration)` `MonoFlopInv(DstVar,InCh,Duration)` `MonoFlopInvLongReset(DstVar,InCh,Duration)` `MonoFlopLongReset(DstVar,InCh,Duration)` `MonoFlopReset(DstVar,InCh,R_InCh,Duration)` `Ms` `NEON_DEF1D` `NEON_DEF2D` `NEON_DEF3D` `NEON_DEF_D` `NEON_LIGHT1` `NEON_LIGHT1D` `NEON_LIGHT1L` `NEON_LIGHT1M` `NEON_LIGHT2` `NEON_LIGHT2D` `NEON_LIGHT2L` `NEON_LIGHT2M` `NEON_LIGHT3` `NEON_LIGHT3D` `NEON_LIGHT3L` `NEON_LIGHT3M` `NEON_LIGHTL` `NEON_LIGHTM` `NEW_LOCAL_VAR_T` `NOT` `New_Local_Var()` `OR` `O_RET_MSG` `PATTERNT10_T` `PATTERNT11_T` `PATTERNT12_T` `PATTERNT13_T` `PATTERNT14_T` `PATTERNT15_T` `PATTERNT16_T` `PATTERNT17_T` `PATTERNT18_T` `PATTERNT19_T` `PATTERNT20_T` `PATTERNT21_T` `PATTERNT22_T` `PATTERNT23_T` `PATTERNT24_T` `PATTERNT25_T` `PATTERNT26_T` `PATTERNT27_T` `PATTERNT28_T` `PATTERNT29_T` `PATTERNT2_T` `PATTERNT30_T` `PATTERNT31_T` `PATTERNT32_T` `PATTERNT33_T` `PATTERNT34_T` `PATTERNT35_T` `PATTERNT36_T` `PATTERNT37_T` `PATTERNT38_T` `PATTERNT39_T` `PATTERNT3_T` `PATTERNT40_T` `PATTERNT41_T` `PATTERNT42_T` `PATTERNT43_T` `PATTERNT44_T` `PATTERNT45_T` `PATTERNT46_T` `PATTERNT47_T` `PATTERNT48_T` `PATTERNT49_T` `PATTERNT4_T` `PATTERNT50_T` `PATTERNT51_T` `PATTERNT52_T` `PATTERNT53_T` `PATTERNT54_T` `PATTERNT55_T` `PATTERNT56_T` `PATTERNT57_T` `PATTERNT58_T` `PATTERNT59_T` `PATTERNT5_T` `PATTERNT60_T` `PATTERNT61_T` `PATTERNT62_T` `PATTERNT63_T` `PATTERNT64_T` `PATTERNT6_T` `PATTERNT7_T` `PATTERNT8_T` `PATTERNT9_T` `PF_INVERT_INP` `PF_NO_SWITCH_OFF` `PF_SLOW` `PM_MODE_MASK` `PM_PINGPONG` `PM_RES` `PM_SEQUENCE_NO_RESTART` `PM_SEQUENCE_STOP` `PM_SEQUENCE_W_ABORT` `PM_SEQUENCE_W_RESTART` `PM_SEQUENZ_NO_RESTART` `PM_SEQUENZ_STOP` `PM_SEQUENZ_W_ABORT` `PM_SEQUENZ_W_RESTART` `PatternT10(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,...)` `PatternT11(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,...)` `PatternT12(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,...)` `PatternT13(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,...)` `PatternT14(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,...)` `PatternT15(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,...)` `PatternT16(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,...)` `PatternT17(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,...)` `PatternT18(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,...)` `PatternT19(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,...)` `PatternT2(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,...)` `PatternT20(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,...)` `PatternT21(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,...)` `PatternT22(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,...)` `PatternT23(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,...)` `PatternT24(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,...)` `PatternT25(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,...)` `PatternT26(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,...)` `PatternT27(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,...)` `PatternT28(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,...)` `PatternT29(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,...)` `PatternT3(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,...)` `PatternT30(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,...)` `PatternT31(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,...)` `PatternT32(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,...)` `PatternT33(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,...)` `PatternT34(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,...)` `PatternT35(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,...)` `PatternT36(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,...)` `PatternT37(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,...)` `PatternT38(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,...)` `PatternT39(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,...)` `PatternT4(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,...)` `PatternT40(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,...)` `PatternT41(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,...)` `PatternT42(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,...)` `PatternT43(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,...)` `PatternT44(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,...)` `PatternT45(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,...)` `PatternT46(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,...)` `PatternT47(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,...)` `PatternT48(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,...)` `PatternT49(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,...)` `PatternT5(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,...)` `PatternT50(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,...)` `PatternT51(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,...)` `PatternT52(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,...)` `PatternT53(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,...)` `PatternT54(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,...)` `PatternT55(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,...)` `PatternT56(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,...)` `PatternT57(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,...)` `PatternT58(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,...)` `PatternT59(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,...)` `PatternT6(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,...)` `PatternT60(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,...)` `PatternT61(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,...)` `PatternT62(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,...)` `PatternT63(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,T63,...)` `PatternT64(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,T63,T64,...)` `PatternT7(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,...)` `PatternT8(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,...)` `PatternT9(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,...)` `PatternTE1(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,...)` `PatternTE10(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,...)` `PatternTE11(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,...)` `PatternTE12(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,...)` `PatternTE13(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,...)` `PatternTE14(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,...)` `PatternTE15(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,...)` `PatternTE16(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,...)` `PatternTE17(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,...)` `PatternTE18(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,...)` `PatternTE19(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,...)` `PatternTE2(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,...)` `PatternTE20(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,...)` `PatternTE21(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,...)` `PatternTE22(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,...)` `PatternTE23(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,...)` `PatternTE24(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,...)` `PatternTE25(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,...)` `PatternTE26(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,...)` `PatternTE27(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,...)` `PatternTE28(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,...)` `PatternTE29(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,...)` `PatternTE3(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,...)` `PatternTE30(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,...)` `PatternTE31(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,...)` `PatternTE32(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,...)` `PatternTE33(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,...)` `PatternTE34(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,...)` `PatternTE35(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,...)` `PatternTE36(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,...)` `PatternTE37(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,...)` `PatternTE38(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,...)` `PatternTE39(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,...)` `PatternTE4(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,...)` `PatternTE40(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,...)` `PatternTE41(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,...)` `PatternTE42(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,...)` `PatternTE43(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,...)` `PatternTE44(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,...)` `PatternTE45(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,...)` `PatternTE46(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,...)` `PatternTE47(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,...)` `PatternTE48(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,...)` `PatternTE49(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,...)` `PatternTE5(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,...)` `PatternTE50(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,...)` `PatternTE51(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,...)` `PatternTE52(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,...)` `PatternTE53(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,...)` `PatternTE54(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,...)` `PatternTE55(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,...)` `PatternTE56(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,...)` `PatternTE57(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,...)` `PatternTE58(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,...)` `PatternTE59(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,...)` `PatternTE6(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,...)` `PatternTE60(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,...)` `PatternTE61(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,...)` `PatternTE62(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,...)` `PatternTE63(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,T63,...)` `PatternTE64(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,T63,T64,...)` `PatternTE7(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,...)` `PatternTE8(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,...)` `PatternTE9(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,...)` `PushButton2I_0_1(InCh,InCh2,LocInCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout)` `PushButton2I_0_2(InCh,InCh2,LocInCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout)` `PushButton2I_0_3(InCh,InCh2,LocInCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout)` `PushButton2I_0_4(InCh,InCh2,LocInCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout)` `PushButton2I_0_5(InCh,InCh2,LocInCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout)` `PushButton2I_RGB_0_1(B_LED,InCh,InCh2,LocInCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,R0,G0,B0,R10,G10,B10,R11,G11,B11)` `PushButton2I_RGB_0_2(B_LED,InCh,InCh2,LocInCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21)` `PushButton2I_RGB_0_3(B_LED,InCh,InCh2,LocInCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21,R30,G30,B30,R31,G31,B31)` `PushButton2I_RGB_0_4(B_LED,InCh,InCh2,LocInCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21,R30,G30,B30,R31,G31,B31,R40,G40,B40,R41,G41,B41)` `PushButton2I_RGB_0_5(B_LED,InCh,InCh2,LocInCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21,R30,G30,B30,R31,G31,B31,R40,G40,B40,R41,G41,B41,R50,G50,B50,R51,G51,B51)` `PushButton2I_w_LED_BL_0_1(B_LED,B_LED_Cx,InCh,InCh2,LocInCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,Val1,BackLight)` `PushButton2I_w_LED_BL_0_2(B_LED,B_LED_Cx,InCh,InCh2,LocInCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,Val1,BackLight)` `PushButton2I_w_LED_BL_0_3(B_LED,B_LED_Cx,InCh,InCh2,LocInCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,Val1,BackLight)` `PushButton2I_w_LED_BL_0_4(B_LED,B_LED_Cx,InCh,InCh2,LocInCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,Val1,BackLight)` `PushButton2I_w_LED_BL_0_5(B_LED,B_LED_Cx,InCh,InCh2,LocInCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,Val1,BackLight)` `PushButton_0_1(InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout)` `PushButton_0_2(InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout)` `PushButton_0_3(InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout)` `PushButton_0_4(InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout)` `PushButton_0_5(InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout)` `PushButton_RGB_0_1(B_LED,InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,R0,G0,B0,R10,G10,B10,R11,G11,B11)` `PushButton_RGB_0_2(B_LED,InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21)` `PushButton_RGB_0_3(B_LED,InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21,R30,G30,B30,R31,G31,B31)` `PushButton_RGB_0_4(B_LED,InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21,R30,G30,B30,R31,G31,B31,R40,G40,B40,R41,G41,B41)` `PushButton_RGB_0_5(B_LED,InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21,R30,G30,B30,R31,G31,B31,R40,G40,B40,R41,G41,B41,R50,G50,B50,R51,G51,B51)` `PushButton_w_LED_0_1(B_LED,B_LED_Cx,InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout)` `PushButton_w_LED_0_2(B_LED,B_LED_Cx,InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout)` `PushButton_w_LED_0_3(B_LED,B_LED_Cx,InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout)` `PushButton_w_LED_0_4(B_LED,B_LED_Cx,InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout)` `PushButton_w_LED_0_5(B_LED,B_LED_Cx,InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout)` `PushButton_w_LED_BL_0_1(B_LED,B_LED_Cx,InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,Val1,BackLight)` `PushButton_w_LED_BL_0_2(B_LED,B_LED_Cx,InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,Val1,BackLight)` `PushButton_w_LED_BL_0_3(B_LED,B_LED_Cx,InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,Val1,BackLight)` `PushButton_w_LED_BL_0_4(B_LED,B_LED_Cx,InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,Val1,BackLight)` `PushButton_w_LED_BL_0_5(B_LED,B_LED_Cx,InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,Val1,BackLight)` `RAM0` `RAM10` `RAM100` `RAM11` `RAM12` `RAM13` `RAM14` `RAM15` `RAM16` `RAM17` `RAM18` `RAM19` `RAM20` `RAM21` `RAM22` `RAM23` `RAM24` `RAM25` `RAM26` `RAM27` `RAM28` `RAM29` `RAM30` `RAM31` `RAM32` `RAM33` `RAM34` `RAM35` `RAM36` `RAM37` `RAM38` `RAM39` `RAM40` `RAM41` `RAM42` `RAM43` `RAM44` `RAM45` `RAM46` `RAM47` `RAM48` `RAM49` `RAM50` `RAM51` `RAM52` `RAM53` `RAM54` `RAM55` `RAM56` `RAM57` `RAM58` `RAM59` `RAM60` `RAM61` `RAM62` `RAM63` `RAM64` `RAM65` `RAM66` `RAM67` `RAM68` `RAM69` `RAM70` `RAM71` `RAM72` `RAM73` `RAM74` `RAM75` `RAM76` `RAM77` `RAM78` `RAM79` `RAM8` `RAM80` `RAM81` `RAM82` `RAM83` `RAM84` `RAM85` `RAM86` `RAM87` `RAM88` `RAM89` `RAM9` `RAM90` `RAM91` `RAM92` `RAM93` `RAM94` `RAM95` `RAM96` `RAM97` `RAM98` `RAM99` `RAMN(n)` `RANDMUX_T` `RANDOM_T` `RECEIVE_LED_COLOR_PER_RS232` `RF_NOT_SAME` `RF_SEQ` `RF_SLOW` `RF_STAY_ON` `RGB_AmpelX(LED,InCh)` `RGB_AmpelXFade(LED,InCh)` `RGB_AmpelX_A(LED,InCh)` `RGB_Heartbeat2(LED,MinBrightness,MaxBrightness)` `RGB_Heartbeat_Color(LED,MinBrightness,MaxBrightness,Color,Duration)` `RGB_Ring(LED,InCh,Brightness,Duration)` `RM_NORMAL` `ROOM_BRIGHT` `ROOM_COL0` `ROOM_COL1` `ROOM_COL2` `ROOM_COL3` `ROOM_COL345` `ROOM_COL4` `ROOM_COL5` `ROOM_COL_CNT` `ROOM_D_RED` `ROOM_TV0` `ROOM_TV1` `RS_FlipFlop(DstVar,R_InCh,S_InCh)` `RS_FlipFlop2(DstVar0,DstVar1,R_InCh,S_InCh)` `RS_FlipFlop2Timeout(DstVar0,DstVar1,R_InCh,S_InCh,Timeout)` `RS_FlipFlopInv(DstVar,R_InCh,S_InCh)` `RS_FlipFlopInvTimeout(DstVar,R_InCh,S_InCh,Timeout)` `RS_FlipFlopTimeout(DstVar,R_InCh,S_InCh,Timeout)` `RandCntMux(DstVar1,DstVarN,InCh,Mode,MinTime,MaxTime)` `RandMux(DstVar1,DstVarN,InCh,Mode,MinTime,MaxTime)` `RandWelding(LED,InCh,Var,MinTime,MaxTime,MinOn,MaxOn)` `Random(DstVar,InCh,Mode,MinTime,MaxTime,MinOn,MaxOn)` `SCHEDULE_T` `SETUP_FASTLED()` `SINGLE_LED1` `SINGLE_LED1D` `SINGLE_LED2` `SINGLE_LED2D` `SINGLE_LED3` `SINGLE_LED3D` `SI_Enable_Sound` `SKIP_ROOM` `SOUND_ADKEY1` `SOUND_ADKEY10` `SOUND_ADKEY2` `SOUND_ADKEY3` `SOUND_ADKEY4` `SOUND_ADKEY5` `SOUND_ADKEY6` `SOUND_ADKEY7` `SOUND_ADKEY8` `SOUND_ADKEY9` `SOUND_JQ6500_ADKEY1_BG` `SOUND_JQ6500_ADKEY1_N` `SOUND_JQ6500_ADKEY2_BG` `SOUND_JQ6500_ADKEY2_N` `SOUND_JQ6500_ADKEY3_BG` `SOUND_JQ6500_ADKEY3_N` `SOUND_JQ6500_ADKEY4_BG` `SOUND_JQ6500_ADKEY4_N` `SOUND_JQ6500_ADKEY5_BG` `SOUND_JQ6500_ADKEY5_N` `SOUND_JQ6500_ADKEY6_BG` `SOUND_JQ6500_ADKEY6_N` `SOUND_JQ6500_ADKEY7_BG` `SOUND_JQ6500_ADKEY7_N` `SOUND_New_ADKEY1` `SOUND_New_ADKEY10` `SOUND_New_ADKEY2` `SOUND_New_ADKEY3` `SOUND_New_ADKEY4` `SOUND_New_ADKEY5` `SOUND_New_ADKEY6` `SOUND_New_ADKEY7` `SOUND_New_ADKEY8` `SOUND_New_ADKEY9` `START_MSG` `START_SEND_INPUTS` `START_VARIABLES` `Schedule(DstVar1,DstVarN,EnableCh,Start,End)` `Servo2(LED,InCh,Single_Cx,Servo1,Servo2,ServoT)` `Servo3(LED,InCh,Single_Cx,Servo1,Servo2,Servo3,ServoT)` `Servo4(LED,InCh,Single_Cx,Servo1,Servo2,Servo3,Servo4,ServoT)` `Servo5(LED,InCh,Single_Cx,Servo1,Servo2,Servo3,Servo4,Servo5,ServoT)` `SingleLedSignal(LED,InCh,Single_Cx,FadeTime)` `SingleLedSignalEx(LED,InCh,Single_Cx,FadeTime,State0_0,State0_1,State1_0,State1_1,State2_0,State2_1,State3_0,State3_1)` `Sound_ADKey(LED,InCh,ADKey1,ADKey2)` `Sound_ADKeyTime(LED,InCh,ADKey1,ADKey2,Time)` `Sound_DecVol(LED,InCh,Steps)` `Sound_IncVol(LED,InCh,Steps)` `Sound_JQ6500_ADKey(LED,InCh,ADKey)` `Sound_JQ6500_ADKeyTime(LED,InCh,ADKey,Time)` `Sound_JQ6500_BG_DecVol(LED,InCh,Steps)` `Sound_JQ6500_BG_IncVol(LED,InCh,Steps)` `Sound_JQ6500_BG_Next(LED,InCh)` `Sound_JQ6500_BG_Next_of_N(LED,InCh,MaxSoundNr)` `Sound_JQ6500_BG_Next_of_N_Reset(LED,InCh,InReset,MaxSoundNr)` `Sound_JQ6500_BG_PlayRandom(LED,InCh,MaxSoundNr)` `Sound_JQ6500_BG_Prev(LED,InCh)` `Sound_JQ6500_BG_Seq1(LED,InCh)` `Sound_JQ6500_BG_Seq2(LED,InCh)` `Sound_JQ6500_BG_Seq3(LED,InCh)` `Sound_JQ6500_BG_Seq4(LED,InCh)` `Sound_JQ6500_BG_Seq5(LED,InCh)` `Sound_JQ6500_DecVol(LED,InCh,Steps)` `Sound_JQ6500_IncVol(LED,InCh,Steps)` `Sound_JQ6500_Next(LED,InCh)` `Sound_JQ6500_Next_of_N(LED,InCh,MaxSoundNr)` `Sound_JQ6500_Next_of_N_Reset(LED,InCh,InReset,MaxSoundNr)` `Sound_JQ6500_PlayRandom(LED,InCh,MaxSoundNr)` `Sound_JQ6500_Prev(LED,InCh)` `Sound_JQ6500_Seq1(LED,InCh)` `Sound_JQ6500_Seq2(LED,InCh)` `Sound_JQ6500_Seq3(LED,InCh)` `Sound_JQ6500_Seq4(LED,InCh)` `Sound_JQ6500_Seq5(LED,InCh)` `Sound_Loop(LED,InCh)` `Sound_New_DecVol(LED,InCh,Steps)` `Sound_New_IncVol(LED,InCh,Steps)` `Sound_New_Loop(LED,InCh)` `Sound_New_Next(LED,InCh)` `Sound_New_Next_of_N(LED,InCh,MaxSoundNr)` `Sound_New_Next_of_N_Reset(LED,InCh,InReset,MaxSoundNr)` `Sound_New_PausePlay(LED,InCh)` `Sound_New_PlayMode(LED,InCh)` `Sound_New_PlayRandom(LED,InCh,MaxSoundNr)` `Sound_New_Prev(LED,InCh)` `Sound_New_Seq1(LED,InCh)` `Sound_New_Seq10(LED,InCh)` `Sound_New_Seq11(LED,InCh)` `Sound_New_Seq12(LED,InCh)` `Sound_New_Seq13(LED,InCh)` `Sound_New_Seq14(LED,InCh)` `Sound_New_Seq2(LED,InCh)` `Sound_New_Seq3(LED,InCh)` `Sound_New_Seq4(LED,InCh)` `Sound_New_Seq5(LED,InCh)` `Sound_New_Seq6(LED,InCh)` `Sound_New_Seq7(LED,InCh)` `Sound_New_Seq8(LED,InCh)` `Sound_New_Seq9(LED,InCh)` `Sound_New_USDSPI(LED,InCh)` `Sound_Next(LED,InCh)` `Sound_Next_of_N(LED,InCh,MaxSoundNr)` `Sound_Next_of_N_Reset(LED,InCh,InReset,MaxSoundNr)` `Sound_PausePlay(LED,InCh)` `Sound_PlayMode(LED,InCh)` `Sound_PlayRandom(LED,InCh,MaxSoundNr)` `Sound_Prev(LED,InCh)` `Sound_Seq1(LED,InCh)` `Sound_Seq10(LED,InCh)` `Sound_Seq11(LED,InCh)` `Sound_Seq12(LED,InCh)` `Sound_Seq13(LED,InCh)` `Sound_Seq14(LED,InCh)` `Sound_Seq2(LED,InCh)` `Sound_Seq3(LED,InCh)` `Sound_Seq4(LED,InCh)` `Sound_Seq5(LED,InCh)` `Sound_Seq6(LED,InCh)` `Sound_Seq7(LED,InCh)` `Sound_Seq8(LED,InCh)` `Sound_Seq9(LED,InCh)` `Sound_USDSPI(LED,InCh)` `Status_ButtonBL_0_1(LED,B_LED_Cx,Val1,BackLight)` `Status_ButtonBL_0_2(LED,B_LED_Cx,Val1,BackLight)` `Status_ButtonBL_0_3(LED,B_LED_Cx,Val1,BackLight)` `Status_ButtonBL_0_4(LED,B_LED_Cx,Val1,BackLight)` `Status_ButtonBL_0_5(LED,B_LED_Cx,Val1,BackLight)` `Status_Button_0_1(LED,B_LED_Cx,Val1)` `Status_Button_0_2(LED,B_LED_Cx,Val1)` `Status_Button_0_3(LED,B_LED_Cx,Val1)` `Status_Button_0_4(LED,B_LED_Cx,Val1)` `Status_Button_0_5(LED,B_LED_Cx,Val1)` `Status_Button_RGB_0_1(LED,R0,G0,B0,R10,G10,B10,R11,G11,B11)` `Status_Button_RGB_0_2(LED,R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21)` `Status_Button_RGB_0_3(LED,R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21,R30,G30,B30,R31,G31,B31)` `Status_Button_RGB_0_4(LED,R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21,R30,G30,B30,R31,G31,B31,R40,G40,B40,R41,G41,B41)` `Status_Button_RGB_0_5(LED,R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21,R30,G30,B30,R31,G31,B31,R40,G40,B40,R41,G41,B41,R50,G50,B50,R51,G51,B51)` `TM_BUT_TEST` `TM_DISABLED` `TM_INP_TEST` `TM_LED_TEST` `TOTAL_SEND_INPUTS` `TOTAL_SWITCHES_A` `TOTAL_SWITCHES_B` `TOTAL_SWITCHES_C` `TOTAL_SWITCHES_D` `TOTAL_VARIABLES` `TWO_BUTTONS_PER_ADDRESS` `T_BIN_MASK` `T_EQUAL_THEN` `T_FlipFlop2Reset(DstVar0,DstVar1,T_InCh,R_InCh)` `T_FlipFlop2ResetTimeout(DstVar0,DstVar1,T_InCh,R_InCh,Timeout)` `T_FlipFlopInvReset(DstVar,T_InCh,R_InCh)` `T_FlipFlopInvResetTimeout(DstVar,T_InCh,R_InCh,Timeout)` `T_FlipFlopReset(DstVar,T_InCh,R_InCh)` `T_FlipFlopResetTimeout(DstVar,T_InCh,R_InCh,Timeout)` `T_LESS_THEN` `T_NOT_BIN_MASK` `T_NOT_EQUAL_THEN` `USE_EXT_ADDR` `USE_GLOBALVAR_T` `USE_LED_TO_VAR` `USE_PROTOCOL_DCC` `USE_RS232_OR_SPI_AS_INPUT` `Use_GlobalVar(GlobVarNr)` `VorsignalBin_RGB(LED,InCh,MaxB16)` `Vorsignal_RGB(LED,InCh,MaxB16)` `WELDING_CONT_T` `WELDING_T` `WITHOUT_CHANNEL_MASK` `WITHOUT_INP_CH` `Welding(LED,InCh)` `WeldingCont(LED,InCh)` `XPatternT1(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,...)` `XPatternT10(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,...)` `XPatternT11(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,...)` `XPatternT12(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,...)` `XPatternT13(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,...)` `XPatternT14(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,...)` `XPatternT15(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,...)` `XPatternT16(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,...)` `XPatternT17(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,...)` `XPatternT18(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,...)` `XPatternT19(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,...)` `XPatternT2(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,...)` `XPatternT20(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,...)` `XPatternT21(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,...)` `XPatternT22(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,...)` `XPatternT23(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,...)` `XPatternT24(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,...)` `XPatternT25(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,...)` `XPatternT26(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,...)` `XPatternT27(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,...)` `XPatternT28(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,...)` `XPatternT29(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,...)` `XPatternT3(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,...)` `XPatternT30(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,...)` `XPatternT31(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,...)` `XPatternT32(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,...)` `XPatternT33(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,...)` `XPatternT34(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,...)` `XPatternT35(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,...)` `XPatternT36(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,...)` `XPatternT37(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,...)` `XPatternT38(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,...)` `XPatternT39(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,...)` `XPatternT4(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,...)` `XPatternT40(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,...)` `XPatternT41(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,...)` `XPatternT42(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,...)` `XPatternT43(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,...)` `XPatternT44(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,...)` `XPatternT45(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,...)` `XPatternT46(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,...)` `XPatternT47(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,...)` `XPatternT48(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,...)` `XPatternT49(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,...)` `XPatternT5(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,...)` `XPatternT50(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,...)` `XPatternT51(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,...)` `XPatternT52(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,...)` `XPatternT53(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,...)` `XPatternT54(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,...)` `XPatternT55(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,...)` `XPatternT56(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,...)` `XPatternT57(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,...)` `XPatternT58(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,...)` `XPatternT59(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,...)` `XPatternT6(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,...)` `XPatternT60(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,...)` `XPatternT61(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,...)` `XPatternT62(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,...)` `XPatternT63(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,T63,...)` `XPatternT64(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,T63,T64,...)` `XPatternT7(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,...)` `XPatternT8(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,...)` `XPatternT9(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,...)` `XPatternTE1(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,...)` `XPatternTE10(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,...)` `XPatternTE11(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,...)` `XPatternTE12(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,...)` `XPatternTE13(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,...)` `XPatternTE14(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,...)` `XPatternTE15(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,...)` `XPatternTE16(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,...)` `XPatternTE17(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,...)` `XPatternTE18(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,...)` `XPatternTE19(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,...)` `XPatternTE2(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,...)` `XPatternTE20(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,...)` `XPatternTE21(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,...)` `XPatternTE22(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,...)` `XPatternTE23(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,...)` `XPatternTE24(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,...)` `XPatternTE25(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,...)` `XPatternTE26(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,...)` `XPatternTE27(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,...)` `XPatternTE28(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,...)` `XPatternTE29(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,...)` `XPatternTE3(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,...)` `XPatternTE30(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,...)` `XPatternTE31(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,...)` `XPatternTE32(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,...)` `XPatternTE33(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,...)` `XPatternTE34(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,...)` `XPatternTE35(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,...)` `XPatternTE36(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,...)` `XPatternTE37(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,...)` `XPatternTE38(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,...)` `XPatternTE39(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,...)` `XPatternTE4(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,...)` `XPatternTE40(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,...)` `XPatternTE41(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,...)` `XPatternTE42(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,...)` `XPatternTE43(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,...)` `XPatternTE44(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,...)` `XPatternTE45(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,...)` `XPatternTE46(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,...)` `XPatternTE47(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,...)` `XPatternTE48(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,...)` `XPatternTE49(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,...)` `XPatternTE5(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,...)` `XPatternTE50(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,...)` `XPatternTE51(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,...)` `XPatternTE52(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,...)` `XPatternTE53(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,...)` `XPatternTE54(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,...)` `XPatternTE55(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,...)` `XPatternTE56(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,...)` `XPatternTE57(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,...)` `XPatternTE58(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,...)` `XPatternTE59(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,...)` `XPatternTE6(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,...)` `XPatternTE60(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,...)` `XPatternTE61(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,...)` `XPatternTE62(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,...)` `XPatternTE63(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,T63,...)` `XPatternTE64(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,T63,T64,...)` `XPatternTE7(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,...)` `XPatternTE8(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,...)` `XPatternTE9(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,...)` `_ALL_LT_MX2(MinTime,MaxTime)` `_ALL_LT_MX4(MinTime1,MaxTime1,MinTime2,MaxTime2)` `_ALL_NEW_BITS` `_ALL_OLD_BITS` `_BIT_NEW` `_BIT_OLD` `_CF_NO_LEDOUTP` `_CF_P_P_SKIP0` `_CF_ROT_SKIP0` `_CHECK_MODE_RF_NOT_SAME(Mode,DstVar1,DstVarN)` `_CM_RS_FlipFlop1` `_CM_RS_FlipFlop2` `_CM_T_FlipFlop1` `_CM_T_FlipFlopEnable2` `_CM_T_FlipFlopReset2` `_C_ALL_not_supported` `_ConvChannelNr2Byte(ChannelNr)` `_Cx2P_DBLFL(Cx)` `_GET_BIN_SIZE(n)` `_Herz_MoRelais_RS(LED,InCh,Single_Cx,DelayHerz1,TmpNr,Inv)` `_LT_MX(MaxTime)` `_LocalVar_New_Sound(LED)` `_LocalVar_Sound(LED)` `_LocalVar_Sound_JQ6500(LED)` `_LocalVar_Sound_JQ6500_BG(LED)` `_MAX_INP_CHANNEL` `_MAX_TIMER_VAL` `_MOBALEDLIB_H_` `_NEW_AND_OLD` `_NOT_NR` `_OR_NR` `_PAT_DBLFL(LedCnt)` `_PF_XFADE` `_RAND_DIV2(MinTime,MaxTime)` `_RAND_DIV4(MinTime1,MaxTime1,MinTime2,MaxTime2)` `_RAND_MODE2(MinTime,MaxTime)` `_RAND_MODE4(MinTime1,MaxTime1,MinTime2,MaxTime2)` `_Tx2B2(Time,OtherTime)` `_Tx2B4(Time,OtherTime1,OtherTime2,OtherTime3)` `__DATE__` `__LEDS_AUTOPROG_H__` `__MACROS_H__` `__TIME__` `sec` `sek`

# Macro Usage (referenced macros only)

## Macros In Scope

### ADDR_MSK [References: 0] Defined? True

#define ADDR_MSK 0x3FFF

`defined @` leds_autoprog.h#34

### ADDR_OFFSET [References: 0] Defined? True

#define ADDR_OFFSET 0

`defined @` leds_autoprog.h#32

### ALL_CHANNELS [References: 0] Defined? True

#define ALL_CHANNELS 4

`defined @` MobaLedLib.h#1259

### AND [References: 0] Defined? True

#define AND ,

`defined @` MobaLedLib.h#1179

These macros depend on me:

AND | _Herz_MoRelais_RS | Herz_MoRelais
Herz_MoRelais_I

### APATTERNT10_T [References: 0] Defined? True

#define APATTERNT10_T 83

`defined @` Macros.h#594

These macros depend on me:

APATTERNT10_T | APatternT10
APatternTE10
XPatternT10
XPatternTE10

### APATTERNT11_T [References: 0] Defined? True

#define APATTERNT11_T 84

`defined @` Macros.h#595

These macros depend on me:

APATTERNT11_T | APatternT11
APatternTE11
XPatternT11 | KS_Hauptsignal_Zs3_Zs1
KS_Hauptsignal_Zs3_Zs1Bin
KS_Hauptsignal_Zs3_Zs1Bin_RGB
KS_Hauptsignal_Zs3_Zs1_RGB
KS_Hauptsignal_Zs3_Zs6_Zs1
KS_Hauptsignal_Zs3_Zs6_Zs1Bin
KS_Hauptsignal_Zs3_Zs6_Zs1Bin_RGB
KS_Hauptsignal_Zs3_Zs6_Zs1_RGB
XPatternTE11

### APATTERNT12_T [References: 0] Defined? True

#define APATTERNT12_T 85

`defined @` Macros.h#596

These macros depend on me:

APATTERNT12_T | APatternT12
APatternTE12
XPatternT12
XPatternTE12

### APATTERNT13_T [References: 0] Defined? True

#define APATTERNT13_T 86

`defined @` Macros.h#597

These macros depend on me:

APATTERNT13_T | APatternT13
APatternTE13
XPatternT13
XPatternTE13

### APATTERNT14_T [References: 0] Defined? True

#define APATTERNT14_T 87

`defined @` Macros.h#598

These macros depend on me:

APATTERNT14_T | APatternT14
APatternTE14
XPatternT14
XPatternTE14

### APATTERNT15_T [References: 0] Defined? True

#define APATTERNT15_T 88

`defined @` Macros.h#599

These macros depend on me:

APATTERNT15_T | APatternT15
APatternTE15
XPatternT15
XPatternTE15

### APATTERNT16_T [References: 0] Defined? True

#define APATTERNT16_T 89

`defined @` Macros.h#600

These macros depend on me:

APATTERNT16_T | APatternT16
APatternTE16
XPatternT16
XPatternTE16

### APATTERNT17_T [References: 0] Defined? True

#define APATTERNT17_T 90

`defined @` Macros.h#601

These macros depend on me:

APATTERNT17_T | APatternT17
APatternTE17
XPatternT17
XPatternTE17

### APATTERNT18_T [References: 0] Defined? True

#define APATTERNT18_T 91

`defined @` Macros.h#602

These macros depend on me:

APATTERNT18_T | APatternT18
APatternTE18
XPatternT18
XPatternTE18

### APATTERNT19_T [References: 0] Defined? True

#define APATTERNT19_T 92

`defined @` Macros.h#603

These macros depend on me:

APATTERNT19_T | APatternT19
APatternTE19
XPatternT19
XPatternTE19

### APATTERNT20_T [References: 0] Defined? True

#define APATTERNT20_T 93

`defined @` Macros.h#604

These macros depend on me:

APATTERNT20_T | APatternT20
APatternTE20
XPatternT20
XPatternTE20

### APATTERNT21_T [References: 0] Defined? True

#define APATTERNT21_T 94

`defined @` Macros.h#605

These macros depend on me:

APATTERNT21_T | APatternT21
APatternTE21
XPatternT21
XPatternTE21

### APATTERNT22_T [References: 0] Defined? True

#define APATTERNT22_T 95

`defined @` Macros.h#606

These macros depend on me:

APATTERNT22_T | APatternT22
APatternTE22
XPatternT22
XPatternTE22

### APATTERNT23_T [References: 0] Defined? True

#define APATTERNT23_T 96

`defined @` Macros.h#607

These macros depend on me:

APATTERNT23_T | APatternT23
APatternTE23
XPatternT23
XPatternTE23

### APATTERNT24_T [References: 0] Defined? True

#define APATTERNT24_T 97

`defined @` Macros.h#608

These macros depend on me:

APATTERNT24_T | APatternT24
APatternTE24
XPatternT24
XPatternTE24

### APATTERNT25_T [References: 0] Defined? True

#define APATTERNT25_T 98

`defined @` Macros.h#609

These macros depend on me:

APATTERNT25_T | APatternT25
APatternTE25
XPatternT25
XPatternTE25

### APATTERNT26_T [References: 0] Defined? True

#define APATTERNT26_T 99

`defined @` Macros.h#610

These macros depend on me:

APATTERNT26_T | APatternT26
APatternTE26
XPatternT26
XPatternTE26

### APATTERNT27_T [References: 0] Defined? True

#define APATTERNT27_T 100

`defined @` Macros.h#611

These macros depend on me:

APATTERNT27_T | APatternT27
APatternTE27
XPatternT27
XPatternTE27

### APATTERNT28_T [References: 0] Defined? True

#define APATTERNT28_T 101

`defined @` Macros.h#612

These macros depend on me:

APATTERNT28_T | APatternT28
APatternTE28
XPatternT28
XPatternTE28

### APATTERNT29_T [References: 0] Defined? True

#define APATTERNT29_T 102

`defined @` Macros.h#613

These macros depend on me:

APATTERNT29_T | APatternT29
APatternTE29
XPatternT29
XPatternTE29

### APATTERNT30_T [References: 0] Defined? True

#define APATTERNT30_T 103

`defined @` Macros.h#614

These macros depend on me:

APATTERNT30_T | APatternT30
APatternTE30
XPatternT30
XPatternTE30

### APATTERNT31_T [References: 0] Defined? True

#define APATTERNT31_T 104

`defined @` Macros.h#615

These macros depend on me:

APATTERNT31_T | APatternT31
APatternTE31
XPatternT31
XPatternTE31

### APATTERNT32_T [References: 0] Defined? True

#define APATTERNT32_T 105

`defined @` Macros.h#616

These macros depend on me:

APATTERNT32_T | APatternT32
APatternTE32
XPatternT32
XPatternTE32

### APATTERNT33_T [References: 0] Defined? True

#define APATTERNT33_T 106

`defined @` Macros.h#617

These macros depend on me:

APATTERNT33_T | APatternT33
APatternTE33
XPatternT33
XPatternTE33

### APATTERNT34_T [References: 0] Defined? True

#define APATTERNT34_T 107

`defined @` Macros.h#618

These macros depend on me:

APATTERNT34_T | APatternT34
APatternTE34
XPatternT34
XPatternTE34

### APATTERNT35_T [References: 0] Defined? True

#define APATTERNT35_T 108

`defined @` Macros.h#619

These macros depend on me:

APATTERNT35_T | APatternT35
APatternTE35
XPatternT35
XPatternTE35

### APATTERNT36_T [References: 0] Defined? True

#define APATTERNT36_T 109

`defined @` Macros.h#620

These macros depend on me:

APATTERNT36_T | APatternT36
APatternTE36
XPatternT36
XPatternTE36

### APATTERNT37_T [References: 0] Defined? True

#define APATTERNT37_T 110

`defined @` Macros.h#621

These macros depend on me:

APATTERNT37_T | APatternT37
APatternTE37
XPatternT37
XPatternTE37

### APATTERNT38_T [References: 0] Defined? True

#define APATTERNT38_T 111

`defined @` Macros.h#622

These macros depend on me:

APATTERNT38_T | APatternT38
APatternTE38
XPatternT38
XPatternTE38

### APATTERNT39_T [References: 0] Defined? True

#define APATTERNT39_T 112

`defined @` Macros.h#623

These macros depend on me:

APATTERNT39_T | APatternT39
APatternTE39
XPatternT39
XPatternTE39

### APATTERNT3_T [References: 0] Defined? True

#define APATTERNT3_T 76

`defined @` Macros.h#587

These macros depend on me:

APATTERNT3_T | APatternT3
APatternTE3
XPatternT3
XPatternTE3

### APATTERNT40_T [References: 0] Defined? True

#define APATTERNT40_T 113

`defined @` Macros.h#624

These macros depend on me:

APATTERNT40_T | APatternT40
APatternTE40
XPatternT40
XPatternTE40

### APATTERNT41_T [References: 0] Defined? True

#define APATTERNT41_T 114

`defined @` Macros.h#625

These macros depend on me:

APATTERNT41_T | APatternT41
APatternTE41
XPatternT41
XPatternTE41

### APATTERNT42_T [References: 0] Defined? True

#define APATTERNT42_T 115

`defined @` Macros.h#626

These macros depend on me:

APATTERNT42_T | APatternT42
APatternTE42
XPatternT42
XPatternTE42

### APATTERNT43_T [References: 0] Defined? True

#define APATTERNT43_T 116

`defined @` Macros.h#627

These macros depend on me:

APATTERNT43_T | APatternT43
APatternTE43
XPatternT43
XPatternTE43

### APATTERNT44_T [References: 0] Defined? True

#define APATTERNT44_T 117

`defined @` Macros.h#628

These macros depend on me:

APATTERNT44_T | APatternT44
APatternTE44
XPatternT44
XPatternTE44

### APATTERNT45_T [References: 0] Defined? True

#define APATTERNT45_T 118

`defined @` Macros.h#629

These macros depend on me:

APATTERNT45_T | APatternT45
APatternTE45
XPatternT45
XPatternTE45

### APATTERNT46_T [References: 0] Defined? True

#define APATTERNT46_T 119

`defined @` Macros.h#630

These macros depend on me:

APATTERNT46_T | APatternT46
APatternTE46
XPatternT46
XPatternTE46

### APATTERNT47_T [References: 0] Defined? True

#define APATTERNT47_T 120

`defined @` Macros.h#631

These macros depend on me:

APATTERNT47_T | APatternT47
APatternTE47
XPatternT47
XPatternTE47

### APATTERNT48_T [References: 0] Defined? True

#define APATTERNT48_T 121

`defined @` Macros.h#632

These macros depend on me:

APATTERNT48_T | APatternT48
APatternTE48
XPatternT48
XPatternTE48

### APATTERNT49_T [References: 0] Defined? True

#define APATTERNT49_T 122

`defined @` Macros.h#633

These macros depend on me:

APATTERNT49_T | APatternT49
APatternTE49
XPatternT49
XPatternTE49

### APATTERNT4_T [References: 0] Defined? True

#define APATTERNT4_T 77

`defined @` Macros.h#588

These macros depend on me:

APATTERNT4_T | APatternT4
APatternTE4
XPatternT4
XPatternTE4

### APATTERNT50_T [References: 0] Defined? True

#define APATTERNT50_T 123

`defined @` Macros.h#634

These macros depend on me:

APATTERNT50_T | APatternT50
APatternTE50
XPatternT50
XPatternTE50

### APATTERNT51_T [References: 0] Defined? True

#define APATTERNT51_T 124

`defined @` Macros.h#635

These macros depend on me:

APATTERNT51_T | APatternT51
APatternTE51
XPatternT51
XPatternTE51

### APATTERNT52_T [References: 0] Defined? True

#define APATTERNT52_T 125

`defined @` Macros.h#636

These macros depend on me:

APATTERNT52_T | APatternT52
APatternTE52
XPatternT52
XPatternTE52

### APATTERNT53_T [References: 0] Defined? True

#define APATTERNT53_T 126

`defined @` Macros.h#637

These macros depend on me:

APATTERNT53_T | APatternT53
APatternTE53
XPatternT53
XPatternTE53

### APATTERNT54_T [References: 0] Defined? True

#define APATTERNT54_T 127

`defined @` Macros.h#638

These macros depend on me:

APATTERNT54_T | APatternT54
APatternTE54
XPatternT54
XPatternTE54

### APATTERNT55_T [References: 0] Defined? True

#define APATTERNT55_T 128

`defined @` Macros.h#639

These macros depend on me:

APATTERNT55_T | APatternT55
APatternTE55
XPatternT55
XPatternTE55

### APATTERNT56_T [References: 0] Defined? True

#define APATTERNT56_T 129

`defined @` Macros.h#640

These macros depend on me:

APATTERNT56_T | APatternT56
APatternTE56
XPatternT56
XPatternTE56

### APATTERNT57_T [References: 0] Defined? True

#define APATTERNT57_T 130

`defined @` Macros.h#641

These macros depend on me:

APATTERNT57_T | APatternT57
APatternTE57
XPatternT57
XPatternTE57

### APATTERNT58_T [References: 0] Defined? True

#define APATTERNT58_T 131

`defined @` Macros.h#642

These macros depend on me:

APATTERNT58_T | APatternT58
APatternTE58
XPatternT58
XPatternTE58

### APATTERNT59_T [References: 0] Defined? True

#define APATTERNT59_T 132

`defined @` Macros.h#643

These macros depend on me:

APATTERNT59_T | APatternT59
APatternTE59
XPatternT59
XPatternTE59

### APATTERNT5_T [References: 0] Defined? True

#define APATTERNT5_T 78

`defined @` Macros.h#589

These macros depend on me:

APATTERNT5_T | APatternT5
APatternTE5
XPatternT5
XPatternTE5

### APATTERNT60_T [References: 0] Defined? True

#define APATTERNT60_T 133

`defined @` Macros.h#644

These macros depend on me:

APATTERNT60_T | APatternT60
APatternTE60
XPatternT60
XPatternTE60

### APATTERNT61_T [References: 0] Defined? True

#define APATTERNT61_T 134

`defined @` Macros.h#645

These macros depend on me:

APATTERNT61_T | APatternT61
APatternTE61
XPatternT61
XPatternTE61

### APATTERNT62_T [References: 0] Defined? True

#define APATTERNT62_T 135

`defined @` Macros.h#646

These macros depend on me:

APATTERNT62_T | APatternT62
APatternTE62
XPatternT62
XPatternTE62

### APATTERNT63_T [References: 0] Defined? True

#define APATTERNT63_T 136

`defined @` Macros.h#647

These macros depend on me:

APATTERNT63_T | APatternT63
APatternTE63
XPatternT63
XPatternTE63

### APATTERNT64_T [References: 0] Defined? True

#define APATTERNT64_T 137

`defined @` Macros.h#648

These macros depend on me:

APATTERNT64_T | APatternT64
APatternTE64
LAST_APATTERN_T
XPatternT64
XPatternTE64

### APATTERNT6_T [References: 0] Defined? True

#define APATTERNT6_T 79

`defined @` Macros.h#590

These macros depend on me:

APATTERNT6_T | APatternT6
APatternTE6
XPatternT6
XPatternTE6

### APATTERNT7_T [References: 0] Defined? True

#define APATTERNT7_T 80

`defined @` Macros.h#591

These macros depend on me:

APATTERNT7_T | APatternT7
APatternTE7
XPatternT7
XPatternTE7

### APATTERNT8_T [References: 0] Defined? True

#define APATTERNT8_T 81

`defined @` Macros.h#592

These macros depend on me:

APATTERNT8_T | APatternT8 | RGB_AmpelXFade
APatternTE8
XPatternT8
XPatternTE8

### APATTERNT9_T [References: 0] Defined? True

#define APATTERNT9_T 82

`defined @` Macros.h#593

These macros depend on me:

APATTERNT9_T | APatternT9
APatternTE9
XPatternT9 | AndreaskrLT
AndreaskrLT3
AndreaskrLT3_RGB
AndreaskrLT_RGB
KS_Vorsignal_Zs3V
KS_Vorsignal_Zs3VBin
KS_Vorsignal_Zs3VBin_RGB
KS_Vorsignal_Zs3V_RGB
XPatternTE9

### APatternT10 [References: 0] Defined? True

#define APatternT10(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,...) \
APATTERNT10_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#186

I depend on these macros:

APatternT10 | APATTERNT10_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT11 [References: 0] Defined? True

#define APatternT11(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,...) \
APATTERNT11_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_W2B(COUNT_VARARGS(__VA_ARGS__)\
), __VA_ARGS__,

`defined @` Macros.h#187

I depend on these macros:

APatternT11 | APATTERNT11_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT12 [References: 0] Defined? True

#define APatternT12(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,...) \
APATTERNT12_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_W2B(COUNT_VARARGS(__\
VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#188

I depend on these macros:

APatternT12 | APATTERNT12_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT13 [References: 0] Defined? True

#define APatternT13(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,...) \
APATTERNT13_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_W2B(COUNT_\
VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#189

I depend on these macros:

APatternT13 | APATTERNT13_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT14 [References: 0] Defined? True

#define APatternT14(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,...) \
APATTERNT14_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#190

I depend on these macros:

APatternT14 | APATTERNT14_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT15 [References: 0] Defined? True

#define APatternT15(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,...) \
APATTERNT15_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#191

I depend on these macros:

APatternT15 | APATTERNT15_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT16 [References: 0] Defined? True

#define APatternT16(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,...) \
APATTERNT16_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#192

I depend on these macros:

APatternT16 | APATTERNT16_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT17 [References: 0] Defined? True

#define APatternT17(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,...) \
APATTERNT17_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#193

I depend on these macros:

APatternT17 | APATTERNT17_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT18 [References: 0] Defined? True

#define APatternT18(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,...) \
APATTERNT18_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__, \

`defined @` Macros.h#194

I depend on these macros:

APatternT18 | APATTERNT18_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT19 [References: 0] Defined? True

#define APatternT19(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,...) \
APATTERNT19_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#195

I depend on these macros:

APatternT19 | APATTERNT19_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT20 [References: 0] Defined? True

#define APatternT20(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,...) \
APATTERNT20_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#196

I depend on these macros:

APatternT20 | APATTERNT20_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT21 [References: 0] Defined? True

#define APatternT21(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,...) \
APATTERNT21_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#197

I depend on these macros:

APatternT21 | APATTERNT21_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT22 [References: 0] Defined? True

#define APatternT22(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,...) .) APATTERNT22_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#198

I depend on these macros:

APatternT22 | APATTERNT22_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT23 [References: 0] Defined? True

#define APatternT23(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,...) 3,...) APATTERNT23_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#199

I depend on these macros:

APatternT23 | APATTERNT23_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT24 [References: 0] Defined? True

#define APatternT24(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,...) 4,...) APATTERNT24_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#200

I depend on these macros:

APatternT24 | APATTERNT24_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT25 [References: 0] Defined? True

#define APatternT25(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,...) 5,...) APATTERNT25_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_W2B(COUNT_VARARGS(__VA\
_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#201

I depend on these macros:

APatternT25 | APATTERNT25_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT26 [References: 0] Defined? True

#define APatternT26(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,...) 6,...) APATTERNT26_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_W2B(COUNT_VA\
RARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#202

I depend on these macros:

APatternT26 | APATTERNT26_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT27 [References: 0] Defined? True

#define APatternT27(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,...) 7,...) APATTERNT27_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_W2\
B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#203

I depend on these macros:

APatternT27 | APATTERNT27_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT28 [References: 0] Defined? True

#define APatternT28(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,...) 8,...) APATTERNT28_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#204

I depend on these macros:

APatternT28 | APATTERNT28_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT29 [References: 0] Defined? True

#define APatternT29(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,...) 9,...) APATTERNT29_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#205

I depend on these macros:

APatternT29 | APATTERNT29_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT3 [References: 0] Defined? True

#define APatternT3(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,...) APATTERNT3_T, \
_CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#179

I depend on these macros:

APatternT3 | APATTERNT3_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT30 [References: 0] Defined? True

#define APatternT30(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,...) 0,...) APATTERNT30_T, _CHKL(LED)+RAM7, \
(NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#206

I depend on these macros:

APatternT30 | APATTERNT30_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT31 [References: 0] Defined? True

#define APatternT31(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,...) 1,...) APATTERNT31_T, _CHKL(LED)+RAM7, \
(NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__, \

`defined @` Macros.h#207

I depend on these macros:

APatternT31 | APATTERNT31_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT32 [References: 0] Defined? True

#define APatternT32(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,...) 2,...) APATTERNT32_T, _CHKL(LED)+RAM7, \
(NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#208

I depend on these macros:

APatternT32 | APATTERNT32_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT33 [References: 0] Defined? True

#define APatternT33(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,...) 3,...) APATTERNT33_T, _CHKL(LED)+RAM7, \
(NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#209

I depend on these macros:

APatternT33 | APATTERNT33_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT34 [References: 0] Defined? True

#define APatternT34(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,...) 4,...) APATTERNT34_T, _CHKL(LED)+RAM7, \
(NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#210

I depend on these macros:

APatternT34 | APATTERNT34_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT35 [References: 0] Defined? True

#define APatternT35(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,...) 5,...) APATTERNT35_T, _CHKL(LED)+RAM7, \
(NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#211

I depend on these macros:

APatternT35 | APATTERNT35_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT36 [References: 0] Defined? True

#define APatternT36(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,...) 6,...) APATTERNT36_T, \
_CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#212

I depend on these macros:

APatternT36 | APATTERNT36_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT37 [References: 0] Defined? True

#define APatternT37(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,...) 7,...) APATTERNT37_T, \
_CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#213

I depend on these macros:

APatternT37 | APATTERNT37_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT38 [References: 0] Defined? True

#define APatternT38(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,...) 8,...) APATTERNT38_T, \
_CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_W2B(COUNT_VARARGS(__VA_A\
RGS__)), __VA_ARGS__,

`defined @` Macros.h#214

I depend on these macros:

APatternT38 | APATTERNT38_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT39 [References: 0] Defined? True

#define APatternT39(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,...) 9,...) APATTERNT39_T, \
_CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_W2B(COUNT_VARA\
RGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#215

I depend on these macros:

APatternT39 | APATTERNT39_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT4 [References: 0] Defined? True

#define APatternT4(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,...) APATTERNT4_T, \
_CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__, \

`defined @` Macros.h#180

I depend on these macros:

APatternT4 | APATTERNT4_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT40 [References: 0] Defined? True

#define APatternT40(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,...) 0,...) \
APATTERNT40_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_W2B(\
COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#216

I depend on these macros:

APatternT40 | APATTERNT40_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT41 [References: 0] Defined? True

#define APatternT41(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,...) 1,...) \
APATTERNT41_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#217

I depend on these macros:

APatternT41 | APATTERNT41_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT42 [References: 0] Defined? True

#define APatternT42(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,...) 2,...) \
APATTERNT42_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#218

I depend on these macros:

APatternT42 | APATTERNT42_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT43 [References: 0] Defined? True

#define APatternT43(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,...) 3,...) \
APATTERNT43_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#219

I depend on these macros:

APatternT43 | APATTERNT43_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT44 [References: 0] Defined? True

#define APatternT44(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,...) 4,...) \
APATTERNT44_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__, \

`defined @` Macros.h#220

I depend on these macros:

APatternT44 | APATTERNT44_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT45 [References: 0] Defined? True

#define APatternT45(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,...) 5,...) \
APATTERNT45_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#221

I depend on these macros:

APatternT45 | APATTERNT45_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT46 [References: 0] Defined? True

#define APatternT46(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,...) 6,...) \
APATTERNT46_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#222

I depend on these macros:

APatternT46 | APATTERNT46_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT47 [References: 0] Defined? True

#define APatternT47(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,...) 7,...) \
APATTERNT47_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#223

I depend on these macros:

APatternT47 | APATTERNT47_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT48 [References: 0] Defined? True

#define APatternT48(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,...) 8,...) \
APATTERNT48_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#224

I depend on these macros:

APatternT48 | APATTERNT48_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT49 [References: 0] Defined? True

#define APatternT49(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,...) 9,...) \
APATTERNT49_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#225

I depend on these macros:

APatternT49 | APATTERNT49_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT5 [References: 0] Defined? True

#define APatternT5(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,...) APATTERNT5_T, \
_CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#181

I depend on these macros:

APatternT5 | APATTERNT5_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT50 [References: 0] Defined? True

#define APatternT50(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,...) 0,...) \
APATTERNT50_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#226

I depend on these macros:

APatternT50 | APATTERNT50_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT51 [References: 0] Defined? True

#define APatternT51(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,...) 1,...) \
APATTERNT51_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_W2B(COUNT_VARARGS(__VA_ARG\
S__)), __VA_ARGS__,

`defined @` Macros.h#227

I depend on these macros:

APatternT51 | APATTERNT51_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT52 [References: 0] Defined? True

#define APatternT52(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,...) 2,...) \
APATTERNT52_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_W2B(COUNT_VARARG\
S(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#228

I depend on these macros:

APatternT52 | APATTERNT52_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT53 [References: 0] Defined? True

#define APatternT53(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,...) 3,...) \
APATTERNT53_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_W2B(CO\
UNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#229

I depend on these macros:

APatternT53 | APATTERNT53_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT54 [References: 0] Defined? True

#define APatternT54(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,...) 4,...) \
APATTERNT54_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#230

I depend on these macros:

APatternT54 | APATTERNT54_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT55 [References: 0] Defined? True

#define APatternT55(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,...) 5,..\
.) APATTERNT55_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#231

I depend on these macros:

APatternT55 | APATTERNT55_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT56 [References: 0] Defined? True

#define APatternT56(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,...) \
6,...) APATTERNT56_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#232

I depend on these macros:

APatternT56 | APATTERNT56_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT57 [References: 0] Defined? True

#define APatternT57(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,...) 6,T57,...) APATTERNT57_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#233

I depend on these macros:

APatternT57 | APATTERNT57_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT58 [References: 0] Defined? True

#define APatternT58(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,...) T57,T58,...) APATTERNT58_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#234

I depend on these macros:

APatternT58 | APATTERNT58_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT59 [References: 0] Defined? True

#define APatternT59(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,...) T58,T59,...) APATTERNT59_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_T2B(T59),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#235

I depend on these macros:

APatternT59 | APATTERNT59_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT6 [References: 0] Defined? True

#define APatternT6(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,...) APATTERNT6_T, \
_CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#182

I depend on these macros:

APatternT6 | APATTERNT6_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT60 [References: 0] Defined? True

#define APatternT60(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,...) T59,T60,...) APATTERNT60_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_T2B(T59),_T2B(T60),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#236

I depend on these macros:

APatternT60 | APATTERNT60_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT61 [References: 0] Defined? True

#define APatternT61(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,...) T60,T61,...) APATTERNT61_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_T2B(T59),_T2B(T60),_T2B(T61),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#237

I depend on these macros:

APatternT61 | APATTERNT61_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT62 [References: 0] Defined? True

#define APatternT62(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,...) T61,T62,...) APATTERNT62_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_T2B(T59),_T2B(T60),_T2B(T61),_T2B(T62),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#238

I depend on these macros:

APatternT62 | APATTERNT62_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT63 [References: 0] Defined? True

#define APatternT63(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,T63,...) T62,T63,...) APATTERNT63_T, _CHKL(LED)+RAM7, \
(NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_T2B(T59),_T2B(T60),_T2B(T61),_T2B(T62),_T2B(T63),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#239

I depend on these macros:

APatternT63 | APATTERNT63_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT64 [References: 0] Defined? True

#define APatternT64(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,T63,T64,...) T63,T64,...) APATTERNT64_T, _CHKL(LED)+RAM7, \
(NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_T2B(T59),_T2B(T60),_T2B(T61),_T2B(T62),_T2B(T63),_T2B(T64),_W2B(COUNT_VARARGS(__VA_ARGS_\
_)), __VA_ARGS__,

`defined @` Macros.h#240

I depend on these macros:

APatternT64 | APATTERNT64_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT7 [References: 0] Defined? True

#define APatternT7(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,...) \
APATTERNT7_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#183

I depend on these macros:

APatternT7 | APATTERNT7_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternT8 [References: 0] Defined? True

#define APatternT8(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,...) \
APATTERNT8_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#184

I depend on these macros:

APatternT8 | APATTERNT8_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

These macros depend on me:

APatternT8 | RGB_AmpelXFade

### APatternT9 [References: 0] Defined? True

#define APatternT9(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,...) \
APATTERNT9_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#185

I depend on these macros:

APatternT9 | APATTERNT9_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE1 [References: 0] Defined? True

#define APatternTE1(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,...) APATTERNT1_T, \
_CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#379

I depend on these macros:

APatternTE1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE10 [References: 0] Defined? True

#define APatternTE10(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,...) \
APATTERNT10_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#388

I depend on these macros:

APatternTE10 | APATTERNT10_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE11 [References: 0] Defined? True

#define APatternTE11(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,...) \
APATTERNT11_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_W2B(COUNT_VARARGS(__VA_ARGS__)\
), __VA_ARGS__,

`defined @` Macros.h#389

I depend on these macros:

APatternTE11 | APATTERNT11_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE12 [References: 0] Defined? True

#define APatternTE12(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,...) \
APATTERNT12_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_W2B(COUNT_VARARGS(__\
VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#390

I depend on these macros:

APatternTE12 | APATTERNT12_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE13 [References: 0] Defined? True

#define APatternTE13(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,...) \
APATTERNT13_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_W2B(COUNT_\
VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#391

I depend on these macros:

APatternTE13 | APATTERNT13_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE14 [References: 0] Defined? True

#define APatternTE14(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,...) \
APATTERNT14_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#392

I depend on these macros:

APatternTE14 | APATTERNT14_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE15 [References: 0] Defined? True

#define APatternTE15(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,...) \
APATTERNT15_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#393

I depend on these macros:

APatternTE15 | APATTERNT15_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE16 [References: 0] Defined? True

#define APatternTE16(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,...) \
APATTERNT16_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#394

I depend on these macros:

APatternTE16 | APATTERNT16_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE17 [References: 0] Defined? True

#define APatternTE17(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,...) \
APATTERNT17_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#395

I depend on these macros:

APatternTE17 | APATTERNT17_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE18 [References: 0] Defined? True

#define APatternTE18(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,...) \
APATTERNT18_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__, \

`defined @` Macros.h#396

I depend on these macros:

APatternTE18 | APATTERNT18_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE19 [References: 0] Defined? True

#define APatternTE19(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,...) \
APATTERNT19_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#397

I depend on these macros:

APatternTE19 | APATTERNT19_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE2 [References: 0] Defined? True

#define APatternTE2(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,...) APATTERNT2_T, \
_CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#380

I depend on these macros:

APatternTE2 | APATTERNT2_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE20 [References: 0] Defined? True

#define APatternTE20(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,...) .) APATTERNT20_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#398

I depend on these macros:

APatternTE20 | APATTERNT20_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE21 [References: 0] Defined? True

#define APatternTE21(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,...) 1,...) APATTERNT21_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#399

I depend on these macros:

APatternTE21 | APATTERNT21_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE22 [References: 0] Defined? True

#define APatternTE22(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,...) 2,...) APATTERNT22_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#400

I depend on these macros:

APatternTE22 | APATTERNT22_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE23 [References: 0] Defined? True

#define APatternTE23(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,...) 3,...) APATTERNT23_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#401

I depend on these macros:

APatternTE23 | APATTERNT23_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE24 [References: 0] Defined? True

#define APatternTE24(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,...) 4,...) APATTERNT24_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#402

I depend on these macros:

APatternTE24 | APATTERNT24_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE25 [References: 0] Defined? True

#define APatternTE25(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,...) 5,...) APATTERNT25_T, _CHKL(LED)+RAM7, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_W2B(COUNT_VARARGS(__VA\
_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#403

I depend on these macros:

APatternTE25 | APATTERNT25_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE26 [References: 0] Defined? True

#define APatternTE26(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,...) 6,...) APATTERNT26_T, _CHKL(LED)+RAM7, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_W2B(COUNT_VA\
RARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#404

I depend on these macros:

APatternTE26 | APATTERNT26_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE27 [References: 0] Defined? True

#define APatternTE27(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,...) 7,...) APATTERNT27_T, _CHKL(LED)+RAM7, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_W2\
B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#405

I depend on these macros:

APatternTE27 | APATTERNT27_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE28 [References: 0] Defined? True

#define APatternTE28(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,...) 8,...) APATTERNT28_T, _CHKL(LED)+RAM7, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#406

I depend on these macros:

APatternTE28 | APATTERNT28_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE29 [References: 0] Defined? True

#define APatternTE29(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,...) 9,...) APATTERNT29_T, _CHKL(LED)+RAM7, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#407

I depend on these macros:

APatternTE29 | APATTERNT29_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE3 [References: 0] Defined? True

#define APatternTE3(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,...) APATTERNT3_T, \
_CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#381

I depend on these macros:

APatternTE3 | APATTERNT3_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE30 [References: 0] Defined? True

#define APatternTE30(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,...) 0,...) APATTERNT30_T, _CHKL(LED)+RAM7, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#408

I depend on these macros:

APatternTE30 | APATTERNT30_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE31 [References: 0] Defined? True

#define APatternTE31(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,...) 1,...) APATTERNT31_T, _CHKL(LED)+RAM7, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__, \

`defined @` Macros.h#409

I depend on these macros:

APatternTE31 | APATTERNT31_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE32 [References: 0] Defined? True

#define APatternTE32(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,...) 2,...) APATTERNT32_T, _CHKL(LED)+RAM7, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#410

I depend on these macros:

APatternTE32 | APATTERNT32_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE33 [References: 0] Defined? True

#define APatternTE33(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,...) 3,...) APATTERNT33_T, _CHKL(LED)+RAM7, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#411

I depend on these macros:

APatternTE33 | APATTERNT33_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE34 [References: 0] Defined? True

#define APatternTE34(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,...) 4,...) APATTERNT34_T, \
_CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#412

I depend on these macros:

APatternTE34 | APATTERNT34_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE35 [References: 0] Defined? True

#define APatternTE35(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,...) 5,...) APATTERNT35_T, \
_CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#413

I depend on these macros:

APatternTE35 | APATTERNT35_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE36 [References: 0] Defined? True

#define APatternTE36(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,...) 6,...) APATTERNT36_T, \
_CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#414

I depend on these macros:

APatternTE36 | APATTERNT36_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE37 [References: 0] Defined? True

#define APatternTE37(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,...) 7,...) APATTERNT37_T, \
_CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#415

I depend on these macros:

APatternTE37 | APATTERNT37_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE38 [References: 0] Defined? True

#define APatternTE38(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,...) 8,...) \
APATTERNT38_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_W2B(COUNT_VARARGS(__VA_A\
RGS__)), __VA_ARGS__,

`defined @` Macros.h#416

I depend on these macros:

APatternTE38 | APATTERNT38_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE39 [References: 0] Defined? True

#define APatternTE39(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,...) 9,...) \
APATTERNT39_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_W2B(COUNT_VARA\
RGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#417

I depend on these macros:

APatternTE39 | APATTERNT39_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE4 [References: 0] Defined? True

#define APatternTE4(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,...) \
APATTERNT4_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__, \

`defined @` Macros.h#382

I depend on these macros:

APatternTE4 | APATTERNT4_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE40 [References: 0] Defined? True

#define APatternTE40(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,...) 0,...) \
APATTERNT40_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_W2B(\
COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#418

I depend on these macros:

APatternTE40 | APATTERNT40_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE41 [References: 0] Defined? True

#define APatternTE41(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,...) 1,...) \
APATTERNT41_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#419

I depend on these macros:

APatternTE41 | APATTERNT41_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE42 [References: 0] Defined? True

#define APatternTE42(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,...) 2,...) \
APATTERNT42_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#420

I depend on these macros:

APatternTE42 | APATTERNT42_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE43 [References: 0] Defined? True

#define APatternTE43(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,...) 3,...) \
APATTERNT43_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#421

I depend on these macros:

APatternTE43 | APATTERNT43_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE44 [References: 0] Defined? True

#define APatternTE44(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,...) 4,...) \
APATTERNT44_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__, \

`defined @` Macros.h#422

I depend on these macros:

APatternTE44 | APATTERNT44_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE45 [References: 0] Defined? True

#define APatternTE45(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,...) 5,...) \
APATTERNT45_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#423

I depend on these macros:

APatternTE45 | APATTERNT45_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE46 [References: 0] Defined? True

#define APatternTE46(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,...) 6,...) \
APATTERNT46_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#424

I depend on these macros:

APatternTE46 | APATTERNT46_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE47 [References: 0] Defined? True

#define APatternTE47(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,...) 7,...) \
APATTERNT47_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#425

I depend on these macros:

APatternTE47 | APATTERNT47_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE48 [References: 0] Defined? True

#define APatternTE48(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,...) 8,...) \
APATTERNT48_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#426

I depend on these macros:

APatternTE48 | APATTERNT48_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE49 [References: 0] Defined? True

#define APatternTE49(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,...) 9,...) \
APATTERNT49_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#427

I depend on these macros:

APatternTE49 | APATTERNT49_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE5 [References: 0] Defined? True

#define APatternTE5(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,...) \
APATTERNT5_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#383

I depend on these macros:

APatternTE5 | APATTERNT5_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE50 [References: 0] Defined? True

#define APatternTE50(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,...) 0,...) \
APATTERNT50_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#428

I depend on these macros:

APatternTE50 | APATTERNT50_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE51 [References: 0] Defined? True

#define APatternTE51(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,...) 1,...) \
APATTERNT51_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_W2B(COUNT_VARARGS(__VA_ARG\
S__)), __VA_ARGS__,

`defined @` Macros.h#429

I depend on these macros:

APatternTE51 | APATTERNT51_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE52 [References: 0] Defined? True

#define APatternTE52(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,...) 2,...) \
APATTERNT52_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_W2B(COUNT_VARARG\
S(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#430

I depend on these macros:

APatternTE52 | APATTERNT52_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE53 [References: 0] Defined? True

#define APatternTE53(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,...) 3,..\
.) APATTERNT53_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_W2B(CO\
UNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#431

I depend on these macros:

APatternTE53 | APATTERNT53_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE54 [References: 0] Defined? True

#define APatternTE54(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,...) \
4,...) APATTERNT54_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#432

I depend on these macros:

APatternTE54 | APATTERNT54_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE55 [References: 0] Defined? True

#define APatternTE55(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,...) 4,T55,...) APATTERNT55_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#433

I depend on these macros:

APatternTE55 | APATTERNT55_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE56 [References: 0] Defined? True

#define APatternTE56(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,...) T55,T56,...) APATTERNT56_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#434

I depend on these macros:

APatternTE56 | APATTERNT56_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE57 [References: 0] Defined? True

#define APatternTE57(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,...) T56,T57,...) APATTERNT57_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#435

I depend on these macros:

APatternTE57 | APATTERNT57_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE58 [References: 0] Defined? True

#define APatternTE58(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,...) T57,T58,...) APATTERNT58_T, _CHKL(LED)+RAM7, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#436

I depend on these macros:

APatternTE58 | APATTERNT58_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE59 [References: 0] Defined? True

#define APatternTE59(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,...) T58,T59,...) APATTERNT59_T, _CHKL(LED)+RAM7, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_T2B(T59),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#437

I depend on these macros:

APatternTE59 | APATTERNT59_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE6 [References: 0] Defined? True

#define APatternTE6(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,...) \
APATTERNT6_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#384

I depend on these macros:

APatternTE6 | APATTERNT6_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE60 [References: 0] Defined? True

#define APatternTE60(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,...) T59,T60,...) APATTERNT60_T, _CHKL(LED)+RAM7, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_T2B(T59),_T2B(T60),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#438

I depend on these macros:

APatternTE60 | APATTERNT60_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE61 [References: 0] Defined? True

#define APatternTE61(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,...) T60,T61,...) APATTERNT61_T, _CHKL(LED)+RAM7, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_T2B(T59),_T2B(T60),_T2B(T61),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#439

I depend on these macros:

APatternTE61 | APATTERNT61_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE62 [References: 0] Defined? True

#define APatternTE62(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,...) T61,T62,...) APATTERNT62_T, _CHKL(LED)+RAM7, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_T2B(T59),_T2B(T60),_T2B(T61),_T2B(T62),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#440

I depend on these macros:

APatternTE62 | APATTERNT62_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE63 [References: 0] Defined? True

#define APatternTE63(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,T63,...) T62,T63,...) APATTERNT63_T, _CHKL(LED)+RAM7, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_T2B(T59),_T2B(T60),_T2B(T61),_T2B(T62),_T2B(T63),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#441

I depend on these macros:

APatternTE63 | APATTERNT63_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE64 [References: 0] Defined? True

#define APatternTE64(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,T63,T64,...) T63,T64,...) APATTERNT64_T, _CHKL(LED)+RAM7, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_T2B(T59),_T2B(T60),_T2B(T61),_T2B(T62),_T2B(T63),_T2B(T64),_W2B(COUNT_VARARGS(__VA_ARGS_\
_)), __VA_ARGS__,

`defined @` Macros.h#442

I depend on these macros:

APatternTE64 | APATTERNT64_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE7 [References: 0] Defined? True

#define APatternTE7(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,...) \
APATTERNT7_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#385

I depend on these macros:

APatternTE7 | APATTERNT7_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE8 [References: 0] Defined? True

#define APatternTE8(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,...) \
APATTERNT8_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#386

I depend on these macros:

APatternTE8 | APATTERNT8_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### APatternTE9 [References: 0] Defined? True

#define APatternTE9(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,...) \
APATTERNT9_T, _CHKL(LED)+RAM7, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#387

I depend on these macros:

APatternTE9 | APATTERNT9_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### AmpelX [References: 0] Defined? True

#define AmpelX(LED,InCh) PatternT4(LED,0,InCh,6,0, 255,0,0,3 Sec,1 Sec,10 Sec,3 \
Sec,201,194,40,73,22,70)

`defined @` MobaLedLib.h#185

I depend on these macros:

AmpelX | PatternT4 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT4_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
Sec

### AndreaskrLT [References: 0] Defined? True

#define AndreaskrLT(LED,Single_Cx,InCh,MaxBrightness,LT_Time,FadeTime,OnTime) \
Bin_InCh_to_TmpVar(InCh, 1) \
XPatternT9(LED,_Cx2StCh(Single_Cx)+132,SI_LocalVar,2,0,MaxBrightness,0,0,FadeTime,FadeTime,LT_Time,FadeTime,OnTime,OnTime,FadeTime,O\
nTime,FadeTime,240,15,48,204,3 ,63,128,0,0,2,64,0,0,65)

`defined @` MobaLedLib.h#165

I depend on these macros:

AndreaskrLT | Bin_InCh_to_TmpVar | BIN_INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT9 | APATTERNT9_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
_Cx2StCh

### AndreaskrLT3 [References: 0] Defined? True

#define AndreaskrLT3(LED,Single_Cx,InCh,MaxBrightness,LT_Time,FadeTime,OnTime) \
Bin_InCh_to_TmpVar(InCh, 1) \
XPatternT9(LED,_Cx2StCh(Single_Cx)+68,SI_LocalVar,3,0,MaxBrightness,0,0,FadeTime,FadeTime,LT_Time,FadeTime,OnTime,OnTime,FadeTime,On\
Time,FadeTime,192,243,0,192,196,48,19 ,63,128,0,0,2,64,0,0,65)

`defined @` MobaLedLib.h#169

I depend on these macros:

AndreaskrLT3 | Bin_InCh_to_TmpVar | BIN_INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT9 | APATTERNT9_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
_Cx2StCh

### AndreaskrLT3_RGB [References: 0] Defined? True

#define AndreaskrLT3_RGB(LED,InCh,MaxBrightness,LT_Time,FadeTime,OnTime) Bin_InCh_to_TmpVar(InCh, \
1) \
XPatternT9(LED,196,SI_LocalVar,9,0,MaxBrightness,0,0,FadeTime,FadeTime,LT_Time,FadeTime,OnTime,OnTime,FadeTime,OnTime,FadeTime,0,0,1\
2,3,48,12,0,0,0,0,0,12,64,5,12,0,48,0,3,80,1 ,63,128,0,0,2,64,0,0,65)

`defined @` MobaLedLib.h#177

I depend on these macros:

AndreaskrLT3_RGB | Bin_InCh_to_TmpVar | BIN_INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT9 | APATTERNT9_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### AndreaskrLT_RGB [References: 0] Defined? True

#define AndreaskrLT_RGB(LED,InCh,MaxBrightness,LT_Time,FadeTime,OnTime) Bin_InCh_to_TmpVar(InCh, \
1) XPatternT9(LED,4,SI_LocalVar,4,0,MaxBrightness,0,0,FadeTime,FadeTime,LT_Time,FadeTime,OnTime,OnTime,FadeTime,OnTime,FadeTime,0,19\
5,195,0,0,3,192,192,3 ,63,128,0,0,2,64,0,0,65)

`defined @` MobaLedLib.h#173

I depend on these macros:

AndreaskrLT_RGB | Bin_InCh_to_TmpVar | BIN_INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT9 | APATTERNT9_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### AndreaskrRGB [References: 0] Defined? True

#define AndreaskrRGB(LED,InCh) APatternT1(LED,0, InCh,4,0,255,0,0,250 ms,129,24)

`defined @` MobaLedLib.h#161

I depend on these macros:

AndreaskrRGB | APatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
ms

### Andreaskreuz [References: 0] Defined? True

#define Andreaskreuz(LED,Cx,InCh) APatternT1(LED,_NStru(Cx, 0,1),InCh,2,0,255,0,0,250 \
ms,105)

`defined @` MobaLedLib.h#160

I depend on these macros:

Andreaskreuz | APatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
_NStru | _Cx2LedCnt
_Cx2StCh
_FreeBits
ms

### BIN_INCH_TO_TMPVAR1_T [References: 0] Defined? True

#define BIN_INCH_TO_TMPVAR1_T 176

`defined @` Macros.h#671

These macros depend on me:

BIN_INCH_TO_TMPVAR1_T | Bin_InCh_to_TmpVar1

### B_GREEN [References: 0] Defined? True

#define B_GREEN (uint16_t)(2<<14)

`defined @` leds_autoprog.h#38

### B_RED [References: 0] Defined? True

#define B_RED (uint16_t)(1<<14)

`defined @` leds_autoprog.h#37

These macros depend on me:

B_RED | B_TAST

### B_TAST [References: 0] Defined? True

#define B_TAST B_RED

`defined @` leds_autoprog.h#40

I depend on these macros:

B_TAST | B_RED

### Bin_InCh_to_TmpVar1 [References: 0] Defined? True

#define Bin_InCh_to_TmpVar1(FirstInCh,InCh_Cnt) BIN_INCH_TO_TMPVAR1_T, FirstInCh, InCh_Cnt, \

`defined @` MobaLedLib.h#147

I depend on these macros:

Bin_InCh_to_TmpVar1 | BIN_INCH_TO_TMPVAR1_T

### Blink2 [References: 0] Defined? True

#define Blink2(LED,Cx,InCh,Pause,Act,Val0,Val1) PatternT2(LED,_NStru(Cx, \
2,1),InCh,_Cx2LedCnt(Cx),Val0,Val1,0, PF_SLOW, Act/16, Pause/16, _Cx2P_BLINK(Cx)) \

`defined @` MobaLedLib.h#154

I depend on these macros:

Blink2 | PF_SLOW
PatternT2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
_Cx2LedCnt
_Cx2P_BLINK | _Cx2LedCnt
_PAT_BLINK
_NStru | _Cx2LedCnt
_Cx2StCh
_FreeBits

### Blink3 [References: 0] Defined? True

#define Blink3(LED,Cx,InCh,Pause,Act,Val0,Val1,Off) PatternT2(LED,_NStru(Cx, \
2,1),InCh,_Cx2LedCnt(Cx),Val0,Val1,Off, PF_SLOW, Act/16, Pause/16, _Cx2P_BLINK(Cx)) \

`defined @` MobaLedLib.h#155

I depend on these macros:

Blink3 | PF_SLOW
PatternT2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
_Cx2LedCnt
_Cx2P_BLINK | _Cx2LedCnt
_PAT_BLINK
_NStru | _Cx2LedCnt
_Cx2StCh
_FreeBits

### Blinker [References: 0] Defined? True

#define Blinker(LED,Cx,InCh,Period) PatternT1(LED,_NStru(Cx, 2,1),InCh,_Cx2LedCnt(Cx), 0, \
255, 0, PF_SLOW,(Period)/32, _Cx2P_BLINK(Cx))

`defined @` MobaLedLib.h#151

I depend on these macros:

Blinker | PF_SLOW
PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
_Cx2LedCnt
_Cx2P_BLINK | _Cx2LedCnt
_PAT_BLINK
_NStru | _Cx2LedCnt
_Cx2StCh
_FreeBits

### BlinkerHD [References: 0] Defined? True

#define BlinkerHD(LED,Cx,InCh,Period) PatternT1(LED,_NStru(Cx, 2,1),InCh,_Cx2LedCnt(Cx),50, \
255, 0, PF_SLOW, (Period)/32, _Cx2P_BLINK(Cx))

`defined @` MobaLedLib.h#153

I depend on these macros:

BlinkerHD | PF_SLOW
PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
_Cx2LedCnt
_Cx2P_BLINK | _Cx2LedCnt
_PAT_BLINK
_NStru | _Cx2LedCnt
_Cx2StCh
_FreeBits

### BlinkerInvInp [References: 0] Defined? True

#define BlinkerInvInp(LED,Cx,InCh,Period) PatternT1(LED,_NStru(Cx, 2,1),InCh,_Cx2LedCnt(Cx), \
0, 255, 0, PF_SLOW+PF_INVERT_INP,(Period)/32, _Cx2P_BLINK(Cx))

`defined @` MobaLedLib.h#152

I depend on these macros:

BlinkerInvInp | PF_INVERT_INP
PF_SLOW
PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
_Cx2LedCnt
_Cx2P_BLINK | _Cx2LedCnt
_PAT_BLINK
_NStru | _Cx2LedCnt
_Cx2StCh
_FreeBits

### BlueLight1 [References: 0] Defined? True

#define BlueLight1(LED,Cx,InCh) PatternT4(LED,_NStru(Cx, 4,1),InCh,_Cx2LedCnt(Cx),0, 255, \
0,0, 48 ms, 74 ms, 48 ms, 496 ms,_Cx2P_DBLFL(Cx))

`defined @` MobaLedLib.h#156

I depend on these macros:

BlueLight1 | PatternT4 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT4_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
_Cx2LedCnt
_Cx2P_DBLFL | _Cx2LedCnt
_PAT_DBLFL | _C_ALL_not_supported
_NStru | _Cx2LedCnt
_Cx2StCh
_FreeBits
ms

### BlueLight2 [References: 0] Defined? True

#define BlueLight2(LED,Cx,InCh) PatternT4(LED,_NStru(Cx, 4,1),InCh,_Cx2LedCnt(Cx),0, 255, \
0,0, 24 ms, 74 ms, 24 ms, 512 ms,_Cx2P_DBLFL(Cx))

`defined @` MobaLedLib.h#157

I depend on these macros:

BlueLight2 | PatternT4 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT4_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
_Cx2LedCnt
_Cx2P_DBLFL | _Cx2LedCnt
_PAT_DBLFL | _C_ALL_not_supported
_NStru | _Cx2LedCnt
_Cx2StCh
_FreeBits
ms

### Button [References: 0] Defined? True

#define Button(LED,Cx,InCh,Duration,Val0,Val1) PatternT1(LED,_NStru(Cx, \
2,1),InCh,_Cx2LedCnt(Cx),Val0,Val1,Val0,PM_SEQUENZ_W_ABORT+PF_SLOW,Duration/16, \
_Cx2P_BLINK(Cx))

`defined @` MobaLedLib.h#149

I depend on these macros:

Button | PF_SLOW
PM_SEQUENZ_W_ABORT
PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
_Cx2LedCnt
_Cx2P_BLINK | _Cx2LedCnt
_PAT_BLINK
_NStru | _Cx2LedCnt
_Cx2StCh
_FreeBits

### ButtonFunc [References: 0] Defined? True

#define ButtonFunc(DstVar,InCh,Duration) Random(DstVar, InCh, RF_STAY_ON, 0, 0, (Duration), \
(Duration))

`defined @` MobaLedLib.h#346

I depend on these macros:

ButtonFunc | RF_STAY_ON
Random | RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RANDOM_T
_RAND_MODE4 | RF_SLOW
_ALL_LT_MX4 | _ALL_LT_MX2 | _LT_MX | _MAX_TIMER_VAL
_Tx2B4 | _RAND_DIV4 | _ALL_LT_MX4 | _ALL_LT_MX2 | _LT_MX | _MAX_TIMER_VAL
_T2B | _W2B

### ButtonNOff [References: 0] Defined? True

#define ButtonNOff(LED,Cx,InCh,Duration,Val0,Val1) PatternT1(LED,_NStru(Cx, \
2,1),InCh,_Cx2LedCnt(Cx),Val0,Val1,Val0,PM_SEQUENZ_NO_RESTART+PF_SLOW,Duration/16,_Cx2P_BLINK(Cx)) \

`defined @` MobaLedLib.h#150

I depend on these macros:

ButtonNOff | PF_SLOW
PM_SEQUENZ_NO_RESTART
PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
_Cx2LedCnt
_Cx2P_BLINK | _Cx2LedCnt
_PAT_BLINK
_NStru | _Cx2LedCnt
_Cx2StCh
_FreeBits

### C12 [References: 0] Defined? True

#define C12 _Cx(2, 0)

`defined @` MobaLedLib.h#969

I depend on these macros:

C12 | _Cx

These macros depend on me:

C12 | C_YELLOW

### C23 [References: 0] Defined? True

#define C23 _Cx(2, 1)

`defined @` MobaLedLib.h#970

I depend on these macros:

C23 | _Cx

These macros depend on me:

C23 | C_CYAN

### CALCULATE_t10 [References: 0] Defined? True

#define CALCULATE_t10

`defined @` MobaLedLib.h#1256

### CALCULATE_t4 [References: 0] Defined? True

#define CALCULATE_t4

`defined @` MobaLedLib.h#1255

### CALCULATE_t4w [References: 0] Defined? True

#define CALCULATE_t4w

`defined @` MobaLedLib.h#1254

### CANDLE1 [References: 0] Defined? True

#define CANDLE1 63

`defined @` MobaLedLib.h#1143

### CANDLE2 [References: 0] Defined? True

#define CANDLE2 64

`defined @` MobaLedLib.h#1144

### CANDLE3 [References: 0] Defined? True

#define CANDLE3 65

`defined @` MobaLedLib.h#1145

### CF_BINARY [References: 0] Defined? True

#define CF_BINARY 0b00000100

`defined @` MobaLedLib.h#1056

These macros depend on me:

CF_BINARY | _CM_RS_FlipFlop1 | MonoFlop
MonoFlopLongReset
MonoFlopReset
RS_FlipFlop | _Herz_MoRelais_RS | Herz_MoRelais
Herz_MoRelais_I
RS_FlipFlopTimeout | _Herz_MoRelais_RS | Herz_MoRelais
Herz_MoRelais_I
_CM_T_FlipFlop1 | T_FlipFlopReset
T_FlipFlopResetTimeout

### CF_INV_ENABLE [References: 0] Defined? True

#define CF_INV_ENABLE 0b00000010

`defined @` MobaLedLib.h#1055

These macros depend on me:

CF_INV_ENABLE | PushButton2I_0_1 | PushButton2I_RGB_0_1
PushButton2I_w_LED_BL_0_1
PushButton2I_0_2 | PushButton2I_RGB_0_2
PushButton2I_w_LED_BL_0_2
PushButton2I_0_3 | PushButton2I_RGB_0_3
PushButton2I_w_LED_BL_0_3
PushButton2I_0_4 | PushButton2I_RGB_0_4
PushButton2I_w_LED_BL_0_4
PushButton2I_0_5 | PushButton2I_RGB_0_5
PushButton2I_w_LED_BL_0_5
Sound_JQ6500_BG_Next_of_N_Reset | Sound_JQ6500_BG_Next_of_N
Sound_JQ6500_Next_of_N_Reset | Sound_JQ6500_Next_of_N
Sound_New_Next_of_N_Reset | Sound_New_Next_of_N
Sound_Next_of_N_Reset | Sound_Next_of_N
_CM_T_FlipFlop1 | T_FlipFlopReset
T_FlipFlopResetTimeout
_CM_T_FlipFlopReset2 | T_FlipFlop2Reset
T_FlipFlop2ResetTimeout
T_FlipFlopInvReset
T_FlipFlopInvResetTimeout

### CF_INV_INPUT [References: 0] Defined? True

#define CF_INV_INPUT 0b00000001

`defined @` MobaLedLib.h#1054

### CF_LOCAL_VAR [References: 0] Defined? True

#define CF_LOCAL_VAR (0b00000010<<8)

`defined @` MobaLedLib.h#1063

These macros depend on me:

CF_LOCAL_VAR | CF_ONLY_LOCALVAR | Sound_JQ6500_BG_Next_of_N_Reset | Sound_JQ6500_BG_Next_of_N
Sound_JQ6500_BG_PlayRandom
Sound_JQ6500_Next_of_N_Reset | Sound_JQ6500_Next_of_N
Sound_JQ6500_PlayRandom
Sound_New_Next_of_N_Reset | Sound_New_Next_of_N
Sound_New_PlayRandom
Sound_Next_of_N_Reset | Sound_Next_of_N
Sound_PlayRandom

### CF_ONLY_LOCALVAR [References: 0] Defined? True

#define CF_ONLY_LOCALVAR (CF_LOCAL_VAR|_CF_NO_LEDOUTP)

`defined @` MobaLedLib.h#1065

I depend on these macros:

CF_ONLY_LOCALVAR | CF_LOCAL_VAR
_CF_NO_LEDOUTP

These macros depend on me:

CF_ONLY_LOCALVAR | Sound_JQ6500_BG_Next_of_N_Reset | Sound_JQ6500_BG_Next_of_N
Sound_JQ6500_BG_PlayRandom
Sound_JQ6500_Next_of_N_Reset | Sound_JQ6500_Next_of_N
Sound_JQ6500_PlayRandom
Sound_New_Next_of_N_Reset | Sound_New_Next_of_N
Sound_New_PlayRandom
Sound_Next_of_N_Reset | Sound_Next_of_N
Sound_PlayRandom

### CF_PINGPONG [References: 0] Defined? True

#define CF_PINGPONG 0b01000000

`defined @` MobaLedLib.h#1060

These macros depend on me:

CF_PINGPONG | _CF_P_P_SKIP0

### CF_RANDOM [References: 0] Defined? True

#define CF_RANDOM (0b00000001<<8)

`defined @` MobaLedLib.h#1062

These macros depend on me:

CF_RANDOM | Sound_JQ6500_BG_PlayRandom
Sound_JQ6500_PlayRandom
Sound_New_PlayRandom
Sound_PlayRandom

### CF_RESET_LONG [References: 0] Defined? True

#define CF_RESET_LONG 0b00001000

`defined @` MobaLedLib.h#1057

These macros depend on me:

CF_RESET_LONG | MonoFlop2LongReset
MonoFlopInvLongReset
MonoFlopLongReset
PushButton2I_0_1 | PushButton2I_RGB_0_1
PushButton2I_w_LED_BL_0_1
PushButton2I_0_2 | PushButton2I_RGB_0_2
PushButton2I_w_LED_BL_0_2
PushButton2I_0_3 | PushButton2I_RGB_0_3
PushButton2I_w_LED_BL_0_3
PushButton2I_0_4 | PushButton2I_RGB_0_4
PushButton2I_w_LED_BL_0_4
PushButton2I_0_5 | PushButton2I_RGB_0_5
PushButton2I_w_LED_BL_0_5
PushButton_0_1 | PushButton_RGB_0_1
PushButton_w_LED_0_1
PushButton_w_LED_BL_0_1
PushButton_0_2 | PushButton_RGB_0_2
PushButton_w_LED_0_2
PushButton_w_LED_BL_0_2
PushButton_0_3 | PushButton_RGB_0_3
PushButton_w_LED_0_3
PushButton_w_LED_BL_0_3
PushButton_0_4 | PushButton_RGB_0_4
PushButton_w_LED_0_4
PushButton_w_LED_BL_0_4
PushButton_0_5 | PushButton_RGB_0_5
PushButton_w_LED_0_5
PushButton_w_LED_BL_0_5

### CF_ROTATE [References: 0] Defined? True

#define CF_ROTATE 0b00100000

`defined @` MobaLedLib.h#1059

These macros depend on me:

CF_ROTATE | PushButton2I_0_1 | PushButton2I_RGB_0_1
PushButton2I_w_LED_BL_0_1
PushButton2I_0_2 | PushButton2I_RGB_0_2
PushButton2I_w_LED_BL_0_2
PushButton2I_0_3 | PushButton2I_RGB_0_3
PushButton2I_w_LED_BL_0_3
PushButton2I_0_4 | PushButton2I_RGB_0_4
PushButton2I_w_LED_BL_0_4
PushButton2I_0_5 | PushButton2I_RGB_0_5
PushButton2I_w_LED_BL_0_5
PushButton_0_1 | PushButton_RGB_0_1
PushButton_w_LED_0_1
PushButton_w_LED_BL_0_1
PushButton_0_2 | PushButton_RGB_0_2
PushButton_w_LED_0_2
PushButton_w_LED_BL_0_2
PushButton_0_3 | PushButton_RGB_0_3
PushButton_w_LED_0_3
PushButton_w_LED_BL_0_3
PushButton_0_4 | PushButton_RGB_0_4
PushButton_w_LED_0_4
PushButton_w_LED_BL_0_4
PushButton_0_5 | PushButton_RGB_0_5
PushButton_w_LED_0_5
PushButton_w_LED_BL_0_5
Sound_JQ6500_BG_Next_of_N_Reset | Sound_JQ6500_BG_Next_of_N
Sound_JQ6500_Next_of_N_Reset | Sound_JQ6500_Next_of_N
Sound_New_Next_of_N_Reset | Sound_New_Next_of_N
Sound_Next_of_N_Reset | Sound_Next_of_N
_CF_ROT_SKIP0
_CM_T_FlipFlop1 | T_FlipFlopReset
T_FlipFlopResetTimeout
_CM_T_FlipFlopEnable2
_CM_T_FlipFlopReset2 | T_FlipFlop2Reset
T_FlipFlop2ResetTimeout
T_FlipFlopInvReset
T_FlipFlopInvResetTimeout

### CF_SKIP0 [References: 0] Defined? True

#define CF_SKIP0 0b10000000

`defined @` MobaLedLib.h#1061

These macros depend on me:

CF_SKIP0 | PushButton2I_0_1 | PushButton2I_RGB_0_1
PushButton2I_w_LED_BL_0_1
PushButton2I_0_2 | PushButton2I_RGB_0_2
PushButton2I_w_LED_BL_0_2
PushButton2I_0_3 | PushButton2I_RGB_0_3
PushButton2I_w_LED_BL_0_3
PushButton2I_0_4 | PushButton2I_RGB_0_4
PushButton2I_w_LED_BL_0_4
PushButton2I_0_5 | PushButton2I_RGB_0_5
PushButton2I_w_LED_BL_0_5
PushButton_0_1 | PushButton_RGB_0_1
PushButton_w_LED_0_1
PushButton_w_LED_BL_0_1
PushButton_0_2 | PushButton_RGB_0_2
PushButton_w_LED_0_2
PushButton_w_LED_BL_0_2
PushButton_0_3 | PushButton_RGB_0_3
PushButton_w_LED_0_3
PushButton_w_LED_BL_0_3
PushButton_0_4 | PushButton_RGB_0_4
PushButton_w_LED_0_4
PushButton_w_LED_BL_0_4
PushButton_0_5 | PushButton_RGB_0_5
PushButton_w_LED_0_5
PushButton_w_LED_BL_0_5
Sound_JQ6500_BG_Next_of_N_Reset | Sound_JQ6500_BG_Next_of_N
Sound_JQ6500_BG_PlayRandom
Sound_JQ6500_Next_of_N_Reset | Sound_JQ6500_Next_of_N
Sound_JQ6500_PlayRandom
Sound_New_Next_of_N_Reset | Sound_New_Next_of_N
Sound_New_PlayRandom
Sound_Next_of_N_Reset | Sound_Next_of_N
Sound_PlayRandom
_CF_P_P_SKIP0
_CF_ROT_SKIP0

### CF_UP_DOWN [References: 0] Defined? True

#define CF_UP_DOWN 0b00010000

`defined @` MobaLedLib.h#1058

These macros depend on me:

CF_UP_DOWN | _CM_RS_FlipFlop1 | MonoFlop
MonoFlopLongReset
MonoFlopReset
RS_FlipFlop | _Herz_MoRelais_RS | Herz_MoRelais
Herz_MoRelais_I
RS_FlipFlopTimeout | _Herz_MoRelais_RS | Herz_MoRelais
Herz_MoRelais_I
_CM_RS_FlipFlop2 | MonoFlop2
MonoFlop2LongReset
MonoFlopInv
MonoFlopInvLongReset
RS_FlipFlop2
RS_FlipFlop2Timeout
RS_FlipFlopInv
RS_FlipFlopInvTimeout

### CM_NORMAL [References: 0] Defined? True

#define CM_NORMAL 0

`defined @` MobaLedLib.h#1053

### COLOR0 [References: 0] Defined? True

#define COLOR0 0

`defined @` MobaLedLib.h#1275

### COLOR1 [References: 0] Defined? True

#define COLOR1 1

`defined @` MobaLedLib.h#1276

### COLOR2 [References: 0] Defined? True

#define COLOR2 2

`defined @` MobaLedLib.h#1277

### COLOR3 [References: 0] Defined? True

#define COLOR3 3

`defined @` MobaLedLib.h#1278

### COLOR4 [References: 0] Defined? True

#define COLOR4 4

`defined @` MobaLedLib.h#1279

### COLOR5 [References: 0] Defined? True

#define COLOR5 5

`defined @` MobaLedLib.h#1280

### COLOR_GASL_B [References: 0] Defined? True

#define COLOR_GASL_B 7

`defined @` MobaLedLib.h#1282

### COLOR_GASL_D [References: 0] Defined? True

#define COLOR_GASL_D 6

`defined @` MobaLedLib.h#1281

### COLOR_NEON_B [References: 0] Defined? True

#define COLOR_NEON_B 10

`defined @` MobaLedLib.h#1285

### COLOR_NEON_D [References: 0] Defined? True

#define COLOR_NEON_D 8

`defined @` MobaLedLib.h#1283

### COLOR_NEON_M [References: 0] Defined? True

#define COLOR_NEON_M 9

`defined @` MobaLedLib.h#1284

### COLOR_SINGLE [References: 0] Defined? True

#define COLOR_SINGLE 15

`defined @` MobaLedLib.h#1290

### COLOR_SINGLE_D [References: 0] Defined? True

#define COLOR_SINGLE_D 16

`defined @` MobaLedLib.h#1291

### COLOR_TV0_A [References: 0] Defined? True

#define COLOR_TV0_A 11

`defined @` MobaLedLib.h#1286

### COLOR_TV0_B [References: 0] Defined? True

#define COLOR_TV0_B 12

`defined @` MobaLedLib.h#1287

### COLOR_TV1_A [References: 0] Defined? True

#define COLOR_TV1_A 13

`defined @` MobaLedLib.h#1288

### COLOR_TV1_B [References: 0] Defined? True

#define COLOR_TV1_B 14

`defined @` MobaLedLib.h#1289

### CONST_T [References: 0] Defined? True

#define CONST_T 1

`defined @` Macros.h#515

### COPYLED_OFF [References: 0] Defined? True

#define COPYLED_OFF 0

`defined @` leds_autoprog.h#138

### COPYLED_OFF_ONCE [References: 0] Defined? True

#define COPYLED_OFF_ONCE 1

`defined @` leds_autoprog.h#142

### COPYLED_T [References: 0] Defined? True

#define COPYLED_T 143

`defined @` Macros.h#657

These macros depend on me:

COPYLED_T | CopyLED

### COUNTER_ID [References: 0] Defined? True

#define COUNTER_ID

`defined @` leds_autoprog.h#160

### COUNTER_T [References: 0] Defined? True

#define COUNTER_T 144

`defined @` Macros.h#658

These macros depend on me:

COUNTER_T | Counter | MonoFlop
MonoFlop2
MonoFlop2LongReset
MonoFlopInv
MonoFlopInvLongReset
MonoFlopLongReset
MonoFlopReset
PushButton2I_0_1 | PushButton2I_RGB_0_1
PushButton2I_w_LED_BL_0_1
PushButton2I_0_2 | PushButton2I_RGB_0_2
PushButton2I_w_LED_BL_0_2
PushButton2I_0_3 | PushButton2I_RGB_0_3
PushButton2I_w_LED_BL_0_3
PushButton2I_0_4 | PushButton2I_RGB_0_4
PushButton2I_w_LED_BL_0_4
PushButton2I_0_5 | PushButton2I_RGB_0_5
PushButton2I_w_LED_BL_0_5
PushButton_0_1 | PushButton_RGB_0_1
PushButton_w_LED_0_1
PushButton_w_LED_BL_0_1
PushButton_0_2 | PushButton_RGB_0_2
PushButton_w_LED_0_2
PushButton_w_LED_BL_0_2
PushButton_0_3 | PushButton_RGB_0_3
PushButton_w_LED_0_3
PushButton_w_LED_BL_0_3
PushButton_0_4 | PushButton_RGB_0_4
PushButton_w_LED_0_4
PushButton_w_LED_BL_0_4
PushButton_0_5 | PushButton_RGB_0_5
PushButton_w_LED_0_5
PushButton_w_LED_BL_0_5
RS_FlipFlop | _Herz_MoRelais_RS | Herz_MoRelais
Herz_MoRelais_I
RS_FlipFlop2
RS_FlipFlop2Timeout
RS_FlipFlopInv
RS_FlipFlopInvTimeout
RS_FlipFlopTimeout | _Herz_MoRelais_RS | Herz_MoRelais
Herz_MoRelais_I
Sound_JQ6500_BG_Next_of_N_Reset | Sound_JQ6500_BG_Next_of_N
Sound_JQ6500_BG_PlayRandom
Sound_JQ6500_Next_of_N_Reset | Sound_JQ6500_Next_of_N
Sound_JQ6500_PlayRandom
Sound_New_Next_of_N_Reset | Sound_New_Next_of_N
Sound_New_PlayRandom
Sound_Next_of_N_Reset | Sound_Next_of_N
Sound_PlayRandom
T_FlipFlop2Reset
T_FlipFlop2ResetTimeout
T_FlipFlopInvReset
T_FlipFlopInvResetTimeout
T_FlipFlopReset
T_FlipFlopResetTimeout

### CPX_ANALOG_INPUT [References: 0] Defined? True

#define CPX_ANALOG_INPUT 201

`defined @` Macros.h#695

### CPX_ANALOG_LIMMITS [References: 0] Defined? True

#define CPX_ANALOG_LIMMITS 202

`defined @` Macros.h#696

### CPX_LED_ASSIGNEMENT [References: 0] Defined? True

#define CPX_LED_ASSIGNEMENT 200

`defined @` Macros.h#694

### C_ALL [References: 0] Defined? True

#define C_ALL _Cx(3, 0)

`defined @` MobaLedLib.h#971

I depend on these macros:

C_ALL | _Cx

These macros depend on me:

C_ALL | C_WHITE
LeuchtfeuerALL

### C_BLUE [References: 0] Defined? True

#define C_BLUE C3

`defined @` MobaLedLib.h#974

I depend on these macros:

C_BLUE | C3 | _Cx

### C_CYAN [References: 0] Defined? True

#define C_CYAN C23

`defined @` MobaLedLib.h#977

I depend on these macros:

C_CYAN | C23 | _Cx

### C_GREEN [References: 0] Defined? True

#define C_GREEN C2

`defined @` MobaLedLib.h#973

I depend on these macros:

C_GREEN | C2 | _Cx

### C_RED [References: 0] Defined? True

#define C_RED C1

`defined @` MobaLedLib.h#972

I depend on these macros:

C_RED | C1 | _Cx

### C_WHITE [References: 0] Defined? True

#define C_WHITE C_ALL

`defined @` MobaLedLib.h#975

I depend on these macros:

C_WHITE | C_ALL | _Cx

### C_YELLOW [References: 0] Defined? True

#define C_YELLOW C12

`defined @` MobaLedLib.h#976

I depend on these macros:

C_YELLOW | C12 | _Cx

### Charlie_Binary [References: 0] Defined? True

#define Charlie_Binary(LED,InCh,BinStates) Bin_InCh_to_TmpVar(InCh, _GET_BIN_SIZE((BinStates))) \
PatternT1(LED,28,SI_LocalVar,3,0,255,0,0,1 \
ms,15,15,15,35,35,35,55,55,55,75,75,75,95,95,95,115,115,115,135,135,135,155,155,155,175,175,175,195,195,195,215,215,215 \
,63,191,191,191,191,191,191,191,191,191,191)

`defined @` MobaLedLib.h#232

I depend on these macros:

Charlie_Binary | Bin_InCh_to_TmpVar | BIN_INCH_TO_TMPVAR_T
PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
_GET_BIN_SIZE
ms

### Charlie_Buttons [References: 0] Defined? True

#define Charlie_Buttons(LED,InCh,States) InCh_to_TmpVar(InCh, States) \
PatternT1(LED,28,SI_LocalVar,3,0,255,0,0,1 \
ms,15,15,15,35,35,35,55,55,55,75,75,75,95,95,95,115,115,115,135,135,135,155,155,155,175,175,175,195,195,195,215,215,215 \
,63,191,191,191,191,191,191,191,191,191,191)

`defined @` MobaLedLib.h#225

I depend on these macros:

Charlie_Buttons | InCh_to_TmpVar | INCH_TO_TMPVAR_T
PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
ms

### ConstrWarnLight10 [References: 0] Defined? True

#define ConstrWarnLight10(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitE) PatternT11(LED,0, \
InCh,10,MinBrightness,MaxBrightness,0,0,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,WaitE,1,8,64,0,2,16,128,0,4,32,0,1,8,0,0) \

`defined @` MobaLedLib.h#217

I depend on these macros:

ConstrWarnLight10 | PatternT11 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT11_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### ConstrWarnLight11 [References: 0] Defined? True

#define ConstrWarnLight11(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitE) \
PatternT12(LED,128,InCh,11,MinBrightness,MaxBrightness,0,0,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,WaitE,1,16,0,1,16,0,1,16,0,1,\
16,0,1,16,0,1,0)

`defined @` MobaLedLib.h#218

I depend on these macros:

ConstrWarnLight11 | PatternT12 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT12_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### ConstrWarnLight12 [References: 0] Defined? True

#define ConstrWarnLight12(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitE) \
PatternT13(LED,128,InCh,12,MinBrightness,MaxBrightness,0,0,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,WaitE,1,32,0,4,128,0,16,0\
,2,64,0,8,0,1,32,0,4,128,0,0)

`defined @` MobaLedLib.h#219

I depend on these macros:

ConstrWarnLight12 | PatternT13 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT13_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### ConstrWarnLight13 [References: 0] Defined? True

#define ConstrWarnLight13(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitE) PatternT14(LED,64, \
InCh,13,MinBrightness,MaxBrightness,0,0,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,WaitE,1,64,0,16,0,4,0,1,64,0,16,0,4,0,1,\
64,0,16,0,4,0,1,0)

`defined @` MobaLedLib.h#220

I depend on these macros:

ConstrWarnLight13 | PatternT14 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT14_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### ConstrWarnLight14 [References: 0] Defined? True

#define ConstrWarnLight14(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitE) \
PatternT15(LED,192,InCh,14,MinBrightness,MaxBrightness,0,0,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,WaitE,1,128,0,64,\
0,32,0,16,0,8,0,4,0,2,0,1,128,0,64,0,32,0,16,0,8,0,0)

`defined @` MobaLedLib.h#221

I depend on these macros:

ConstrWarnLight14 | PatternT15 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT15_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### ConstrWarnLight15 [References: 0] Defined? True

#define ConstrWarnLight15(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitE) PatternT16(LED,0, \
InCh,15,MinBrightness,MaxBrightness,0,0,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,WaitE,1,0,1,0,1,0,1,0,1,0,1,0,1,\
0,1,0,1,0,1,0,1,0,1,0,1,0,1,0,1,0)

`defined @` MobaLedLib.h#222

I depend on these macros:

ConstrWarnLight15 | PatternT16 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT16_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### ConstrWarnLight3 [References: 0] Defined? True

#define ConstrWarnLight3(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitE) PatternT4( \
LED,128,InCh,3, MinBrightness,MaxBrightness,0,0,OnT,OnT,OnT,WaitE,17,1,0,0,0)

`defined @` MobaLedLib.h#210

I depend on these macros:

ConstrWarnLight3 | PatternT4 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT4_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### ConstrWarnLight4 [References: 0] Defined? True

#define ConstrWarnLight4(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitE) PatternT5( LED,0, \
InCh,4, MinBrightness,MaxBrightness,0,0,OnT,OnT,OnT,OnT,WaitE,33,132,0,0,0,0)

`defined @` MobaLedLib.h#211

I depend on these macros:

ConstrWarnLight4 | PatternT5 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT5_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### ConstrWarnLight5 [References: 0] Defined? True

#define ConstrWarnLight5(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitE) PatternT6( \
LED,128,InCh,5, MinBrightness,MaxBrightness,0,0,OnT,OnT,OnT,OnT,OnT,WaitE,65,16,4,1,0,0,0,0) \

`defined @` MobaLedLib.h#212

I depend on these macros:

ConstrWarnLight5 | PatternT6 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT6_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### ConstrWarnLight6 [References: 0] Defined? True

#define ConstrWarnLight6(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitE) PatternT7( LED,0, \
InCh,6, MinBrightness,MaxBrightness,0,0,OnT,OnT,OnT,OnT,OnT,OnT,WaitE,129,64,32,16,8,0,0,0,0) \

`defined @` MobaLedLib.h#213

I depend on these macros:

ConstrWarnLight6 | PatternT7 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT7_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### ConstrWarnLight7 [References: 0] Defined? True

#define ConstrWarnLight7(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitE) PatternT8( \
LED,128,InCh,7, MinBrightness,MaxBrightness,0,0,OnT,OnT,OnT,OnT,OnT,OnT,OnT,WaitE,1,1,1,1,1,1,1,0,0,0,0) \

`defined @` MobaLedLib.h#214

I depend on these macros:

ConstrWarnLight7 | PatternT8 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT8_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### ConstrWarnLight8 [References: 0] Defined? True

#define ConstrWarnLight8(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitE) PatternT9( LED,0, \
InCh,8, MinBrightness,MaxBrightness,0,0,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,WaitE,1,2,4,8,16,32,64,128,0,0,0,0) \

`defined @` MobaLedLib.h#215

I depend on these macros:

ConstrWarnLight8 | PatternT9 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT9_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### ConstrWarnLight9 [References: 0] Defined? True

#define ConstrWarnLight9(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitE) PatternT10(LED,128,InCh,9, \
MinBrightness,MaxBrightness,0,0,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,OnT,WaitE,1,4,16,64,0,1,4,16,64,0,1,0,0,0) \

`defined @` MobaLedLib.h#216

I depend on these macros:

ConstrWarnLight9 | PatternT10 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT10_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### ConstrWarnLightFlash10 [References: 0] Defined? True

#define ConstrWarnLightFlash10(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitT,WaitE) \
PatternT20(LED,0, \
InCh,10,MinBrightness,MaxBrightness,0,0,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,On\
T,WaitE,1,0,32,0,0,4,0,128,0,0,16,0,0,2,0,64,0,0,8,0,0,1,0,32,0)

`defined @` MobaLedLib.h#203

I depend on these macros:

ConstrWarnLightFlash10 | PatternT20 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT20_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### ConstrWarnLightFlash11 [References: 0] Defined? True

#define ConstrWarnLightFlash11(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitT,WaitE) \
PatternT22(LED,192,InCh,11,MinBrightness,MaxBrightness,0,0,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT\
,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitE,1,0,128,0,0,64,0,0,32,0,0,16,0,0,8,0,0,4,0,0,2,0,0,1,0,128,0,0,64,0,0) \

`defined @` MobaLedLib.h#204

I depend on these macros:

ConstrWarnLightFlash11 | PatternT22 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT22_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### ConstrWarnLightFlash12 [References: 0] Defined? True

#define ConstrWarnLightFlash12(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitT,WaitE) \
PatternT24(LED,0, \
InCh,12,MinBrightness,MaxBrightness,0,0,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,On\
T,WaitT,OnT,WaitT,OnT,WaitE,1,0,0,2,0,0,4,0,0,8,0,0,16,0,0,32,0,0,64,0,0,128,0,0,0,1,0,0,2,0,0,4,0,0,8,0) \

`defined @` MobaLedLib.h#205

I depend on these macros:

ConstrWarnLightFlash12 | PatternT24 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT24_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### ConstrWarnLightFlash13 [References: 0] Defined? True

#define ConstrWarnLightFlash13(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitT,WaitE) \
PatternT26(LED,192,InCh,13,MinBrightness,MaxBrightness,0,0,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT\
,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitE,1,0,0,8,0,0,64,0,0,0,2,0,0,16,0,0,128,0,0,0,4,0,0,32,0,0,0,1,0,0,8,0,0,64,0\
,0,0,2,0,0,16,0,0)

`defined @` MobaLedLib.h#206

I depend on these macros:

ConstrWarnLightFlash13 | PatternT26 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT26_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### ConstrWarnLightFlash14 [References: 0] Defined? True

#define ConstrWarnLightFlash14(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitT,WaitE) \
PatternT28(LED,0, \
InCh,14,MinBrightness,MaxBrightness,0,0,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,On\
T,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitE,1,0,0,32,0,0,0,4,0,0,128,0,0,0,16,0,0,0,2,0,0,64,0,0,0,8,0,0,0,1,0,0,32,0,0,0,4,0,0,\
128,0,0,0,16,0,0,0,2,0)

`defined @` MobaLedLib.h#207

I depend on these macros:

ConstrWarnLightFlash14 | PatternT28 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT28_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### ConstrWarnLightFlash15 [References: 0] Defined? True

#define ConstrWarnLightFlash15(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitT,WaitE) \
PatternT30(LED,192,InCh,15,MinBrightness,MaxBrightness,0,0,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT\
,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitE,1,0,0,128,0,0,0,64,0,0,0,32,0,0,0,16,0,0,0,8,0,0,0,4,0,\
0,0,2,0,0,0,1,0,0,128,0,0,0,64,0,0,0,32,0,0,0,16,0,0,0,8,0,0,0,4,0,0)

`defined @` MobaLedLib.h#208

I depend on these macros:

ConstrWarnLightFlash15 | PatternT30 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT30_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### ConstrWarnLightFlash3 [References: 0] Defined? True

#define ConstrWarnLightFlash3(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitT,WaitE) \
PatternT6( LED,128,InCh,3, MinBrightness,MaxBrightness,0,0,OnT,WaitT,OnT,WaitT,OnT,WaitE,129,64,0,0,0) \

`defined @` MobaLedLib.h#196

I depend on these macros:

ConstrWarnLightFlash3 | PatternT6 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT6_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### ConstrWarnLightFlash4 [References: 0] Defined? True

#define ConstrWarnLightFlash4(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitT,WaitE) \
PatternT8( LED,0, InCh,4, MinBrightness,MaxBrightness,0,0,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitE,1,2,4,8,0,0) \

`defined @` MobaLedLib.h#197

I depend on these macros:

ConstrWarnLightFlash4 | PatternT8 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT8_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### ConstrWarnLightFlash5 [References: 0] Defined? True

#define ConstrWarnLightFlash5(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitT,WaitE) \
PatternT10(LED,128,InCh,5, MinBrightness,MaxBrightness,0,0,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitE,1,8,64,0,2,16,0,0) \

`defined @` MobaLedLib.h#198

I depend on these macros:

ConstrWarnLightFlash5 | PatternT10 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT10_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### ConstrWarnLightFlash6 [References: 0] Defined? True

#define ConstrWarnLightFlash6(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitT,WaitE) \
PatternT12(LED,0, InCh,6, \
MinBrightness,MaxBrightness,0,0,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitE,1,32,0,4,128,0,16,0,2) \

`defined @` MobaLedLib.h#199

I depend on these macros:

ConstrWarnLightFlash6 | PatternT12 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT12_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### ConstrWarnLightFlash7 [References: 0] Defined? True

#define ConstrWarnLightFlash7(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitT,WaitE) \
PatternT14(LED,192,InCh,7, \
MinBrightness,MaxBrightness,0,0,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitE,1,128,0,64,0,32,0,16,0,8,0,4,0\
)

`defined @` MobaLedLib.h#200

I depend on these macros:

ConstrWarnLightFlash7 | PatternT14 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT14_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### ConstrWarnLightFlash8 [References: 0] Defined? True

#define ConstrWarnLightFlash8(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitT,WaitE) \
PatternT16(LED,0, InCh,8, \
MinBrightness,MaxBrightness,0,0,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitE,1,0,2,0,4,0,8,0,16,0\
,32,0,64,0,128,0)

`defined @` MobaLedLib.h#201

I depend on these macros:

ConstrWarnLightFlash8 | PatternT16 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT16_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### ConstrWarnLightFlash9 [References: 0] Defined? True

#define ConstrWarnLightFlash9(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitT,WaitE) \
PatternT18(LED,192,InCh,9, \
MinBrightness,MaxBrightness,0,0,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitE,1,0,8,0,64\
,0,0,2,0,16,0,128,0,0,4,0,32,0,0,1,0)

`defined @` MobaLedLib.h#202

I depend on these macros:

ConstrWarnLightFlash9 | PatternT18 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT18_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### ConstrWarnLightRGB6 [References: 0] Defined? True

#define ConstrWarnLightRGB6(LED,InCh,MinBrightness,MaxBrightness,OnT,WaitT,WaitE) \
PatternT12(LED,28,InCh,18,0,255,0,0,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitT,OnT,WaitE,MaxBrightness,MaxBrightness,0,MinBri\
ghtness,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinB\
rightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,\
MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MaxBrightness,MaxBrightness,0,MinBrightnes\
s,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightn\
ess,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MinBri\
ghtness,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MaxBrightness,MaxBrightness,0,MinBrightness,MinB\
rightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,\
MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightnes\
s,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MaxBrightness,MaxBrightness,0,MinBrightness,MinBrightn\
ess,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MinBri\
ghtness,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinB\
rightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MaxBrightness,MaxBrightness,0,MinBrightness,MinBrightness,0,\
MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightnes\
s,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightn\
ess,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MaxBrightness,MaxBrightness,0,MinBrightness,MinBrightness,0,MinBri\
ghtness,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinBrightness,0,MinBrightness,MinB\
rightness,0)

`defined @` MobaLedLib.h#194

I depend on these macros:

ConstrWarnLightRGB6 | PatternT12 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT12_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### CopyLED [References: 0] Defined? True

#define CopyLED(LED,InCh,SrcLED) COPYLED_T, _CHKL(LED), InCh, _CHKL(SrcLED),

`defined @` MobaLedLib.h#128

I depend on these macros:

CopyLED | COPYLED_T
_CHKL | NUM_LEDS
_ERR_LED_RANGE

### Counter [References: 0] Defined? True

#define Counter(Mode,InCh,Enable,TimeOut,...) COUNTER_T, _W2B(Mode), InCh+RAM3, Enable, \
_T2B((TimeOut)/16), COUNT_VARARGS(__VA_ARGS__), __VA_ARGS__,

`defined @` MobaLedLib.h#115

I depend on these macros:

Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B

These macros depend on me:

Counter | MonoFlop
MonoFlop2
MonoFlop2LongReset
MonoFlopInv
MonoFlopInvLongReset
MonoFlopLongReset
MonoFlopReset
PushButton2I_0_1 | PushButton2I_RGB_0_1
PushButton2I_w_LED_BL_0_1
PushButton2I_0_2 | PushButton2I_RGB_0_2
PushButton2I_w_LED_BL_0_2
PushButton2I_0_3 | PushButton2I_RGB_0_3
PushButton2I_w_LED_BL_0_3
PushButton2I_0_4 | PushButton2I_RGB_0_4
PushButton2I_w_LED_BL_0_4
PushButton2I_0_5 | PushButton2I_RGB_0_5
PushButton2I_w_LED_BL_0_5
PushButton_0_1 | PushButton_RGB_0_1
PushButton_w_LED_0_1
PushButton_w_LED_BL_0_1
PushButton_0_2 | PushButton_RGB_0_2
PushButton_w_LED_0_2
PushButton_w_LED_BL_0_2
PushButton_0_3 | PushButton_RGB_0_3
PushButton_w_LED_0_3
PushButton_w_LED_BL_0_3
PushButton_0_4 | PushButton_RGB_0_4
PushButton_w_LED_0_4
PushButton_w_LED_BL_0_4
PushButton_0_5 | PushButton_RGB_0_5
PushButton_w_LED_0_5
PushButton_w_LED_BL_0_5
RS_FlipFlop | _Herz_MoRelais_RS | Herz_MoRelais
Herz_MoRelais_I
RS_FlipFlop2
RS_FlipFlop2Timeout
RS_FlipFlopInv
RS_FlipFlopInvTimeout
RS_FlipFlopTimeout | _Herz_MoRelais_RS | Herz_MoRelais
Herz_MoRelais_I
Sound_JQ6500_BG_Next_of_N_Reset | Sound_JQ6500_BG_Next_of_N
Sound_JQ6500_BG_PlayRandom
Sound_JQ6500_Next_of_N_Reset | Sound_JQ6500_Next_of_N
Sound_JQ6500_PlayRandom
Sound_New_Next_of_N_Reset | Sound_New_Next_of_N
Sound_New_PlayRandom
Sound_Next_of_N_Reset | Sound_Next_of_N
Sound_PlayRandom
T_FlipFlop2Reset
T_FlipFlop2ResetTimeout
T_FlipFlopInvReset
T_FlipFlopInvResetTimeout
T_FlipFlopReset
T_FlipFlopResetTimeout

### DISABLE [References: 0] Defined? True

#define DISABLE _OR_NR, NOT

`defined @` MobaLedLib.h#1181

I depend on these macros:

DISABLE | NOT | _NOT_NR | SI_1
_OR_NR | SI_0

### Def_Neon_Misha [References: 0] Defined? True

#define Def_Neon_Misha(LED,InCh,Var,Min_Delay,Max_Delay) Random(Var, InCh, RM_NORMAL, \
Min_Delay, Max_Delay, 500 ms, 2000 ms) PatternT8(LED,8, Var,3,1,128,0,0,300 ms,100 \
ms,300 ms,100 ms,4 sec,400 ms,100 ms,100 ms,0,254,3,248,191,136,17,128,100)

`defined @` MobaLedLib.h#189

I depend on these macros:

Def_Neon_Misha | PatternT8 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT8_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
RM_NORMAL
Random | RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RANDOM_T
_RAND_MODE4 | RF_SLOW
_ALL_LT_MX4 | _ALL_LT_MX2 | _LT_MX | _MAX_TIMER_VAL
_Tx2B4 | _RAND_DIV4 | _ALL_LT_MX4 | _ALL_LT_MX2 | _LT_MX | _MAX_TIMER_VAL
_T2B | _W2B
ms
sec | Sec

### DepSignal4 [References: 0] Defined? True

#define DepSignal4(LED,InCh,MaxB128) InCh_to_TmpVar(InCh, 4) XPatternT1(LED,12,SI_LocalVar,5,0,MaxB128,0,0,125 \
ms,15,240,0,15,0,240,15,240,0,16 ,63,191,191,191)

`defined @` MobaLedLib.h#253

I depend on these macros:

DepSignal4 | InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### DepSignal4Bin [References: 0] Defined? True

#define DepSignal4Bin(LED,InCh,MaxB128) Bin_InCh_to_TmpVar(InCh, 2) \
XPatternT1(LED,12,SI_LocalVar,5,0,MaxB128,0,0,125 ms,15,240,0,15,0,240,15,240,0,16 \
,63,191,191,191)

`defined @` MobaLedLib.h#267

I depend on these macros:

DepSignal4Bin | Bin_InCh_to_TmpVar | BIN_INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### DepSignal4Bin_RGB [References: 0] Defined? True

#define DepSignal4Bin_RGB(LED,InCh,MaxB128) Bin_InCh_to_TmpVar(InCh, 2) \
XPatternT1(LED,12,SI_LocalVar,18,0,MaxB128,0,0,125 \
ms,0,240,0,15,0,0,0,0,0,240,0,0,0,0,0,0,0,0,240,0,0,0,0,0,0,240,15,0,240,0,0,16,17,17,1,0 \
,63,191,191,191)

`defined @` MobaLedLib.h#264

I depend on these macros:

DepSignal4Bin_RGB | Bin_InCh_to_TmpVar | BIN_INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### DepSignal4_RGB [References: 0] Defined? True

#define DepSignal4_RGB(LED,InCh,MaxB128) InCh_to_TmpVar(InCh, 4) \
XPatternT1(LED,12,SI_LocalVar,18,0,MaxB128,0,0,125 \
ms,0,240,0,15,0,0,0,0,0,240,0,0,0,0,0,0,0,0,240,0,0,0,0,0,0,240,15,0,240,0,0,16,17,17,1,0 \
,63,191,191,191)

`defined @` MobaLedLib.h#250

I depend on these macros:

DepSignal4_RGB | InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### ENABLE [References: 0] Defined? True

#define ENABLE _OR_NR,

`defined @` MobaLedLib.h#1180

I depend on these macros:

ENABLE | _OR_NR | SI_0

### EXT_PROC_BASE_T [References: 0] Defined? True

#define EXT_PROC_BASE_T 240

`defined @` Macros.h#691

### EntrySignal3 [References: 0] Defined? True

#define EntrySignal3(LED,InCh,MaxB128) InCh_to_TmpVar(InCh, 3) XPatternT1(LED,224,SI_LocalVar,3,0,MaxB128,0,0,125 \
ms,145,1 ,63,191,191)

`defined @` MobaLedLib.h#246

I depend on these macros:

EntrySignal3 | InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### EntrySignal3Bin [References: 0] Defined? True

#define EntrySignal3Bin(LED,InCh,MaxB128) Bin_InCh_to_TmpVar(InCh, 2) \
XPatternT1(LED,224,SI_LocalVar,3,0,MaxB128,0,0,125 ms,145,1 ,63,191,191)

`defined @` MobaLedLib.h#260

I depend on these macros:

EntrySignal3Bin | Bin_InCh_to_TmpVar | BIN_INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### EntrySignal3Bin_RGB [References: 0] Defined? True

#define EntrySignal3Bin_RGB(LED,InCh,MaxB128) Bin_InCh_to_TmpVar(InCh, 2) \
XPatternT1(LED,160,SI_LocalVar,9,0,MaxB128,0,0,500 ms,64,4,104,0 ,63,191,191)

`defined @` MobaLedLib.h#257

I depend on these macros:

EntrySignal3Bin_RGB | Bin_InCh_to_TmpVar | BIN_INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### EntrySignal3_RGB [References: 0] Defined? True

#define EntrySignal3_RGB(LED,InCh) EntrySignal3_RGB_BT(LED,InCh,128,125 ms)

`defined @` MobaLedLib.h#239

I depend on these macros:

EntrySignal3_RGB | EntrySignal3_RGB_BT | InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### EntrySignal3_RGB_B [References: 0] Defined? True

#define EntrySignal3_RGB_B(LED,InCh,MaxBrightness) EntrySignal3_RGB_BT(LED,InCh,MaxBrightness,125 \
ms)

`defined @` MobaLedLib.h#240

I depend on these macros:

EntrySignal3_RGB_B | EntrySignal3_RGB_BT | InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### EntrySignal3_RGB_BT [References: 0] Defined? True

#define EntrySignal3_RGB_BT(LED,InCh,MaxBrightness,FadeTime) InCh_to_TmpVar(InCh, 3) \
XPatternT1(LED,160,SI_LocalVar,9,0,MaxBrightness,0,0,FadeTime,64,4,104,0 ,63,191,191) \

`defined @` MobaLedLib.h#242

I depend on these macros:

EntrySignal3_RGB_BT | InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

These macros depend on me:

EntrySignal3_RGB_BT | EntrySignal3_RGB
EntrySignal3_RGB_B
EntrySignal3_RGB_T

### EntrySignal3_RGB_T [References: 0] Defined? True

#define EntrySignal3_RGB_T(LED,InCh,FadeTime) EntrySignal3_RGB_BT(LED,InCh,128,FadeTime)

`defined @` MobaLedLib.h#241

I depend on these macros:

EntrySignal3_RGB_T | EntrySignal3_RGB_BT | InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### FASTLED_INTERNAL [References: 0] Defined? True

#define FASTLED_INTERNAL

`defined @` MobaLedLib.h#35

### FIRE_T [References: 0] Defined? True

#define FIRE_T 139

`defined @` Macros.h#653

These macros depend on me:

FIRE_T | Fire

### Fire [References: 0] Defined? True

#define Fire(LED,InCh,LedCnt,Brightness) FIRE_T, _CHKL(LED)+RAM1+RAMN(LedCnt),_ChkIn(InCh),LedCnt,Brightness, \

`defined @` MobaLedLib.h#92

I depend on these macros:

Fire | FIRE_T
RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE

### Flash [References: 0] Defined? True

#define Flash(LED,Cx,InCh,Var,MinTime,MaxTime) Random(Var, InCh, RM_NORMAL, MinTime, \
MaxTime, 30 ms, 30 ms) Const(LED, Cx, Var, 0, 255)

`defined @` MobaLedLib.h#187

I depend on these macros:

Flash | Const | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
Sec
_Cx2LedCnt
_Cx2P_BLINK | _Cx2LedCnt
_PAT_BLINK
_NStru | _Cx2LedCnt
_Cx2StCh
_FreeBits
RM_NORMAL
Random | RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RANDOM_T
_RAND_MODE4 | RF_SLOW
_ALL_LT_MX4 | _ALL_LT_MX2 | _LT_MX | _MAX_TIMER_VAL
_Tx2B4 | _RAND_DIV4 | _ALL_LT_MX4 | _ALL_LT_MX2 | _LT_MX | _MAX_TIMER_VAL
_T2B | _W2B
ms

### GAS_LIGHT [References: 0] Defined? True

#define GAS_LIGHT 27

`defined @` MobaLedLib.h#1107

### GAS_LIGHT1 [References: 0] Defined? True

#define GAS_LIGHT1 28

`defined @` MobaLedLib.h#1108

### GAS_LIGHT1D [References: 0] Defined? True

#define GAS_LIGHT1D 32

`defined @` MobaLedLib.h#1112

### GAS_LIGHT2D [References: 0] Defined? True

#define GAS_LIGHT2D 33

`defined @` MobaLedLib.h#1113

### GAS_LIGHT3 [References: 0] Defined? True

#define GAS_LIGHT3 30

`defined @` MobaLedLib.h#1110

### GAS_LIGHT3D [References: 0] Defined? True

#define GAS_LIGHT3D 34

`defined @` MobaLedLib.h#1114

### GAS_LIGHTD [References: 0] Defined? True

#define GAS_LIGHTD 31

`defined @` MobaLedLib.h#1111

### GEN_BUTTON_RELEASE [References: 0] Defined? True

#define GEN_BUTTON_RELEASE

`defined @` leds_autoprog.h#28

### GEN_BUTTON_RELEASE_COM [References: 0] Defined? True

#define GEN_BUTTON_RELEASE_COM GEN_OFF

`defined @` leds_autoprog.h#29

### GasLights [References: 0] Defined? True

#define GasLights(LED,InCh,...) HOUSE_T, _CHKL(LED)+RAMH,_ChkIn(InCh),127, 255, GAS_MIN_T, \
GAS_MAX_T, COUNT_VARARGS(__VA_ARGS__), __VA_ARGS__,

`defined @` MobaLedLib.h#88

I depend on these macros:

GasLights | COUNT_VARARGS | _GET_NTH_ARG
HOUSE_T
RAMH | RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE

### GasLights_Inv [References: 0] Defined? True

#define GasLights_Inv(LED,InCh,...) HOUSE_T, _CHKL(LED)+RAMH,_ChkIn(InCh),127 |0x80,255, \
GAS_MIN_T, GAS_MAX_T, COUNT_VARARGS(__VA_ARGS__), __VA_ARGS__,

`defined @` MobaLedLib.h#91

I depend on these macros:

GasLights_Inv | COUNT_VARARGS | _GET_NTH_ARG
HOUSE_T
RAMH | RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE

### GleissperrsignalBin_RGB [References: 0] Defined? True

#define GleissperrsignalBin_RGB(LED,InCh,MaxB32) Bin_InCh_to_TmpVar(InCh, 1) \
XPatternT1(LED,12,SI_LocalVar,12,0,MaxB32,0,0,600 ms,0,0,0,0,0,0,0,64,0,0,64,0,0,0,0,0,0,0,51,3,0,51,3,0 \
,0,63,128,63)

`defined @` MobaLedLib.h#330

I depend on these macros:

GleissperrsignalBin_RGB | Bin_InCh_to_TmpVar | BIN_INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### Gleissperrsignal_RGB [References: 0] Defined? True

#define Gleissperrsignal_RGB(LED,InCh,MaxB32) InCh_to_TmpVar(InCh, 2) \
XPatternT1(LED,12,SI_LocalVar,12,0,MaxB32,0,0,600 ms,0,0,0,0,0,0,0,64,0,0,64,0,0,0,0,0,0,0,51,3,0,51,3,0 \
,0,63,128,63)

`defined @` MobaLedLib.h#296

I depend on these macros:

Gleissperrsignal_RGB | InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### HP_2_2Bin_RGB [References: 0] Defined? True

#define HP_2_2Bin_RGB(LED,InCh,MaxB16) Bin_InCh_to_TmpVar(InCh, 1) \
XPatternT1(LED,12,SI_LocalVar,12,0,MaxB16,0,0,500 ms,0,0,0,0,0,0,0,128,0,8,0,0,0,0,0,0,0,0,128,0,0,0,0,8 \
,0,63,128,63)

`defined @` MobaLedLib.h#336

I depend on these macros:

HP_2_2Bin_RGB | Bin_InCh_to_TmpVar | BIN_INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### HP_2_2_RGB [References: 0] Defined? True

#define HP_2_2_RGB(LED,InCh,MaxB16) InCh_to_TmpVar(InCh, 2) XPatternT1(LED,12,SI_LocalVar,12,0,MaxB16,0,0,500 \
ms,0,0,0,0,0,0,0,128,0,8,0,0,0,0,0,0,0,0,128,0,0,0,0,8 ,0,63,128,63)

`defined @` MobaLedLib.h#302

I depend on these macros:

HP_2_2_RGB | InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### HS_5_PlusBin_RGB [References: 0] Defined? True

#define HS_5_PlusBin_RGB(LED,InCh,MaxB64) Bin_InCh_to_TmpVar(InCh, 3) \
XPatternT1(LED,12,SI_LocalVar,27,0,MaxB64,0,0,500 \
ms,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,8,0,0,8,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,4,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0\
,0,0,112,5,0,0,4,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,8,0,0,0,128,136,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,112,5,0,0,4,0\
,0,0,0,0,3,0,0,3,0,0,0,0,0,0,0,0,0,0,0,0,0,112,5,0,0,4,0,0,0,52,0,0,53,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,4,0,0,0,0,0,3,0,0,3,0,0\
,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,4,0,0,0,52,0,0,53,0,0 ,0,63,128,63,128,63,128,63,128,63,128,63,128,63,128,63) \

`defined @` MobaLedLib.h#328

I depend on these macros:

HS_5_PlusBin_RGB | Bin_InCh_to_TmpVar | BIN_INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### HS_5_Plus_RGB [References: 0] Defined? True

#define HS_5_Plus_RGB(LED,InCh,MaxB64) InCh_to_TmpVar(InCh, 8) XPatternT1(LED,12,SI_LocalVar,27,0,MaxB64,0,0,500 \
ms,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,8,0,0,8,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,4,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0\
,0,0,112,5,0,0,4,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,8,0,0,0,128,136,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,112,5,0,0,4,0\
,0,0,0,0,3,0,0,3,0,0,0,0,0,0,0,0,0,0,0,0,0,112,5,0,0,4,0,0,0,52,0,0,53,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,4,0,0,0,0,0,3,0,0,3,0,0\
,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,4,0,0,0,52,0,0,53,0,0 ,0,63,128,63,128,63,128,63,128,63,128,63,128,63,128,63) \

`defined @` MobaLedLib.h#294

I depend on these macros:

HS_5_Plus_RGB | InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### HS_5lBin_RGB [References: 0] Defined? True

#define HS_5lBin_RGB(LED,InCh,MaxB64) Bin_InCh_to_TmpVar(InCh, 2) \
XPatternT1(LED,12,SI_LocalVar,15,0,MaxB64,0,0,500 \
ms,0,0,0,0,0,0,0,0,0,8,0,0,8,0,0,0,0,0,0,0,0,0,0,0,0,0,8,0,0,0,0,0,0,0,0,0,0,240,10,0,0,8,0,0,0,0,0,0,0,0,0,0,0,0,8,0,0,0,240,255 \
,0,63,128,63,128,63,128,63)

`defined @` MobaLedLib.h#324

I depend on these macros:

HS_5lBin_RGB | Bin_InCh_to_TmpVar | BIN_INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### HS_5l_RGB [References: 0] Defined? True

#define HS_5l_RGB(LED,InCh,MaxB64) InCh_to_TmpVar(InCh, 4) XPatternT1(LED,12,SI_LocalVar,15,0,MaxB64,0,0,500 \
ms,0,0,0,0,0,0,0,0,0,8,0,0,8,0,0,0,0,0,0,0,0,0,0,0,0,0,8,0,0,0,0,0,0,0,0,0,0,240,10,0,0,8,0,0,0,0,0,0,0,0,0,0,0,0,8,0,0,0,240,255 \
,0,63,128,63,128,63,128,63)

`defined @` MobaLedLib.h#290

I depend on these macros:

HS_5l_RGB | InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### HS_5rBin_RGB [References: 0] Defined? True

#define HS_5rBin_RGB(LED,InCh,MaxB64) Bin_InCh_to_TmpVar(InCh, 2) \
XPatternT1(LED,12,SI_LocalVar,15,0,MaxB64,0,0,500 \
ms,0,0,0,0,0,0,0,0,0,8,0,0,8,0,0,0,0,0,0,0,0,0,0,0,0,0,8,0,0,0,0,0,0,0,0,0,0,240,10,0,0,8,0,0,0,0,0,0,0,0,0,0,0,0,8,0,0,0,240,255 \
,0,63,128,63,128,63,128,63)

`defined @` MobaLedLib.h#326

I depend on these macros:

HS_5rBin_RGB | Bin_InCh_to_TmpVar | BIN_INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### HS_5r_RGB [References: 0] Defined? True

#define HS_5r_RGB(LED,InCh,MaxB64) InCh_to_TmpVar(InCh, 4) XPatternT1(LED,12,SI_LocalVar,15,0,MaxB64,0,0,500 \
ms,0,0,0,0,0,0,0,0,0,8,0,0,8,0,0,0,0,0,0,0,0,0,0,0,0,0,8,0,0,0,0,0,0,0,0,0,0,240,10,0,0,8,0,0,0,0,0,0,0,0,0,0,0,0,8,0,0,0,240,255 \
,0,63,128,63,128,63,128,63)

`defined @` MobaLedLib.h#292

I depend on these macros:

HS_5r_RGB | InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### HS_EinfachBin_RGB [References: 0] Defined? True

#define HS_EinfachBin_RGB(LED,InCh,MaxB32) Bin_InCh_to_TmpVar(InCh, 2) \
XPatternT1(LED,12,SI_LocalVar,12,0,MaxB32,0,0,500 \
ms,0,0,0,0,0,0,0,240,0,0,128,0,0,0,0,0,0,0,0,0,0,192,0,0,0,0,0,0,0,0,191,0,0,192,0,0 \
,0,63,128,63,128,63)

`defined @` MobaLedLib.h#332

I depend on these macros:

HS_EinfachBin_RGB | Bin_InCh_to_TmpVar | BIN_INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### HS_Einfach_RGB [References: 0] Defined? True

#define HS_Einfach_RGB(LED,InCh,MaxB32) InCh_to_TmpVar(InCh, 3) XPatternT1(LED,12,SI_LocalVar,12,0,MaxB32,0,0,500 \
ms,0,0,0,0,0,0,0,240,0,0,128,0,0,0,0,0,0,0,0,0,0,192,0,0,0,0,0,0,0,0,191,0,0,192,0,0 \
,0,63,128,63,128,63)

`defined @` MobaLedLib.h#298

I depend on these macros:

HS_Einfach_RGB | InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### Herz_2MoRelais [References: 0] Defined? True

#define Herz_2MoRelais(LED,InCh,Single_Cx,DelayHerz2) InCh_to_TmpVar1(InCh, 2) \
PatternT2(LED,_Cx2StCh(Single_Cx)+192,SI_LocalVar,2,0,255,0,0,200 ms,DelayHerz2,16,2 \
,127,128,63,128,63)

`defined @` MobaLedLib.h#680

I depend on these macros:

Herz_2MoRelais | InCh_to_TmpVar1 | INCH_TO_TMPVAR1_T
PatternT2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
_Cx2StCh
ms

### Herz_2MoRelais_I [References: 0] Defined? True

#define Herz_2MoRelais_I(LED,InCh,Single_Cx,DelayHerz2) InCh_to_TmpVar1(InCh, 2) \
PatternT2(LED,_Cx2StCh(Single_Cx)+192,SI_LocalVar,2,0,255,0,0,200 ms,DelayHerz2,32,1 \
,127,128,63,128,63)

`defined @` MobaLedLib.h#684

I depend on these macros:

Herz_2MoRelais_I | InCh_to_TmpVar1 | INCH_TO_TMPVAR1_T
PatternT2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
_Cx2StCh
ms

### Herz_BiRelais [References: 0] Defined? True

#define Herz_BiRelais(LED,InCh,Single_Cx,DelayHerz1) InCh_to_TmpVar1(InCh, 2) \
PatternT2(LED,_Cx2StCh(Single_Cx)+192,SI_LocalVar,2,0,255,0,0,200 ms,DelayHerz1,16,2 \
,127,128,1,128,1)

`defined @` MobaLedLib.h#635

I depend on these macros:

Herz_BiRelais | InCh_to_TmpVar1 | INCH_TO_TMPVAR1_T
PatternT2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
_Cx2StCh
ms

### Herz_BiRelais_I [References: 0] Defined? True

#define Herz_BiRelais_I(LED,InCh,Single_Cx,DelayHerz1) InCh_to_TmpVar1(InCh, 2) \
PatternT2(LED,_Cx2StCh(Single_Cx)+192,SI_LocalVar,2,0,255,0,0,200 ms,DelayHerz1,32,1 \
,127,128,1,128,1)

`defined @` MobaLedLib.h#639

I depend on these macros:

Herz_BiRelais_I | InCh_to_TmpVar1 | INCH_TO_TMPVAR1_T
PatternT2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
_Cx2StCh
ms

### Herz_BiRelais_I_V1_AB [References: 0] Defined? True

#define Herz_BiRelais_I_V1_AB(LED,InCh,DelayHerz1) InCh_to_TmpVar1(InCh, 2) \
PatternT2(LED,192,SI_LocalVar,2,0,255,0,0,200 ms,DelayHerz1,16,2 ,127,128,1,128,1) \

`defined @` MobaLedLib.h#608

I depend on these macros:

Herz_BiRelais_I_V1_AB | InCh_to_TmpVar1 | INCH_TO_TMPVAR1_T
PatternT2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
ms

### Herz_BiRelais_I_V1_CD [References: 0] Defined? True

#define Herz_BiRelais_I_V1_CD(LED,InCh,DelayHerz1) InCh_to_TmpVar1(InCh, 2) PatternT2(LED, \
98,SI_LocalVar,1,0,255,0,0,200 ms, DelayHerz1,16 ,127,128,1,128,1) \
PatternT2(LED+1,97,SI_LocalVar,1,0,255,0,0,200 ms, DelayHerz1,4 ,127,128,1,128,1) \

`defined @` MobaLedLib.h#618

I depend on these macros:

Herz_BiRelais_I_V1_CD | InCh_to_TmpVar1 | INCH_TO_TMPVAR1_T
PatternT2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
ms

### Herz_BiRelais_I_V1_EF [References: 0] Defined? True

#define Herz_BiRelais_I_V1_EF(LED,InCh,DelayHerz1) InCh_to_TmpVar1(InCh, 2) \
PatternT2(LED,96,SI_LocalVar,1,0,255,0,0,200 ms, DelayHerz1,16 ,127,128,1,128,1) \
PatternT2(LED,98,SI_LocalVar,1,0,255,0,0,200 ms, DelayHerz1,4 ,127,128,1,128,1)

`defined @` MobaLedLib.h#628

I depend on these macros:

Herz_BiRelais_I_V1_EF | InCh_to_TmpVar1 | INCH_TO_TMPVAR1_T
PatternT2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
ms

### Herz_BiRelais_V1_AB [References: 0] Defined? True

#define Herz_BiRelais_V1_AB(LED,InCh,DelayHerz1) InCh_to_TmpVar1(InCh, 2) \
PatternT2(LED,192,SI_LocalVar,2,0,255,0,0,200 ms, DelayHerz1,32,1 ,127,128,1,128,1) \

`defined @` MobaLedLib.h#604

I depend on these macros:

Herz_BiRelais_V1_AB | InCh_to_TmpVar1 | INCH_TO_TMPVAR1_T
PatternT2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
ms

### Herz_BiRelais_V1_CD [References: 0] Defined? True

#define Herz_BiRelais_V1_CD(LED,InCh,DelayHerz1) InCh_to_TmpVar1(InCh, 2) PatternT2(LED, \
98,SI_LocalVar,1,0,255,0,0,200 ms, DelayHerz1,4 ,127,128,1,128,1) \
PatternT2(LED+1,97,SI_LocalVar,1,0,255,0,0,200 ms, DelayHerz1,16 ,127,128,1,128,1) \

`defined @` MobaLedLib.h#613

I depend on these macros:

Herz_BiRelais_V1_CD | InCh_to_TmpVar1 | INCH_TO_TMPVAR1_T
PatternT2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
ms

### Herz_BiRelais_V1_EF [References: 0] Defined? True

#define Herz_BiRelais_V1_EF(LED,InCh,DelayHerz1) InCh_to_TmpVar1(InCh, 2) \
PatternT2(LED,96,SI_LocalVar,1,0,255,0,0,200 ms, DelayHerz1,4 ,127,128,1,128,1) \
PatternT2(LED,98,SI_LocalVar,1,0,255,0,0,200 ms, DelayHerz1,16 ,127,128,1,128,1)

`defined @` MobaLedLib.h#623

I depend on these macros:

Herz_BiRelais_V1_EF | InCh_to_TmpVar1 | INCH_TO_TMPVAR1_T
PatternT2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
ms

### Herz_MoRelais [References: 0] Defined? True

#define Herz_MoRelais(LED,InCh,Single_Cx,DelayHerz1,TmpNr) _Herz_MoRelais_RS(LED, InCh, \
Single_Cx, DelayHerz1, TmpNr, 0)

`defined @` MobaLedLib.h#655

I depend on these macros:

Herz_MoRelais | _Herz_MoRelais_RS | AND
Const | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
Sec
_Cx2LedCnt
_Cx2P_BLINK | _Cx2LedCnt
_PAT_BLINK
_NStru | _Cx2LedCnt
_Cx2StCh
_FreeBits
Logic | COUNT_VARARGS | _GET_NTH_ARG
LOGIC_T
NOT | _NOT_NR | SI_1
RS_FlipFlop | Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
_CM_RS_FlipFlop1 | CF_BINARY
CF_UP_DOWN
RS_FlipFlopTimeout | Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
_CM_RS_FlipFlop1 | CF_BINARY
CF_UP_DOWN
ms

### Herz_MoRelais_I [References: 0] Defined? True

#define Herz_MoRelais_I(LED,InCh,Single_Cx,DelayHerz1,TmpNr) _Herz_MoRelais_RS(LED, InCh, \
Single_Cx, DelayHerz1, TmpNr, 1)

`defined @` MobaLedLib.h#658

I depend on these macros:

Herz_MoRelais_I | _Herz_MoRelais_RS | AND
Const | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
Sec
_Cx2LedCnt
_Cx2P_BLINK | _Cx2LedCnt
_PAT_BLINK
_NStru | _Cx2LedCnt
_Cx2StCh
_FreeBits
Logic | COUNT_VARARGS | _GET_NTH_ARG
LOGIC_T
NOT | _NOT_NR | SI_1
RS_FlipFlop | Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
_CM_RS_FlipFlop1 | CF_BINARY
CF_UP_DOWN
RS_FlipFlopTimeout | Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
_CM_RS_FlipFlop1 | CF_BINARY
CF_UP_DOWN
ms

### House [References: 0] Defined? True

#define House(LED,InCh,On_Min,On_Limit,...) HOUSE_T, _CHKL(LED)+RAMH,_ChkIn(InCh),On_Min, \
On_Limit,HOUSE_MIN_T,HOUSE_MAX_T,COUNT_VARARGS(__VA_ARGS__), __VA_ARGS__,

`defined @` MobaLedLib.h#86

I depend on these macros:

House | COUNT_VARARGS | _GET_NTH_ARG
HOUSE_T
RAMH | RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE

### HouseT_Inv [References: 0] Defined? True

#define HouseT_Inv(LED,InCh,On_Min,On_Limit,Min_T,Max_T,...) HOUSE_T, \
_CHKL(LED)+RAMH,_ChkIn(InCh),On_Min|0x80,On_Limit,Min_T, Max_T, COUNT_VARARGS(__VA_ARGS__), \
__VA_ARGS__,

`defined @` MobaLedLib.h#90

I depend on these macros:

HouseT_Inv | COUNT_VARARGS | _GET_NTH_ARG
HOUSE_T
RAMH | RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE

### House_Inv [References: 0] Defined? True

#define House_Inv(LED,InCh,On_Min,On_Limit,...) HOUSE_T, \
_CHKL(LED)+RAMH,_ChkIn(InCh),On_Min|0x80,On_Limit,HOUSE_MIN_T,HOUSE_MAX_T,COUNT_VARARGS(__VA_ARGS__), \
__VA_ARGS__,

`defined @` MobaLedLib.h#89

I depend on these macros:

House_Inv | COUNT_VARARGS | _GET_NTH_ARG
HOUSE_T
RAMH | RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE

### INCH_TO_TMPVAR1_T [References: 0] Defined? True

#define INCH_TO_TMPVAR1_T 174

`defined @` Macros.h#669

These macros depend on me:

INCH_TO_TMPVAR1_T | InCh_to_TmpVar1 | Herz_2MoRelais
Herz_2MoRelais_I
Herz_BiRelais
Herz_BiRelais_I
Herz_BiRelais_I_V1_AB
Herz_BiRelais_I_V1_CD
Herz_BiRelais_I_V1_EF
Herz_BiRelais_V1_AB
Herz_BiRelais_V1_CD
Herz_BiRelais_V1_EF
Servo2 | Servo3 | Servo4 | Servo5
Servo5
Servo4 | Servo5
Servo5
Servo3 | Servo4 | Servo5
Servo5
Servo4 | Servo5
Servo5

### INCH_TO_TMPVAR_T [References: 0] Defined? True

#define INCH_TO_TMPVAR_T 173

`defined @` Macros.h#668

These macros depend on me:

INCH_TO_TMPVAR_T | InCh_to_TmpVar | Charlie_Buttons
DepSignal4
DepSignal4_RGB
EntrySignal3
EntrySignal3_RGB_BT | EntrySignal3_RGB
EntrySignal3_RGB_B
EntrySignal3_RGB_T
Gleissperrsignal_RGB
HP_2_2_RGB
HS_5_Plus_RGB
HS_5l_RGB
HS_5r_RGB
HS_Einfach_RGB
PushButton2I_0_1 | PushButton2I_RGB_0_1
PushButton2I_w_LED_BL_0_1
PushButton2I_0_2 | PushButton2I_RGB_0_2
PushButton2I_w_LED_BL_0_2
PushButton2I_0_3 | PushButton2I_RGB_0_3
PushButton2I_w_LED_BL_0_3
PushButton2I_0_4 | PushButton2I_RGB_0_4
PushButton2I_w_LED_BL_0_4
PushButton2I_0_5 | PushButton2I_RGB_0_5
PushButton2I_w_LED_BL_0_5
PushButton_0_1 | PushButton_RGB_0_1
PushButton_w_LED_0_1
PushButton_w_LED_BL_0_1
PushButton_0_2 | PushButton_RGB_0_2
PushButton_w_LED_0_2
PushButton_w_LED_BL_0_2
PushButton_0_3 | PushButton_RGB_0_3
PushButton_w_LED_0_3
PushButton_w_LED_BL_0_3
PushButton_0_4 | PushButton_RGB_0_4
PushButton_w_LED_0_4
PushButton_w_LED_BL_0_4
PushButton_0_5 | PushButton_RGB_0_5
PushButton_w_LED_0_5
PushButton_w_LED_BL_0_5
Vorsignal_RGB

### INP_OFF [References: 0] Defined? True

#define INP_OFF 0b00000000

`defined @` MobaLedLib.h#1195

### IS_COUNTER [References: 0] Defined? True

#define IS_COUNTER (uint8_t)0x80

`defined @` leds_autoprog.h#157

### IS_PULSE [References: 0] Defined? True

#define IS_PULSE (uint8_t)0x40

`defined @` leds_autoprog.h#158

### InCh_to_TmpVar [References: 0] Defined? True

#define InCh_to_TmpVar(FirstInCh,InCh_Cnt) INCH_TO_TMPVAR_T, FirstInCh, InCh_Cnt,

`defined @` MobaLedLib.h#144

I depend on these macros:

InCh_to_TmpVar | INCH_TO_TMPVAR_T

These macros depend on me:

InCh_to_TmpVar | Charlie_Buttons
DepSignal4
DepSignal4_RGB
EntrySignal3
EntrySignal3_RGB_BT | EntrySignal3_RGB
EntrySignal3_RGB_B
EntrySignal3_RGB_T
Gleissperrsignal_RGB
HP_2_2_RGB
HS_5_Plus_RGB
HS_5l_RGB
HS_5r_RGB
HS_Einfach_RGB
PushButton2I_0_1 | PushButton2I_RGB_0_1
PushButton2I_w_LED_BL_0_1
PushButton2I_0_2 | PushButton2I_RGB_0_2
PushButton2I_w_LED_BL_0_2
PushButton2I_0_3 | PushButton2I_RGB_0_3
PushButton2I_w_LED_BL_0_3
PushButton2I_0_4 | PushButton2I_RGB_0_4
PushButton2I_w_LED_BL_0_4
PushButton2I_0_5 | PushButton2I_RGB_0_5
PushButton2I_w_LED_BL_0_5
PushButton_0_1 | PushButton_RGB_0_1
PushButton_w_LED_0_1
PushButton_w_LED_BL_0_1
PushButton_0_2 | PushButton_RGB_0_2
PushButton_w_LED_0_2
PushButton_w_LED_BL_0_2
PushButton_0_3 | PushButton_RGB_0_3
PushButton_w_LED_0_3
PushButton_w_LED_BL_0_3
PushButton_0_4 | PushButton_RGB_0_4
PushButton_w_LED_0_4
PushButton_w_LED_BL_0_4
PushButton_0_5 | PushButton_RGB_0_5
PushButton_w_LED_0_5
PushButton_w_LED_BL_0_5
Vorsignal_RGB

### InCh_to_TmpVar1 [References: 0] Defined? True

#define InCh_to_TmpVar1(FirstInCh,InCh_Cnt) INCH_TO_TMPVAR1_T, FirstInCh, InCh_Cnt,

`defined @` MobaLedLib.h#145

I depend on these macros:

InCh_to_TmpVar1 | INCH_TO_TMPVAR1_T

These macros depend on me:

InCh_to_TmpVar1 | Herz_2MoRelais
Herz_2MoRelais_I
Herz_BiRelais
Herz_BiRelais_I
Herz_BiRelais_I_V1_AB
Herz_BiRelais_I_V1_CD
Herz_BiRelais_I_V1_EF
Herz_BiRelais_V1_AB
Herz_BiRelais_V1_CD
Herz_BiRelais_V1_EF
Servo2 | Servo3 | Servo4 | Servo5
Servo5
Servo4 | Servo5
Servo5
Servo3 | Servo4 | Servo5
Servo5
Servo4 | Servo5
Servo5

### InCnt_MSK [References: 0] Defined? True

#define InCnt_MSK 0x003F

`defined @` leds_autoprog.h#156

### KS_Hauptsignal_Zs3_Zs1 [References: 0] Defined? True

#define KS_Hauptsignal_Zs3_Zs1(LED,InCh,MaxB128) InCh_to_LocalVar(InCh, 4) \
XPatternT11(LED,128,SI_LocalVar,4,0,MaxB128,0,0,500 ms,500 ms,500 ms,500 ms,500 \
ms,500 ms,500 ms,500 ms,200 ms,500 ms,200 ms,32,64,80,160,42,2 ,0,63,128,63,128,63,128,64,0,0,1) \

`defined @` MobaLedLib.h#280

I depend on these macros:

KS_Hauptsignal_Zs3_Zs1 | SI_LocalVar | SI_0
XPatternT11 | APATTERNT11_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### KS_Hauptsignal_Zs3_Zs1Bin [References: 0] Defined? True

#define KS_Hauptsignal_Zs3_Zs1Bin(LED,InCh,MaxB128) Bin_InCh_to_TmpVar(InCh, 2) \
XPatternT11(LED,128,SI_LocalVar,4,0,MaxB128,0,0,500 ms,500 ms,500 ms,500 ms,500 \
ms,500 ms,500 ms,500 ms,200 ms,500 ms,200 ms,32,64,80,160,42,2 ,0,63,128,63,128,63,128,64,0,0,1) \

`defined @` MobaLedLib.h#314

I depend on these macros:

KS_Hauptsignal_Zs3_Zs1Bin | Bin_InCh_to_TmpVar | BIN_INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT11 | APATTERNT11_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### KS_Hauptsignal_Zs3_Zs1Bin_RGB [References: 0] Defined? True

#define KS_Hauptsignal_Zs3_Zs1Bin_RGB(LED,InCh,MaxB128) Bin_InCh_to_TmpVar(InCh, 2) \
XPatternT11(LED,128,SI_LocalVar,12,0,MaxB128,0,0,500 ms,500 ms,500 ms,500 ms,500 \
ms,500 ms,500 ms,500 ms,200 ms,500 ms,200 ms,0,128,0,0,0,8,0,112,8,0,128,224,8,142,0,8,0 \
,0,63,128,63,128,63,128,64,0,0,1)

`defined @` MobaLedLib.h#311

I depend on these macros:

KS_Hauptsignal_Zs3_Zs1Bin_RGB | Bin_InCh_to_TmpVar | BIN_INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT11 | APATTERNT11_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### KS_Hauptsignal_Zs3_Zs1_RGB [References: 0] Defined? True

#define KS_Hauptsignal_Zs3_Zs1_RGB(LED,InCh,MaxB128) InCh_to_LocalVar(InCh, 4) \
XPatternT11(LED,128,SI_LocalVar,12,0,MaxB128,0,0,500 ms,500 ms,500 ms,500 ms,500 \
ms,500 ms,500 ms,500 ms,200 ms,500 ms,200 ms,0,128,0,0,0,8,0,112,8,0,128,224,8,142,0,8,0 \
,0,63,128,63,128,63,128,64,0,0,1)

`defined @` MobaLedLib.h#277

I depend on these macros:

KS_Hauptsignal_Zs3_Zs1_RGB | SI_LocalVar | SI_0
XPatternT11 | APATTERNT11_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### KS_Hauptsignal_Zs3_Zs6_Zs1 [References: 0] Defined? True

#define KS_Hauptsignal_Zs3_Zs6_Zs1(LED,InCh,MaxB128) InCh_to_LocalVar(InCh, 4) \
XPatternT11(LED,32,SI_LocalVar,5,0,MaxB128,0,0,500 ms,500 ms,500 ms,500 ms,500 \
ms,500 ms,500 ms,500 ms,200 ms,500 ms,200 ms,64,0,2,42,80,74,8 ,0,63,128,63,128,63,128,64,0,0,1) \

`defined @` MobaLedLib.h#286

I depend on these macros:

KS_Hauptsignal_Zs3_Zs6_Zs1 | SI_LocalVar | SI_0
XPatternT11 | APATTERNT11_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### KS_Hauptsignal_Zs3_Zs6_Zs1Bin [References: 0] Defined? True

#define KS_Hauptsignal_Zs3_Zs6_Zs1Bin(LED,InCh,MaxB128) Bin_InCh_to_TmpVar(InCh, 2) \
XPatternT11(LED,32,SI_LocalVar,5,0,MaxB128,0,0,500 ms,500 ms,500 ms,500 ms,500 \
ms,500 ms,500 ms,500 ms,200 ms,500 ms,200 ms,64,0,2,42,80,74,8 ,0,63,128,63,128,63,128,64,0,0,1) \

`defined @` MobaLedLib.h#320

I depend on these macros:

KS_Hauptsignal_Zs3_Zs6_Zs1Bin | Bin_InCh_to_TmpVar | BIN_INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT11 | APATTERNT11_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### KS_Hauptsignal_Zs3_Zs6_Zs1Bin_RGB [References: 0] Defined? True

#define KS_Hauptsignal_Zs3_Zs6_Zs1Bin_RGB(LED,InCh,MaxB128) Bin_InCh_to_TmpVar(InCh, 2) \
XPatternT11(LED,96,SI_LocalVar,15,0,MaxB128,0,0,500 ms,500 ms,500 ms,500 ms,500 \
ms,500 ms,500 ms,500 ms,200 ms,500 ms,200 ms,0,0,4,0,0,0,16,0,0,56,132,3,0,16,28,8,14,4,0,2,0 \
,0,63,128,63,128,63,128,64,0,0,1)

`defined @` MobaLedLib.h#317

I depend on these macros:

KS_Hauptsignal_Zs3_Zs6_Zs1Bin_RGB | Bin_InCh_to_TmpVar | BIN_INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT11 | APATTERNT11_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### KS_Hauptsignal_Zs3_Zs6_Zs1_RGB [References: 0] Defined? True

#define KS_Hauptsignal_Zs3_Zs6_Zs1_RGB(LED,InCh,MaxB128) InCh_to_LocalVar(InCh, 4) \
XPatternT11(LED,96,SI_LocalVar,15,0,MaxB128,0,0,500 ms,500 ms,500 ms,500 ms,500 \
ms,500 ms,500 ms,500 ms,200 ms,500 ms,200 ms,0,0,4,0,0,0,16,0,0,56,132,3,0,16,28,8,14,4,0,2,0 \
,0,63,128,63,128,63,128,64,0,0,1)

`defined @` MobaLedLib.h#283

I depend on these macros:

KS_Hauptsignal_Zs3_Zs6_Zs1_RGB | SI_LocalVar | SI_0
XPatternT11 | APATTERNT11_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### KS_Vorsignal_Zs3V [References: 0] Defined? True

#define KS_Vorsignal_Zs3V(LED,InCh,MaxB128) InCh_to_LocalVar(InCh, 3) \
XPatternT9(LED,128,SI_LocalVar,4,0,MaxB128,0,0,500 ms,500 ms,500 ms,500 ms,500 \
ms,500 ms,200 ms,500 ms,200 ms,144,32,224,206,12 ,0,63,128,63,128,64,0,0,1)

`defined @` MobaLedLib.h#274

I depend on these macros:

KS_Vorsignal_Zs3V | SI_LocalVar | SI_0
XPatternT9 | APATTERNT9_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### KS_Vorsignal_Zs3VBin [References: 0] Defined? True

#define KS_Vorsignal_Zs3VBin(LED,InCh,MaxB128) Bin_InCh_to_TmpVar(InCh, 2) \
XPatternT9(LED,128,SI_LocalVar,4,0,MaxB128,0,0,500 ms,500 ms,500 ms,500 ms,500 \
ms,500 ms,200 ms,500 ms,200 ms,144,32,224,206,12 ,0,63,128,63,128,64,0,0,1)

`defined @` MobaLedLib.h#308

I depend on these macros:

KS_Vorsignal_Zs3VBin | Bin_InCh_to_TmpVar | BIN_INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT9 | APATTERNT9_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### KS_Vorsignal_Zs3VBin_RGB [References: 0] Defined? True

#define KS_Vorsignal_Zs3VBin_RGB(LED,InCh,MaxB128) Bin_InCh_to_TmpVar(InCh, 2) \
XPatternT9(LED,128,SI_LocalVar,12,0,MaxB128,0,0,500 ms,500 ms,500 ms,500 ms,500 \
ms,500 ms,200 ms,500 ms,200 ms,0,48,224,0,0,1,0,0,237,208,14,236,192,14 \
,0,63,128,63,128,64,0,0,1)

`defined @` MobaLedLib.h#305

I depend on these macros:

KS_Vorsignal_Zs3VBin_RGB | Bin_InCh_to_TmpVar | BIN_INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT9 | APATTERNT9_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### KS_Vorsignal_Zs3V_RGB [References: 0] Defined? True

#define KS_Vorsignal_Zs3V_RGB(LED,InCh,MaxB128) InCh_to_LocalVar(InCh, 3) \
XPatternT9(LED,128,SI_LocalVar,12,0,MaxB128,0,0,500 ms,500 ms,500 ms,500 ms,500 \
ms,500 ms,200 ms,500 ms,200 ms,0,48,224,0,0,1,0,0,237,208,14,236,192,14 \
,0,63,128,63,128,64,0,0,1)

`defined @` MobaLedLib.h#271

I depend on these macros:

KS_Vorsignal_Zs3V_RGB | SI_LocalVar | SI_0
XPatternT9 | APATTERNT9_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### LAST_APATTERN_T [References: 0] Defined? True

#define LAST_APATTERN_T APATTERNT64_T

`defined @` Macros.h#650

I depend on these macros:

LAST_APATTERN_T | APATTERNT64_T

### LAST_PATTERN_T [References: 0] Defined? True

#define LAST_PATTERN_T PATTERNT64_T

`defined @` Macros.h#583

I depend on these macros:

LAST_PATTERN_T | PATTERNT64_T

### LEDS_PER_CHANNEL [References: 0] Defined? True

#define LEDS_PER_CHANNEL ",32"

`defined @` leds_autoprog.h#22

### LOGIC_T [References: 0] Defined? True

#define LOGIC_T 184

`defined @` Macros.h#689

These macros depend on me:

LOGIC_T | Logic | PushButton2I_0_1 | PushButton2I_RGB_0_1
PushButton2I_w_LED_BL_0_1
PushButton2I_0_2 | PushButton2I_RGB_0_2
PushButton2I_w_LED_BL_0_2
PushButton2I_0_3 | PushButton2I_RGB_0_3
PushButton2I_w_LED_BL_0_3
PushButton2I_0_4 | PushButton2I_RGB_0_4
PushButton2I_w_LED_BL_0_4
PushButton2I_0_5 | PushButton2I_RGB_0_5
PushButton2I_w_LED_BL_0_5
_Herz_MoRelais_RS | Herz_MoRelais
Herz_MoRelais_I

### Leuchtfeuer [References: 0] Defined? True

#define Leuchtfeuer(LED,Cx,InCh) PatternT4(LED,_NStru(Cx, 4,1),InCh,_Cx2LedCnt(Cx),0, 255, \
0,0,1000 ms,500 ms,1000 ms,1500 ms,_Cx2P_DBLFL(Cx))

`defined @` MobaLedLib.h#158

I depend on these macros:

Leuchtfeuer | PatternT4 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT4_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
_Cx2LedCnt
_Cx2P_DBLFL | _Cx2LedCnt
_PAT_DBLFL | _C_ALL_not_supported
_NStru | _Cx2LedCnt
_Cx2StCh
_FreeBits
ms

### LeuchtfeuerALL [References: 0] Defined? True

#define LeuchtfeuerALL(LED,InCh) PatternT4(LED,_NStru(C_ALL,4,1),InCh,_Cx2LedCnt(C_ALL),0,255, \
0,0,1000 ms,500 ms,1000 ms,1500 ms,0b11000111, 0b00000001)

`defined @` MobaLedLib.h#159

I depend on these macros:

LeuchtfeuerALL | C_ALL | _Cx
PatternT4 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT4_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
_Cx2LedCnt
_NStru | _Cx2LedCnt
_Cx2StCh
_FreeBits
ms

### Logic [References: 0] Defined? True

#define Logic(DstVar,...) LOGIC_T, DstVar, COUNT_VARARGS(__VA_ARGS__), __VA_ARGS__,

`defined @` MobaLedLib.h#114

I depend on these macros:

Logic | COUNT_VARARGS | _GET_NTH_ARG
LOGIC_T

These macros depend on me:

Logic | PushButton2I_0_1 | PushButton2I_RGB_0_1
PushButton2I_w_LED_BL_0_1
PushButton2I_0_2 | PushButton2I_RGB_0_2
PushButton2I_w_LED_BL_0_2
PushButton2I_0_3 | PushButton2I_RGB_0_3
PushButton2I_w_LED_BL_0_3
PushButton2I_0_4 | PushButton2I_RGB_0_4
PushButton2I_w_LED_BL_0_4
PushButton2I_0_5 | PushButton2I_RGB_0_5
PushButton2I_w_LED_BL_0_5
_Herz_MoRelais_RS | Herz_MoRelais
Herz_MoRelais_I

### Min [References: 0] Defined? True

#define Min *60000L

`defined @` MobaLedLib.h#1014

### MobaLedLibPtr_Create [References: 0] Defined? True

#define MobaLedLibPtr_Create(leds) pMobaLedLib = new MobaLedLib_C(leds, sizeof(leds)/sizeof(CRGB), \
Config, Config_RAM, sizeof(Config_RAM)); MobaLedLib_C& MobaLedLib = *pMobaLedLib; \

`defined @` MobaLedLib.h#948

### MobaLedLib_Copy_to_InpStruct [References: 0] Defined? True

#define MobaLedLib_Copy_to_InpStruct(Src,ByteCnt,ChannelNr) MobaLedLib.Copy_Bits_to_InpStructArray(Src, \
ByteCnt, _ConvChannelNr2Byte(ChannelNr))

`defined @` MobaLedLib.h#960

I depend on these macros:

MobaLedLib_Copy_to_InpStruct | _ConvChannelNr2Byte

### MobaLedLib_Create [References: 0] Defined? True

#define MobaLedLib_Create(leds) uint8_t Config_RAM[__COUNTER__/2]; MobaLedLib_C MobaLedLib(leds, \
sizeof(leds)/sizeof(CRGB), Config, Config_RAM, sizeof(Config_RAM));

`defined @` MobaLedLib.h#946

### MobaLedLib_Prepare [References: 0] Defined? True

#define MobaLedLib_Prepare() MobaLedLib_C* pMobaLedLib; uint8_t Config_RAM[__COUNTER__/2]; \

`defined @` MobaLedLib.h#921

### MobaLedLib_Ver [References: 0] Defined? True

#define MobaLedLib_Ver 3.0.0

`defined @` MobaLedLib.h#33

### MonoFlop [References: 0] Defined? True

#define MonoFlop(DstVar,InCh,Duration) Counter(_CM_RS_FlipFlop1, InCh, SI_0, Duration, \
DstVar)

`defined @` MobaLedLib.h#355

I depend on these macros:

MonoFlop | Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
SI_0
_CM_RS_FlipFlop1 | CF_BINARY
CF_UP_DOWN

### MonoFlop2 [References: 0] Defined? True

#define MonoFlop2(DstVar0,DstVar1,InCh,Duration) Counter(_CM_RS_FlipFlop2, InCh, SI_0, \
Duration, DstVar0, DstVar1)

`defined @` MobaLedLib.h#372

I depend on these macros:

MonoFlop2 | Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
SI_0
_CM_RS_FlipFlop2 | CF_UP_DOWN

### MonoFlop2LongReset [References: 0] Defined? True

#define MonoFlop2LongReset(DstVar0,DstVar1,InCh,Duration) Counter(_CM_RS_FlipFlop2|CF_RESET_LONG, \
InCh, SI_0, Duration, DstVar0, DstVar1)

`defined @` MobaLedLib.h#373

I depend on these macros:

MonoFlop2LongReset | CF_RESET_LONG
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
SI_0
_CM_RS_FlipFlop2 | CF_UP_DOWN

### MonoFlopInv [References: 0] Defined? True

#define MonoFlopInv(DstVar,InCh,Duration) Counter(_CM_RS_FlipFlop2, InCh, SI_0, Duration, \
DstVar, DstVar)

`defined @` MobaLedLib.h#364

I depend on these macros:

MonoFlopInv | Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
SI_0
_CM_RS_FlipFlop2 | CF_UP_DOWN

### MonoFlopInvLongReset [References: 0] Defined? True

#define MonoFlopInvLongReset(DstVar,InCh,Duration) Counter(_CM_RS_FlipFlop2|CF_RESET_LONG, \
InCh, SI_0, Duration, DstVar, DstVar)

`defined @` MobaLedLib.h#365

I depend on these macros:

MonoFlopInvLongReset | CF_RESET_LONG
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
SI_0
_CM_RS_FlipFlop2 | CF_UP_DOWN

### MonoFlopLongReset [References: 0] Defined? True

#define MonoFlopLongReset(DstVar,InCh,Duration) Counter(_CM_RS_FlipFlop1|CF_RESET_LONG, \
InCh, SI_0, Duration, DstVar)

`defined @` MobaLedLib.h#357

I depend on these macros:

MonoFlopLongReset | CF_RESET_LONG
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
SI_0
_CM_RS_FlipFlop1 | CF_BINARY
CF_UP_DOWN

### MonoFlopReset [References: 0] Defined? True

#define MonoFlopReset(DstVar,InCh,R_InCh,Duration) Counter(_CM_RS_FlipFlop1, InCh, R_InCh, \
Duration, DstVar)

`defined @` MobaLedLib.h#356

I depend on these macros:

MonoFlopReset | Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
_CM_RS_FlipFlop1 | CF_BINARY
CF_UP_DOWN

### Ms [References: 0] Defined? True

#define Ms

`defined @` MobaLedLib.h#1019

### NEON_DEF1D [References: 0] Defined? True

#define NEON_DEF1D 52

`defined @` MobaLedLib.h#1132

### NEON_DEF2D [References: 0] Defined? True

#define NEON_DEF2D 53

`defined @` MobaLedLib.h#1133

### NEON_DEF3D [References: 0] Defined? True

#define NEON_DEF3D 54

`defined @` MobaLedLib.h#1134

### NEON_DEF_D [References: 0] Defined? True

#define NEON_DEF_D 51

`defined @` MobaLedLib.h#1131

### NEON_LIGHT1 [References: 0] Defined? True

#define NEON_LIGHT1 36

`defined @` MobaLedLib.h#1116

### NEON_LIGHT1D [References: 0] Defined? True

#define NEON_LIGHT1D 40

`defined @` MobaLedLib.h#1120

### NEON_LIGHT1L [References: 0] Defined? True

#define NEON_LIGHT1L 48

`defined @` MobaLedLib.h#1128

### NEON_LIGHT1M [References: 0] Defined? True

#define NEON_LIGHT1M 44

`defined @` MobaLedLib.h#1124

### NEON_LIGHT2 [References: 0] Defined? True

#define NEON_LIGHT2 37

`defined @` MobaLedLib.h#1117

### NEON_LIGHT2D [References: 0] Defined? True

#define NEON_LIGHT2D 41

`defined @` MobaLedLib.h#1121

### NEON_LIGHT2L [References: 0] Defined? True

#define NEON_LIGHT2L 49

`defined @` MobaLedLib.h#1129

### NEON_LIGHT2M [References: 0] Defined? True

#define NEON_LIGHT2M 45

`defined @` MobaLedLib.h#1125

### NEON_LIGHT3 [References: 0] Defined? True

#define NEON_LIGHT3 38

`defined @` MobaLedLib.h#1118

### NEON_LIGHT3D [References: 0] Defined? True

#define NEON_LIGHT3D 42

`defined @` MobaLedLib.h#1122

### NEON_LIGHT3L [References: 0] Defined? True

#define NEON_LIGHT3L 50

`defined @` MobaLedLib.h#1130

### NEON_LIGHT3M [References: 0] Defined? True

#define NEON_LIGHT3M 46

`defined @` MobaLedLib.h#1126

### NEON_LIGHTL [References: 0] Defined? True

#define NEON_LIGHTL 47

`defined @` MobaLedLib.h#1127

### NEON_LIGHTM [References: 0] Defined? True

#define NEON_LIGHTM 43

`defined @` MobaLedLib.h#1123

### NEW_LOCAL_VAR_T [References: 0] Defined? True

#define NEW_LOCAL_VAR_T 171

`defined @` Macros.h#661

These macros depend on me:

NEW_LOCAL_VAR_T | New_Local_Var | Sound_JQ6500_BG_Next_of_N_Reset | Sound_JQ6500_BG_Next_of_N
Sound_JQ6500_BG_PlayRandom
Sound_JQ6500_Next_of_N_Reset | Sound_JQ6500_Next_of_N
Sound_JQ6500_PlayRandom
Sound_New_Next_of_N_Reset | Sound_New_Next_of_N
Sound_New_PlayRandom
Sound_Next_of_N_Reset | Sound_Next_of_N
Sound_PlayRandom

### NOT [References: 0] Defined? True

#define NOT _NOT_NR,

`defined @` MobaLedLib.h#1178

I depend on these macros:

NOT | _NOT_NR | SI_1

These macros depend on me:

NOT | DISABLE
_Herz_MoRelais_RS | Herz_MoRelais
Herz_MoRelais_I

### New_Local_Var [References: 0] Defined? True

#define New_Local_Var() NEW_LOCAL_VAR_T+RAM2,

`defined @` MobaLedLib.h#132

I depend on these macros:

New_Local_Var | NEW_LOCAL_VAR_T
RAM2 | RAM1

These macros depend on me:

New_Local_Var | Sound_JQ6500_BG_Next_of_N_Reset | Sound_JQ6500_BG_Next_of_N
Sound_JQ6500_BG_PlayRandom
Sound_JQ6500_Next_of_N_Reset | Sound_JQ6500_Next_of_N
Sound_JQ6500_PlayRandom
Sound_New_Next_of_N_Reset | Sound_New_Next_of_N
Sound_New_PlayRandom
Sound_Next_of_N_Reset | Sound_Next_of_N
Sound_PlayRandom

### OR [References: 0] Defined? True

#define OR ,_OR_NR,

`defined @` MobaLedLib.h#1177

I depend on these macros:

OR | _OR_NR | SI_0

These macros depend on me:

OR | PushButton2I_0_1 | PushButton2I_RGB_0_1
PushButton2I_w_LED_BL_0_1
PushButton2I_0_2 | PushButton2I_RGB_0_2
PushButton2I_w_LED_BL_0_2
PushButton2I_0_3 | PushButton2I_RGB_0_3
PushButton2I_w_LED_BL_0_3
PushButton2I_0_4 | PushButton2I_RGB_0_4
PushButton2I_w_LED_BL_0_4
PushButton2I_0_5 | PushButton2I_RGB_0_5
PushButton2I_w_LED_BL_0_5

### O_RET_MSG [References: 0] Defined? True

#define O_RET_MSG (uint16_t)(3<<14)

`defined @` leds_autoprog.h#39

### PATTERNT10_T [References: 0] Defined? True

#define PATTERNT10_T 19

`defined @` Macros.h#528

These macros depend on me:

PATTERNT10_T | PatternT10 | ConstrWarnLight9
ConstrWarnLightFlash5
PatternTE10

### PATTERNT11_T [References: 0] Defined? True

#define PATTERNT11_T 20

`defined @` Macros.h#529

These macros depend on me:

PATTERNT11_T | PatternT11 | ConstrWarnLight10
PatternTE11

### PATTERNT12_T [References: 0] Defined? True

#define PATTERNT12_T 21

`defined @` Macros.h#530

These macros depend on me:

PATTERNT12_T | PatternT12 | ConstrWarnLight11
ConstrWarnLightFlash6
ConstrWarnLightRGB6
RGB_AmpelX_A
PatternTE12

### PATTERNT13_T [References: 0] Defined? True

#define PATTERNT13_T 22

`defined @` Macros.h#531

These macros depend on me:

PATTERNT13_T | PatternT13 | ConstrWarnLight12
PatternTE13

### PATTERNT14_T [References: 0] Defined? True

#define PATTERNT14_T 23

`defined @` Macros.h#532

These macros depend on me:

PATTERNT14_T | PatternT14 | ConstrWarnLight13
ConstrWarnLightFlash7
PatternTE14

### PATTERNT15_T [References: 0] Defined? True

#define PATTERNT15_T 24

`defined @` Macros.h#533

These macros depend on me:

PATTERNT15_T | PatternT15 | ConstrWarnLight14
PatternTE15

### PATTERNT16_T [References: 0] Defined? True

#define PATTERNT16_T 25

`defined @` Macros.h#534

These macros depend on me:

PATTERNT16_T | PatternT16 | ConstrWarnLight15
ConstrWarnLightFlash8
PatternTE16

### PATTERNT17_T [References: 0] Defined? True

#define PATTERNT17_T 26

`defined @` Macros.h#535

These macros depend on me:

PATTERNT17_T | PatternT17
PatternTE17

### PATTERNT18_T [References: 0] Defined? True

#define PATTERNT18_T 27

`defined @` Macros.h#536

These macros depend on me:

PATTERNT18_T | PatternT18 | ConstrWarnLightFlash9
PatternTE18

### PATTERNT19_T [References: 0] Defined? True

#define PATTERNT19_T 28

`defined @` Macros.h#537

These macros depend on me:

PATTERNT19_T | PatternT19
PatternTE19

### PATTERNT20_T [References: 0] Defined? True

#define PATTERNT20_T 29

`defined @` Macros.h#538

These macros depend on me:

PATTERNT20_T | PatternT20 | ConstrWarnLightFlash10
PatternTE20

### PATTERNT21_T [References: 0] Defined? True

#define PATTERNT21_T 30

`defined @` Macros.h#539

These macros depend on me:

PATTERNT21_T | PatternT21
PatternTE21

### PATTERNT22_T [References: 0] Defined? True

#define PATTERNT22_T 31

`defined @` Macros.h#540

These macros depend on me:

PATTERNT22_T | PatternT22 | ConstrWarnLightFlash11
PatternTE22

### PATTERNT23_T [References: 0] Defined? True

#define PATTERNT23_T 32

`defined @` Macros.h#541

These macros depend on me:

PATTERNT23_T | PatternT23
PatternTE23

### PATTERNT24_T [References: 0] Defined? True

#define PATTERNT24_T 33

`defined @` Macros.h#542

These macros depend on me:

PATTERNT24_T | PatternT24 | ConstrWarnLightFlash12
PatternTE24

### PATTERNT25_T [References: 0] Defined? True

#define PATTERNT25_T 34

`defined @` Macros.h#543

These macros depend on me:

PATTERNT25_T | PatternT25
PatternTE25

### PATTERNT26_T [References: 0] Defined? True

#define PATTERNT26_T 35

`defined @` Macros.h#544

These macros depend on me:

PATTERNT26_T | PatternT26 | ConstrWarnLightFlash13
PatternTE26

### PATTERNT27_T [References: 0] Defined? True

#define PATTERNT27_T 36

`defined @` Macros.h#545

These macros depend on me:

PATTERNT27_T | PatternT27
PatternTE27

### PATTERNT28_T [References: 0] Defined? True

#define PATTERNT28_T 37

`defined @` Macros.h#546

These macros depend on me:

PATTERNT28_T | PatternT28 | ConstrWarnLightFlash14
PatternTE28

### PATTERNT29_T [References: 0] Defined? True

#define PATTERNT29_T 38

`defined @` Macros.h#547

These macros depend on me:

PATTERNT29_T | PatternT29
PatternTE29

### PATTERNT2_T [References: 0] Defined? True

#define PATTERNT2_T 11

`defined @` Macros.h#520

These macros depend on me:

PATTERNT2_T | PatternT2 | Blink2
Blink3
Herz_2MoRelais
Herz_2MoRelais_I
Herz_BiRelais
Herz_BiRelais_I
Herz_BiRelais_I_V1_AB
Herz_BiRelais_I_V1_CD
Herz_BiRelais_I_V1_EF
Herz_BiRelais_V1_AB
Herz_BiRelais_V1_CD
Herz_BiRelais_V1_EF
Sound_ADKeyTime | Sound_DecVol
Sound_IncVol
Sound_New_DecVol
Sound_New_IncVol
Sound_JQ6500_ADKeyTime | Sound_JQ6500_BG_DecVol
Sound_JQ6500_BG_IncVol
Sound_JQ6500_DecVol
Sound_JQ6500_IncVol
PatternTE2 | Sound_ADKey | Sound_Loop
Sound_New_Loop
Sound_New_Next
Sound_New_PausePlay
Sound_New_PlayMode
Sound_New_Prev
Sound_New_Seq1
Sound_New_Seq10
Sound_New_Seq11
Sound_New_Seq12
Sound_New_Seq13
Sound_New_Seq14
Sound_New_Seq2
Sound_New_Seq3
Sound_New_Seq4
Sound_New_Seq5
Sound_New_Seq6
Sound_New_Seq7
Sound_New_Seq8
Sound_New_Seq9
Sound_New_USDSPI
Sound_Next
Sound_PausePlay
Sound_PlayMode
Sound_Prev
Sound_Seq1
Sound_Seq10
Sound_Seq11
Sound_Seq12
Sound_Seq13
Sound_Seq14
Sound_Seq2
Sound_Seq3
Sound_Seq4
Sound_Seq5
Sound_Seq6
Sound_Seq7
Sound_Seq8
Sound_Seq9
Sound_USDSPI
Sound_JQ6500_ADKey | Sound_JQ6500_BG_Next
Sound_JQ6500_BG_Prev
Sound_JQ6500_BG_Seq1
Sound_JQ6500_BG_Seq2
Sound_JQ6500_BG_Seq3
Sound_JQ6500_BG_Seq4
Sound_JQ6500_BG_Seq5
Sound_JQ6500_Next
Sound_JQ6500_Prev
Sound_JQ6500_Seq1
Sound_JQ6500_Seq2
Sound_JQ6500_Seq3
Sound_JQ6500_Seq4
Sound_JQ6500_Seq5

### PATTERNT30_T [References: 0] Defined? True

#define PATTERNT30_T 39

`defined @` Macros.h#548

These macros depend on me:

PATTERNT30_T | PatternT30 | ConstrWarnLightFlash15
PatternTE30

### PATTERNT31_T [References: 0] Defined? True

#define PATTERNT31_T 40

`defined @` Macros.h#549

These macros depend on me:

PATTERNT31_T | PatternT31
PatternTE31

### PATTERNT32_T [References: 0] Defined? True

#define PATTERNT32_T 41

`defined @` Macros.h#550

These macros depend on me:

PATTERNT32_T | PatternT32
PatternTE32

### PATTERNT33_T [References: 0] Defined? True

#define PATTERNT33_T 42

`defined @` Macros.h#551

These macros depend on me:

PATTERNT33_T | PatternT33
PatternTE33

### PATTERNT34_T [References: 0] Defined? True

#define PATTERNT34_T 43

`defined @` Macros.h#552

These macros depend on me:

PATTERNT34_T | PatternT34
PatternTE34

### PATTERNT35_T [References: 0] Defined? True

#define PATTERNT35_T 44

`defined @` Macros.h#553

These macros depend on me:

PATTERNT35_T | PatternT35
PatternTE35

### PATTERNT36_T [References: 0] Defined? True

#define PATTERNT36_T 45

`defined @` Macros.h#554

These macros depend on me:

PATTERNT36_T | PatternT36
PatternTE36

### PATTERNT37_T [References: 0] Defined? True

#define PATTERNT37_T 46

`defined @` Macros.h#555

These macros depend on me:

PATTERNT37_T | PatternT37
PatternTE37

### PATTERNT38_T [References: 0] Defined? True

#define PATTERNT38_T 47

`defined @` Macros.h#556

These macros depend on me:

PATTERNT38_T | PatternT38
PatternTE38

### PATTERNT39_T [References: 0] Defined? True

#define PATTERNT39_T 48

`defined @` Macros.h#557

These macros depend on me:

PATTERNT39_T | PatternT39
PatternTE39

### PATTERNT3_T [References: 0] Defined? True

#define PATTERNT3_T 12

`defined @` Macros.h#521

These macros depend on me:

PATTERNT3_T | PatternT3
PatternTE3

### PATTERNT40_T [References: 0] Defined? True

#define PATTERNT40_T 49

`defined @` Macros.h#558

These macros depend on me:

PATTERNT40_T | PatternT40
PatternTE40

### PATTERNT41_T [References: 0] Defined? True

#define PATTERNT41_T 50

`defined @` Macros.h#559

These macros depend on me:

PATTERNT41_T | PatternT41
PatternTE41

### PATTERNT42_T [References: 0] Defined? True

#define PATTERNT42_T 51

`defined @` Macros.h#560

These macros depend on me:

PATTERNT42_T | PatternT42
PatternTE42

### PATTERNT43_T [References: 0] Defined? True

#define PATTERNT43_T 52

`defined @` Macros.h#561

These macros depend on me:

PATTERNT43_T | PatternT43
PatternTE43

### PATTERNT44_T [References: 0] Defined? True

#define PATTERNT44_T 53

`defined @` Macros.h#562

These macros depend on me:

PATTERNT44_T | PatternT44
PatternTE44

### PATTERNT45_T [References: 0] Defined? True

#define PATTERNT45_T 54

`defined @` Macros.h#563

These macros depend on me:

PATTERNT45_T | PatternT45
PatternTE45

### PATTERNT46_T [References: 0] Defined? True

#define PATTERNT46_T 55

`defined @` Macros.h#564

These macros depend on me:

PATTERNT46_T | PatternT46
PatternTE46

### PATTERNT47_T [References: 0] Defined? True

#define PATTERNT47_T 56

`defined @` Macros.h#565

These macros depend on me:

PATTERNT47_T | PatternT47
PatternTE47

### PATTERNT48_T [References: 0] Defined? True

#define PATTERNT48_T 57

`defined @` Macros.h#566

These macros depend on me:

PATTERNT48_T | PatternT48
PatternTE48

### PATTERNT49_T [References: 0] Defined? True

#define PATTERNT49_T 58

`defined @` Macros.h#567

These macros depend on me:

PATTERNT49_T | PatternT49
PatternTE49

### PATTERNT4_T [References: 0] Defined? True

#define PATTERNT4_T 13

`defined @` Macros.h#522

These macros depend on me:

PATTERNT4_T | PatternT4 | AmpelX
BlueLight1
BlueLight2
ConstrWarnLight3
Leuchtfeuer
LeuchtfeuerALL
RGB_AmpelX
PatternTE4

### PATTERNT50_T [References: 0] Defined? True

#define PATTERNT50_T 59

`defined @` Macros.h#568

These macros depend on me:

PATTERNT50_T | PatternT50
PatternTE50

### PATTERNT51_T [References: 0] Defined? True

#define PATTERNT51_T 60

`defined @` Macros.h#569

These macros depend on me:

PATTERNT51_T | PatternT51
PatternTE51

### PATTERNT52_T [References: 0] Defined? True

#define PATTERNT52_T 61

`defined @` Macros.h#570

These macros depend on me:

PATTERNT52_T | PatternT52
PatternTE52

### PATTERNT53_T [References: 0] Defined? True

#define PATTERNT53_T 62

`defined @` Macros.h#571

These macros depend on me:

PATTERNT53_T | PatternT53
PatternTE53

### PATTERNT54_T [References: 0] Defined? True

#define PATTERNT54_T 63

`defined @` Macros.h#572

These macros depend on me:

PATTERNT54_T | PatternT54
PatternTE54

### PATTERNT55_T [References: 0] Defined? True

#define PATTERNT55_T 64

`defined @` Macros.h#573

These macros depend on me:

PATTERNT55_T | PatternT55
PatternTE55

### PATTERNT56_T [References: 0] Defined? True

#define PATTERNT56_T 65

`defined @` Macros.h#574

These macros depend on me:

PATTERNT56_T | PatternT56
PatternTE56

### PATTERNT57_T [References: 0] Defined? True

#define PATTERNT57_T 66

`defined @` Macros.h#575

These macros depend on me:

PATTERNT57_T | PatternT57
PatternTE57

### PATTERNT58_T [References: 0] Defined? True

#define PATTERNT58_T 67

`defined @` Macros.h#576

These macros depend on me:

PATTERNT58_T | PatternT58
PatternTE58

### PATTERNT59_T [References: 0] Defined? True

#define PATTERNT59_T 68

`defined @` Macros.h#577

These macros depend on me:

PATTERNT59_T | PatternT59
PatternTE59

### PATTERNT5_T [References: 0] Defined? True

#define PATTERNT5_T 14

`defined @` Macros.h#523

These macros depend on me:

PATTERNT5_T | PatternT5 | ConstrWarnLight4
PatternTE5

### PATTERNT60_T [References: 0] Defined? True

#define PATTERNT60_T 69

`defined @` Macros.h#578

These macros depend on me:

PATTERNT60_T | PatternT60
PatternTE60

### PATTERNT61_T [References: 0] Defined? True

#define PATTERNT61_T 70

`defined @` Macros.h#579

These macros depend on me:

PATTERNT61_T | PatternT61
PatternTE61

### PATTERNT62_T [References: 0] Defined? True

#define PATTERNT62_T 71

`defined @` Macros.h#580

These macros depend on me:

PATTERNT62_T | PatternT62
PatternTE62

### PATTERNT63_T [References: 0] Defined? True

#define PATTERNT63_T 72

`defined @` Macros.h#581

These macros depend on me:

PATTERNT63_T | PatternT63
PatternTE63

### PATTERNT64_T [References: 0] Defined? True

#define PATTERNT64_T 73

`defined @` Macros.h#582

These macros depend on me:

PATTERNT64_T | LAST_PATTERN_T
PatternT64
PatternTE64

### PATTERNT6_T [References: 0] Defined? True

#define PATTERNT6_T 15

`defined @` Macros.h#524

These macros depend on me:

PATTERNT6_T | PatternT6 | ConstrWarnLight5
ConstrWarnLightFlash3
PatternTE6

### PATTERNT7_T [References: 0] Defined? True

#define PATTERNT7_T 16

`defined @` Macros.h#525

These macros depend on me:

PATTERNT7_T | PatternT7 | ConstrWarnLight6
PatternTE7

### PATTERNT8_T [References: 0] Defined? True

#define PATTERNT8_T 17

`defined @` Macros.h#526

These macros depend on me:

PATTERNT8_T | PatternT8 | ConstrWarnLight7
ConstrWarnLightFlash4
Def_Neon_Misha
PatternTE8

### PATTERNT9_T [References: 0] Defined? True

#define PATTERNT9_T 18

`defined @` Macros.h#527

These macros depend on me:

PATTERNT9_T | PatternT9 | ConstrWarnLight8
PatternTE9

### PF_INVERT_INP [References: 0] Defined? True

#define PF_INVERT_INP 0x80

`defined @` MobaLedLib.h#1042

These macros depend on me:

PF_INVERT_INP | BlinkerInvInp

### PF_NO_SWITCH_OFF [References: 0] Defined? True

#define PF_NO_SWITCH_OFF 0x10

`defined @` MobaLedLib.h#1039

### PF_SLOW [References: 0] Defined? True

#define PF_SLOW 0x40

`defined @` MobaLedLib.h#1041

These macros depend on me:

PF_SLOW | Blink2
Blink3
Blinker
BlinkerHD
BlinkerInvInp
Button
ButtonNOff

### PM_MODE_MASK [References: 0] Defined? True

#define PM_MODE_MASK 0x07

`defined @` MobaLedLib.h#1030

### PM_PINGPONG [References: 0] Defined? True

#define PM_PINGPONG 5

`defined @` MobaLedLib.h#1027

### PM_RES [References: 0] Defined? True

#define PM_RES 7

`defined @` MobaLedLib.h#1029

### PM_SEQUENCE_NO_RESTART [References: 0] Defined? True

#define PM_SEQUENCE_NO_RESTART 3

`defined @` MobaLedLib.h#1034

### PM_SEQUENCE_STOP [References: 0] Defined? True

#define PM_SEQUENCE_STOP 4

`defined @` MobaLedLib.h#1035

### PM_SEQUENCE_W_ABORT [References: 0] Defined? True

#define PM_SEQUENCE_W_ABORT 2

`defined @` MobaLedLib.h#1033

### PM_SEQUENCE_W_RESTART [References: 0] Defined? True

#define PM_SEQUENCE_W_RESTART 1

`defined @` MobaLedLib.h#1032

### PM_SEQUENZ_NO_RESTART [References: 0] Defined? True

#define PM_SEQUENZ_NO_RESTART 3

`defined @` MobaLedLib.h#1025

These macros depend on me:

PM_SEQUENZ_NO_RESTART | ButtonNOff
Sound_ADKey | Sound_Loop
Sound_New_Loop
Sound_New_Next
Sound_New_PausePlay
Sound_New_PlayMode
Sound_New_Prev
Sound_New_Seq1
Sound_New_Seq10
Sound_New_Seq11
Sound_New_Seq12
Sound_New_Seq13
Sound_New_Seq14
Sound_New_Seq2
Sound_New_Seq3
Sound_New_Seq4
Sound_New_Seq5
Sound_New_Seq6
Sound_New_Seq7
Sound_New_Seq8
Sound_New_Seq9
Sound_New_USDSPI
Sound_Next
Sound_PausePlay
Sound_PlayMode
Sound_Prev
Sound_Seq1
Sound_Seq10
Sound_Seq11
Sound_Seq12
Sound_Seq13
Sound_Seq14
Sound_Seq2
Sound_Seq3
Sound_Seq4
Sound_Seq5
Sound_Seq6
Sound_Seq7
Sound_Seq8
Sound_Seq9
Sound_USDSPI
Sound_ADKeyTime | Sound_DecVol
Sound_IncVol
Sound_New_DecVol
Sound_New_IncVol
Sound_JQ6500_ADKey | Sound_JQ6500_BG_Next
Sound_JQ6500_BG_Prev
Sound_JQ6500_BG_Seq1
Sound_JQ6500_BG_Seq2
Sound_JQ6500_BG_Seq3
Sound_JQ6500_BG_Seq4
Sound_JQ6500_BG_Seq5
Sound_JQ6500_Next
Sound_JQ6500_Prev
Sound_JQ6500_Seq1
Sound_JQ6500_Seq2
Sound_JQ6500_Seq3
Sound_JQ6500_Seq4
Sound_JQ6500_Seq5
Sound_JQ6500_ADKeyTime | Sound_JQ6500_BG_DecVol
Sound_JQ6500_BG_IncVol
Sound_JQ6500_DecVol
Sound_JQ6500_IncVol

### PM_SEQUENZ_STOP [References: 0] Defined? True

#define PM_SEQUENZ_STOP 4

`defined @` MobaLedLib.h#1026

### PM_SEQUENZ_W_ABORT [References: 0] Defined? True

#define PM_SEQUENZ_W_ABORT 2

`defined @` MobaLedLib.h#1024

These macros depend on me:

PM_SEQUENZ_W_ABORT | Button

### PM_SEQUENZ_W_RESTART [References: 0] Defined? True

#define PM_SEQUENZ_W_RESTART 1

`defined @` MobaLedLib.h#1023

### PatternT10 [References: 0] Defined? True

#define PatternT10(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,...) \
PATTERNT10_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#121

I depend on these macros:

PatternT10 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT10_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

These macros depend on me:

PatternT10 | ConstrWarnLight9
ConstrWarnLightFlash5

### PatternT11 [References: 0] Defined? True

#define PatternT11(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,...) \
PATTERNT11_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_W2B(COUNT_VARARGS(__VA_ARGS__)\
), __VA_ARGS__,

`defined @` Macros.h#122

I depend on these macros:

PatternT11 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT11_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

These macros depend on me:

PatternT11 | ConstrWarnLight10

### PatternT12 [References: 0] Defined? True

#define PatternT12(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,...) \
PATTERNT12_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_W2B(COUNT_VARARGS(__\
VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#123

I depend on these macros:

PatternT12 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT12_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

These macros depend on me:

PatternT12 | ConstrWarnLight11
ConstrWarnLightFlash6
ConstrWarnLightRGB6
RGB_AmpelX_A

### PatternT13 [References: 0] Defined? True

#define PatternT13(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,...) \
PATTERNT13_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_W2B(COUNT_\
VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#124

I depend on these macros:

PatternT13 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT13_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

These macros depend on me:

PatternT13 | ConstrWarnLight12

### PatternT14 [References: 0] Defined? True

#define PatternT14(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,...) \
PATTERNT14_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#125

I depend on these macros:

PatternT14 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT14_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

These macros depend on me:

PatternT14 | ConstrWarnLight13
ConstrWarnLightFlash7

### PatternT15 [References: 0] Defined? True

#define PatternT15(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,...) \
PATTERNT15_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#126

I depend on these macros:

PatternT15 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT15_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

These macros depend on me:

PatternT15 | ConstrWarnLight14

### PatternT16 [References: 0] Defined? True

#define PatternT16(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,...) \
PATTERNT16_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#127

I depend on these macros:

PatternT16 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT16_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

These macros depend on me:

PatternT16 | ConstrWarnLight15
ConstrWarnLightFlash8

### PatternT17 [References: 0] Defined? True

#define PatternT17(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,...) \
PATTERNT17_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#128

I depend on these macros:

PatternT17 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT17_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT18 [References: 0] Defined? True

#define PatternT18(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,...) \
PATTERNT18_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__, \

`defined @` Macros.h#129

I depend on these macros:

PatternT18 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT18_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

These macros depend on me:

PatternT18 | ConstrWarnLightFlash9

### PatternT19 [References: 0] Defined? True

#define PatternT19(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,...) \
PATTERNT19_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#130

I depend on these macros:

PatternT19 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT19_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT2 [References: 0] Defined? True

#define PatternT2(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,...) PATTERNT2_T, \
_CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#113

I depend on these macros:

PatternT2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

These macros depend on me:

PatternT2 | Blink2
Blink3
Herz_2MoRelais
Herz_2MoRelais_I
Herz_BiRelais
Herz_BiRelais_I
Herz_BiRelais_I_V1_AB
Herz_BiRelais_I_V1_CD
Herz_BiRelais_I_V1_EF
Herz_BiRelais_V1_AB
Herz_BiRelais_V1_CD
Herz_BiRelais_V1_EF
Sound_ADKeyTime | Sound_DecVol
Sound_IncVol
Sound_New_DecVol
Sound_New_IncVol
Sound_JQ6500_ADKeyTime | Sound_JQ6500_BG_DecVol
Sound_JQ6500_BG_IncVol
Sound_JQ6500_DecVol
Sound_JQ6500_IncVol

### PatternT20 [References: 0] Defined? True

#define PatternT20(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,...) \
PATTERNT20_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#131

I depend on these macros:

PatternT20 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT20_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

These macros depend on me:

PatternT20 | ConstrWarnLightFlash10

### PatternT21 [References: 0] Defined? True

#define PatternT21(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,...) \
PATTERNT21_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#132

I depend on these macros:

PatternT21 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT21_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT22 [References: 0] Defined? True

#define PatternT22(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,...)
) PATTERNT22_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#133

I depend on these macros:

PatternT22 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT22_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

These macros depend on me:

PatternT22 | ConstrWarnLightFlash11

### PatternT23 [References: 0] Defined? True

#define PatternT23(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,...) ,...) PATTERNT23_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#134

I depend on these macros:

PatternT23 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT23_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT24 [References: 0] Defined? True

#define PatternT24(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,...) 4,...) PATTERNT24_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#135

I depend on these macros:

PatternT24 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT24_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

These macros depend on me:

PatternT24 | ConstrWarnLightFlash12

### PatternT25 [References: 0] Defined? True

#define PatternT25(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,...) 5,...) PATTERNT25_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_W2B(COUNT_VARARGS(__VA\
_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#136

I depend on these macros:

PatternT25 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT25_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT26 [References: 0] Defined? True

#define PatternT26(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,...) 6,...) PATTERNT26_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_W2B(COUNT_VA\
RARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#137

I depend on these macros:

PatternT26 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT26_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

These macros depend on me:

PatternT26 | ConstrWarnLightFlash13

### PatternT27 [References: 0] Defined? True

#define PatternT27(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,...) 7,...) PATTERNT27_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_W2\
B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#138

I depend on these macros:

PatternT27 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT27_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT28 [References: 0] Defined? True

#define PatternT28(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,...) 8,...) PATTERNT28_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#139

I depend on these macros:

PatternT28 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT28_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

These macros depend on me:

PatternT28 | ConstrWarnLightFlash14

### PatternT29 [References: 0] Defined? True

#define PatternT29(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,...) 9,...) PATTERNT29_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#140

I depend on these macros:

PatternT29 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT29_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT3 [References: 0] Defined? True

#define PatternT3(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,...) PATTERNT3_T, \
_CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#114

I depend on these macros:

PatternT3 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT3_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT30 [References: 0] Defined? True

#define PatternT30(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,...) 0,...) PATTERNT30_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#141

I depend on these macros:

PatternT30 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT30_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

These macros depend on me:

PatternT30 | ConstrWarnLightFlash15

### PatternT31 [References: 0] Defined? True

#define PatternT31(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,...) 1,...) PATTERNT31_T, _CHKL(LED)+RAM5, \
(NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__, \

`defined @` Macros.h#142

I depend on these macros:

PatternT31 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT31_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT32 [References: 0] Defined? True

#define PatternT32(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,...) 2,...) PATTERNT32_T, _CHKL(LED)+RAM5, \
(NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#143

I depend on these macros:

PatternT32 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT32_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT33 [References: 0] Defined? True

#define PatternT33(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,...) 3,...) PATTERNT33_T, _CHKL(LED)+RAM5, \
(NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#144

I depend on these macros:

PatternT33 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT33_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT34 [References: 0] Defined? True

#define PatternT34(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,...) 4,...) PATTERNT34_T, _CHKL(LED)+RAM5, \
(NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#145

I depend on these macros:

PatternT34 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT34_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT35 [References: 0] Defined? True

#define PatternT35(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,...) 5,...) PATTERNT35_T, _CHKL(LED)+RAM5, \
(NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#146

I depend on these macros:

PatternT35 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT35_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT36 [References: 0] Defined? True

#define PatternT36(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,...) 6,...) PATTERNT36_T, _CHKL(LED)+RAM5, \
(NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#147

I depend on these macros:

PatternT36 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT36_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT37 [References: 0] Defined? True

#define PatternT37(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,...) 7,...) PATTERNT37_T, \
_CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#148

I depend on these macros:

PatternT37 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT37_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT38 [References: 0] Defined? True

#define PatternT38(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,...) 8,...) PATTERNT38_T, \
_CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_W2B(COUNT_VARARGS(__VA_A\
RGS__)), __VA_ARGS__,

`defined @` Macros.h#149

I depend on these macros:

PatternT38 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT38_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT39 [References: 0] Defined? True

#define PatternT39(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,...) 9,...) PATTERNT39_T, \
_CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_W2B(COUNT_VARA\
RGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#150

I depend on these macros:

PatternT39 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT39_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT4 [References: 0] Defined? True

#define PatternT4(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,...) PATTERNT4_T, \
_CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__, \

`defined @` Macros.h#115

I depend on these macros:

PatternT4 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT4_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

These macros depend on me:

PatternT4 | AmpelX
BlueLight1
BlueLight2
ConstrWarnLight3
Leuchtfeuer
LeuchtfeuerALL
RGB_AmpelX

### PatternT40 [References: 0] Defined? True

#define PatternT40(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,...) 0,...) PATTERNT40_T, \
_CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_W2B(\
COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#151

I depend on these macros:

PatternT40 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT40_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT41 [References: 0] Defined? True

#define PatternT41(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,...) 1,...) \
PATTERNT41_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#152

I depend on these macros:

PatternT41 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT41_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT42 [References: 0] Defined? True

#define PatternT42(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,...) 2,...) \
PATTERNT42_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#153

I depend on these macros:

PatternT42 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT42_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT43 [References: 0] Defined? True

#define PatternT43(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,...) 3,...) \
PATTERNT43_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#154

I depend on these macros:

PatternT43 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT43_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT44 [References: 0] Defined? True

#define PatternT44(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,...) 4,...) \
PATTERNT44_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__, \

`defined @` Macros.h#155

I depend on these macros:

PatternT44 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT44_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT45 [References: 0] Defined? True

#define PatternT45(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,...) 5,...) \
PATTERNT45_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#156

I depend on these macros:

PatternT45 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT45_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT46 [References: 0] Defined? True

#define PatternT46(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,...) 6,...) \
PATTERNT46_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#157

I depend on these macros:

PatternT46 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT46_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT47 [References: 0] Defined? True

#define PatternT47(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,...) 7,...) \
PATTERNT47_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#158

I depend on these macros:

PatternT47 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT47_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT48 [References: 0] Defined? True

#define PatternT48(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,...) 8,...) \
PATTERNT48_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#159

I depend on these macros:

PatternT48 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT48_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT49 [References: 0] Defined? True

#define PatternT49(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,...) 9,...) \
PATTERNT49_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#160

I depend on these macros:

PatternT49 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT49_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT5 [References: 0] Defined? True

#define PatternT5(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,...) PATTERNT5_T, \
_CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#116

I depend on these macros:

PatternT5 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT5_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

These macros depend on me:

PatternT5 | ConstrWarnLight4

### PatternT50 [References: 0] Defined? True

#define PatternT50(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,...) 0,...) \
PATTERNT50_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#161

I depend on these macros:

PatternT50 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT50_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT51 [References: 0] Defined? True

#define PatternT51(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,...) 1,...) \
PATTERNT51_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_W2B(COUNT_VARARGS(__VA_ARG\
S__)), __VA_ARGS__,

`defined @` Macros.h#162

I depend on these macros:

PatternT51 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT51_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT52 [References: 0] Defined? True

#define PatternT52(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,...) 2,...) \
PATTERNT52_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_W2B(COUNT_VARARG\
S(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#163

I depend on these macros:

PatternT52 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT52_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT53 [References: 0] Defined? True

#define PatternT53(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,...) 3,...) \
PATTERNT53_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_W2B(CO\
UNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#164

I depend on these macros:

PatternT53 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT53_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT54 [References: 0] Defined? True

#define PatternT54(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,...) 4,...) \
PATTERNT54_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#165

I depend on these macros:

PatternT54 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT54_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT55 [References: 0] Defined? True

#define PatternT55(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,...) 5,...\
) PATTERNT55_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#166

I depend on these macros:

PatternT55 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT55_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT56 [References: 0] Defined? True

#define PatternT56(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,...) 6\
,...) PATTERNT56_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#167

I depend on these macros:

PatternT56 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT56_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT57 [References: 0] Defined? True

#define PatternT57(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,...) ,T57,...) PATTERNT57_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#168

I depend on these macros:

PatternT57 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT57_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT58 [References: 0] Defined? True

#define PatternT58(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,...) T57,T58,...) PATTERNT58_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#169

I depend on these macros:

PatternT58 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT58_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT59 [References: 0] Defined? True

#define PatternT59(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,...) T58,T59,...) PATTERNT59_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_T2B(T59),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#170

I depend on these macros:

PatternT59 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT59_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT6 [References: 0] Defined? True

#define PatternT6(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,...) PATTERNT6_T, \
_CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#117

I depend on these macros:

PatternT6 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT6_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

These macros depend on me:

PatternT6 | ConstrWarnLight5
ConstrWarnLightFlash3

### PatternT60 [References: 0] Defined? True

#define PatternT60(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,...) T59,T60,...) PATTERNT60_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_T2B(T59),_T2B(T60),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#171

I depend on these macros:

PatternT60 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT60_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT61 [References: 0] Defined? True

#define PatternT61(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,...) T60,T61,...) PATTERNT61_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_T2B(T59),_T2B(T60),_T2B(T61),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#172

I depend on these macros:

PatternT61 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT61_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT62 [References: 0] Defined? True

#define PatternT62(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,...) T61,T62,...) PATTERNT62_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_T2B(T59),_T2B(T60),_T2B(T61),_T2B(T62),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#173

I depend on these macros:

PatternT62 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT62_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT63 [References: 0] Defined? True

#define PatternT63(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,T63,...) T62,T63,...) PATTERNT63_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_T2B(T59),_T2B(T60),_T2B(T61),_T2B(T62),_T2B(T63),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#174

I depend on these macros:

PatternT63 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT63_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT64 [References: 0] Defined? True

#define PatternT64(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,T63,T64,...) T63,T64,...) PATTERNT64_T, _CHKL(LED)+RAM5, \
(NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_T2B(T59),_T2B(T60),_T2B(T61),_T2B(T62),_T2B(T63),_T2B(T64),_W2B(COUNT_VARARGS(__VA_ARGS_\
_)), __VA_ARGS__,

`defined @` Macros.h#175

I depend on these macros:

PatternT64 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT64_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternT7 [References: 0] Defined? True

#define PatternT7(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,...) \
PATTERNT7_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#118

I depend on these macros:

PatternT7 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT7_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

These macros depend on me:

PatternT7 | ConstrWarnLight6

### PatternT8 [References: 0] Defined? True

#define PatternT8(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,...) \
PATTERNT8_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#119

I depend on these macros:

PatternT8 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT8_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

These macros depend on me:

PatternT8 | ConstrWarnLight7
ConstrWarnLightFlash4
Def_Neon_Misha

### PatternT9 [References: 0] Defined? True

#define PatternT9(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,...) \
PATTERNT9_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),SI_1, LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#120

I depend on these macros:

PatternT9 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT9_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

These macros depend on me:

PatternT9 | ConstrWarnLight8

### PatternTE1 [References: 0] Defined? True

#define PatternTE1(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,...) PATTERNT1_T, \
_CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#314

I depend on these macros:

PatternTE1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE10 [References: 0] Defined? True

#define PatternTE10(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,...) \
PATTERNT10_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#323

I depend on these macros:

PatternTE10 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT10_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE11 [References: 0] Defined? True

#define PatternTE11(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,...) \
PATTERNT11_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_W2B(COUNT_VARARGS(__VA_ARGS__)\
), __VA_ARGS__,

`defined @` Macros.h#324

I depend on these macros:

PatternTE11 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT11_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE12 [References: 0] Defined? True

#define PatternTE12(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,...) \
PATTERNT12_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_W2B(COUNT_VARARGS(__\
VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#325

I depend on these macros:

PatternTE12 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT12_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE13 [References: 0] Defined? True

#define PatternTE13(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,...) \
PATTERNT13_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_W2B(COUNT_\
VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#326

I depend on these macros:

PatternTE13 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT13_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE14 [References: 0] Defined? True

#define PatternTE14(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,...) \
PATTERNT14_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#327

I depend on these macros:

PatternTE14 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT14_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE15 [References: 0] Defined? True

#define PatternTE15(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,...) \
PATTERNT15_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#328

I depend on these macros:

PatternTE15 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT15_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE16 [References: 0] Defined? True

#define PatternTE16(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,...) \
PATTERNT16_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#329

I depend on these macros:

PatternTE16 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT16_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE17 [References: 0] Defined? True

#define PatternTE17(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,...) \
PATTERNT17_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#330

I depend on these macros:

PatternTE17 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT17_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE18 [References: 0] Defined? True

#define PatternTE18(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,...) \
PATTERNT18_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__, \

`defined @` Macros.h#331

I depend on these macros:

PatternTE18 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT18_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE19 [References: 0] Defined? True

#define PatternTE19(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,...) \
PATTERNT19_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#332

I depend on these macros:

PatternTE19 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT19_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE2 [References: 0] Defined? True

#define PatternTE2(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,...) PATTERNT2_T, \
_CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#315

I depend on these macros:

PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

These macros depend on me:

PatternTE2 | Sound_ADKey | Sound_Loop
Sound_New_Loop
Sound_New_Next
Sound_New_PausePlay
Sound_New_PlayMode
Sound_New_Prev
Sound_New_Seq1
Sound_New_Seq10
Sound_New_Seq11
Sound_New_Seq12
Sound_New_Seq13
Sound_New_Seq14
Sound_New_Seq2
Sound_New_Seq3
Sound_New_Seq4
Sound_New_Seq5
Sound_New_Seq6
Sound_New_Seq7
Sound_New_Seq8
Sound_New_Seq9
Sound_New_USDSPI
Sound_Next
Sound_PausePlay
Sound_PlayMode
Sound_Prev
Sound_Seq1
Sound_Seq10
Sound_Seq11
Sound_Seq12
Sound_Seq13
Sound_Seq14
Sound_Seq2
Sound_Seq3
Sound_Seq4
Sound_Seq5
Sound_Seq6
Sound_Seq7
Sound_Seq8
Sound_Seq9
Sound_USDSPI
Sound_JQ6500_ADKey | Sound_JQ6500_BG_Next
Sound_JQ6500_BG_Prev
Sound_JQ6500_BG_Seq1
Sound_JQ6500_BG_Seq2
Sound_JQ6500_BG_Seq3
Sound_JQ6500_BG_Seq4
Sound_JQ6500_BG_Seq5
Sound_JQ6500_Next
Sound_JQ6500_Prev
Sound_JQ6500_Seq1
Sound_JQ6500_Seq2
Sound_JQ6500_Seq3
Sound_JQ6500_Seq4
Sound_JQ6500_Seq5

### PatternTE20 [References: 0] Defined? True

#define PatternTE20(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,...)
) PATTERNT20_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#333

I depend on these macros:

PatternTE20 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT20_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE21 [References: 0] Defined? True

#define PatternTE21(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,...) ,...) PATTERNT21_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#334

I depend on these macros:

PatternTE21 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT21_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE22 [References: 0] Defined? True

#define PatternTE22(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,...) 2,...) PATTERNT22_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#335

I depend on these macros:

PatternTE22 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT22_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE23 [References: 0] Defined? True

#define PatternTE23(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,...) 3,...) PATTERNT23_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#336

I depend on these macros:

PatternTE23 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT23_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE24 [References: 0] Defined? True

#define PatternTE24(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,...) 4,...) PATTERNT24_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#337

I depend on these macros:

PatternTE24 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT24_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE25 [References: 0] Defined? True

#define PatternTE25(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,...) 5,...) PATTERNT25_T, _CHKL(LED)+RAM5, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_W2B(COUNT_VARARGS(__VA\
_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#338

I depend on these macros:

PatternTE25 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT25_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE26 [References: 0] Defined? True

#define PatternTE26(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,...) 6,...) PATTERNT26_T, _CHKL(LED)+RAM5, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_W2B(COUNT_VA\
RARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#339

I depend on these macros:

PatternTE26 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT26_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE27 [References: 0] Defined? True

#define PatternTE27(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,...) 7,...) PATTERNT27_T, _CHKL(LED)+RAM5, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_W2\
B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#340

I depend on these macros:

PatternTE27 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT27_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE28 [References: 0] Defined? True

#define PatternTE28(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,...) 8,...) PATTERNT28_T, _CHKL(LED)+RAM5, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#341

I depend on these macros:

PatternTE28 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT28_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE29 [References: 0] Defined? True

#define PatternTE29(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,...) 9,...) PATTERNT29_T, _CHKL(LED)+RAM5, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#342

I depend on these macros:

PatternTE29 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT29_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE3 [References: 0] Defined? True

#define PatternTE3(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,...) PATTERNT3_T, \
_CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#316

I depend on these macros:

PatternTE3 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT3_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE30 [References: 0] Defined? True

#define PatternTE30(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,...) 0,...) PATTERNT30_T, _CHKL(LED)+RAM5, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#343

I depend on these macros:

PatternTE30 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT30_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE31 [References: 0] Defined? True

#define PatternTE31(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,...) 1,...) PATTERNT31_T, _CHKL(LED)+RAM5, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__, \

`defined @` Macros.h#344

I depend on these macros:

PatternTE31 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT31_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE32 [References: 0] Defined? True

#define PatternTE32(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,...) 2,...) PATTERNT32_T, _CHKL(LED)+RAM5, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#345

I depend on these macros:

PatternTE32 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT32_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE33 [References: 0] Defined? True

#define PatternTE33(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,...) 3,...) PATTERNT33_T, _CHKL(LED)+RAM5, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#346

I depend on these macros:

PatternTE33 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT33_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE34 [References: 0] Defined? True

#define PatternTE34(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,...) 4,...) PATTERNT34_T, _CHKL(LED)+RAM5, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#347

I depend on these macros:

PatternTE34 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT34_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE35 [References: 0] Defined? True

#define PatternTE35(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,...) 5,...) PATTERNT35_T, \
_CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#348

I depend on these macros:

PatternTE35 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT35_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE36 [References: 0] Defined? True

#define PatternTE36(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,...) 6,...) PATTERNT36_T, \
_CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#349

I depend on these macros:

PatternTE36 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT36_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE37 [References: 0] Defined? True

#define PatternTE37(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,...) 7,...) PATTERNT37_T, \
_CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#350

I depend on these macros:

PatternTE37 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT37_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE38 [References: 0] Defined? True

#define PatternTE38(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,...) 8,...) PATTERNT38_T, \
_CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_W2B(COUNT_VARARGS(__VA_A\
RGS__)), __VA_ARGS__,

`defined @` Macros.h#351

I depend on these macros:

PatternTE38 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT38_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE39 [References: 0] Defined? True

#define PatternTE39(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,...) 9,...) \
PATTERNT39_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_W2B(COUNT_VARA\
RGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#352

I depend on these macros:

PatternTE39 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT39_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE4 [References: 0] Defined? True

#define PatternTE4(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,...) PATTERNT4_T, \
_CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__, \

`defined @` Macros.h#317

I depend on these macros:

PatternTE4 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT4_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE40 [References: 0] Defined? True

#define PatternTE40(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,...) 0,...) \
PATTERNT40_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_W2B(\
COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#353

I depend on these macros:

PatternTE40 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT40_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE41 [References: 0] Defined? True

#define PatternTE41(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,...) 1,...) \
PATTERNT41_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#354

I depend on these macros:

PatternTE41 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT41_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE42 [References: 0] Defined? True

#define PatternTE42(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,...) 2,...) \
PATTERNT42_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#355

I depend on these macros:

PatternTE42 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT42_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE43 [References: 0] Defined? True

#define PatternTE43(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,...) 3,...) \
PATTERNT43_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#356

I depend on these macros:

PatternTE43 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT43_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE44 [References: 0] Defined? True

#define PatternTE44(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,...) 4,...) \
PATTERNT44_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__, \

`defined @` Macros.h#357

I depend on these macros:

PatternTE44 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT44_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE45 [References: 0] Defined? True

#define PatternTE45(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,...) 5,...) \
PATTERNT45_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#358

I depend on these macros:

PatternTE45 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT45_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE46 [References: 0] Defined? True

#define PatternTE46(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,...) 6,...) \
PATTERNT46_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#359

I depend on these macros:

PatternTE46 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT46_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE47 [References: 0] Defined? True

#define PatternTE47(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,...) 7,...) \
PATTERNT47_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#360

I depend on these macros:

PatternTE47 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT47_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE48 [References: 0] Defined? True

#define PatternTE48(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,...) 8,...) \
PATTERNT48_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#361

I depend on these macros:

PatternTE48 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT48_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE49 [References: 0] Defined? True

#define PatternTE49(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,...) 9,...) \
PATTERNT49_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#362

I depend on these macros:

PatternTE49 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT49_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE5 [References: 0] Defined? True

#define PatternTE5(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,...) \
PATTERNT5_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#318

I depend on these macros:

PatternTE5 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT5_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE50 [References: 0] Defined? True

#define PatternTE50(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,...) 0,...) \
PATTERNT50_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#363

I depend on these macros:

PatternTE50 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT50_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE51 [References: 0] Defined? True

#define PatternTE51(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,...) 1,...) \
PATTERNT51_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_W2B(COUNT_VARARGS(__VA_ARG\
S__)), __VA_ARGS__,

`defined @` Macros.h#364

I depend on these macros:

PatternTE51 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT51_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE52 [References: 0] Defined? True

#define PatternTE52(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,...) 2,...) \
PATTERNT52_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_W2B(COUNT_VARARG\
S(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#365

I depend on these macros:

PatternTE52 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT52_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE53 [References: 0] Defined? True

#define PatternTE53(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,...) 3,...\
) PATTERNT53_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_W2B(CO\
UNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#366

I depend on these macros:

PatternTE53 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT53_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE54 [References: 0] Defined? True

#define PatternTE54(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,...) 4\
,...) PATTERNT54_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#367

I depend on these macros:

PatternTE54 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT54_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE55 [References: 0] Defined? True

#define PatternTE55(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,...) ,T55,...) PATTERNT55_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#368

I depend on these macros:

PatternTE55 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT55_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE56 [References: 0] Defined? True

#define PatternTE56(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,...) T55,T56,...) PATTERNT56_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#369

I depend on these macros:

PatternTE56 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT56_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE57 [References: 0] Defined? True

#define PatternTE57(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,...) T56,T57,...) PATTERNT57_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#370

I depend on these macros:

PatternTE57 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT57_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE58 [References: 0] Defined? True

#define PatternTE58(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,...) T57,T58,...) PATTERNT58_T, _CHKL(LED)+RAM5, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#371

I depend on these macros:

PatternTE58 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT58_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE59 [References: 0] Defined? True

#define PatternTE59(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,...) T58,T59,...) PATTERNT59_T, _CHKL(LED)+RAM5, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_T2B(T59),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#372

I depend on these macros:

PatternTE59 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT59_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE6 [References: 0] Defined? True

#define PatternTE6(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,...) \
PATTERNT6_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#319

I depend on these macros:

PatternTE6 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT6_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE60 [References: 0] Defined? True

#define PatternTE60(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,...) T59,T60,...) PATTERNT60_T, _CHKL(LED)+RAM5, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_T2B(T59),_T2B(T60),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#373

I depend on these macros:

PatternTE60 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT60_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE61 [References: 0] Defined? True

#define PatternTE61(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,...) T60,T61,...) PATTERNT61_T, _CHKL(LED)+RAM5, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_T2B(T59),_T2B(T60),_T2B(T61),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#374

I depend on these macros:

PatternTE61 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT61_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE62 [References: 0] Defined? True

#define PatternTE62(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,...) T61,T62,...) PATTERNT62_T, _CHKL(LED)+RAM5, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_T2B(T59),_T2B(T60),_T2B(T61),_T2B(T62),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#375

I depend on these macros:

PatternTE62 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT62_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE63 [References: 0] Defined? True

#define PatternTE63(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,T63,...) T62,T63,...) PATTERNT63_T, _CHKL(LED)+RAM5, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_T2B(T59),_T2B(T60),_T2B(T61),_T2B(T62),_T2B(T63),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#376

I depend on these macros:

PatternTE63 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT63_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE64 [References: 0] Defined? True

#define PatternTE64(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,T63,T64,...) T63,T64,...) PATTERNT64_T, _CHKL(LED)+RAM5, \
(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_\
T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2\
B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(\
T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T5\
4),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_T2B(T59),_T2B(T60),_T2B(T61),_T2B(T62),_T2B(T63),_T2B(T64),_W2B(COUNT_VARARGS(__VA_ARGS_\
_)), __VA_ARGS__,

`defined @` Macros.h#377

I depend on these macros:

PatternTE64 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT64_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE7 [References: 0] Defined? True

#define PatternTE7(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,...) \
PATTERNT7_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#320

I depend on these macros:

PatternTE7 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT7_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE8 [References: 0] Defined? True

#define PatternTE8(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,...) \
PATTERNT8_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#321

I depend on these macros:

PatternTE8 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT8_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PatternTE9 [References: 0] Defined? True

#define PatternTE9(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,...) \
PATTERNT9_T, _CHKL(LED)+RAM5, (NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode, \
_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#322

I depend on these macros:

PatternTE9 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT9_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### PushButton2I_0_1 [References: 0] Defined? True

#define PushButton2I_0_1(InCh,InCh2,LocInCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout) \
Logic(LocInCh, InCh+1 OR InCh2==SI_0?InCh+1:InCh2) \
Counter((Rotate?CF_ROTATE:0)|(Use0?0:CF_SKIP0)|(ResetLong?CF_RESET_LONG:0)|OptCtrPar|CF_INV_ENABLE, \
LocInCh, InCh, Timeout, TmpNr+0, TmpNr+1) InCh_to_TmpVar(TmpNr, 1+1)

`defined @` MobaLedLib.h#456

I depend on these macros:

PushButton2I_0_1 | CF_INV_ENABLE
CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
Logic | COUNT_VARARGS | _GET_NTH_ARG
LOGIC_T
OR | _OR_NR | SI_0
SI_0

These macros depend on me:

PushButton2I_0_1 | PushButton2I_RGB_0_1
PushButton2I_w_LED_BL_0_1

### PushButton2I_0_2 [References: 0] Defined? True

#define PushButton2I_0_2(InCh,InCh2,LocInCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout) \
Logic(LocInCh, InCh+1 OR InCh2==SI_0?InCh+1:InCh2) \
Counter((Rotate?CF_ROTATE:0)|(Use0?0:CF_SKIP0)|(ResetLong?CF_RESET_LONG:0)|OptCtrPar|CF_INV_ENABLE, \
LocInCh, InCh, Timeout, TmpNr+0, TmpNr+1, TmpNr+2) InCh_to_TmpVar(TmpNr, 2+1)

`defined @` MobaLedLib.h#461

I depend on these macros:

PushButton2I_0_2 | CF_INV_ENABLE
CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
Logic | COUNT_VARARGS | _GET_NTH_ARG
LOGIC_T
OR | _OR_NR | SI_0
SI_0

These macros depend on me:

PushButton2I_0_2 | PushButton2I_RGB_0_2
PushButton2I_w_LED_BL_0_2

### PushButton2I_0_3 [References: 0] Defined? True

#define PushButton2I_0_3(InCh,InCh2,LocInCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout) \
Logic(LocInCh, InCh+1 OR InCh2==SI_0?InCh+1:InCh2) \
Counter((Rotate?CF_ROTATE:0)|(Use0?0:CF_SKIP0)|(ResetLong?CF_RESET_LONG:0)|OptCtrPar|CF_INV_ENABLE, \
LocInCh, InCh, Timeout, TmpNr+0, TmpNr+1, TmpNr+2, TmpNr+3) InCh_to_TmpVar(TmpNr, \
3+1)

`defined @` MobaLedLib.h#466

I depend on these macros:

PushButton2I_0_3 | CF_INV_ENABLE
CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
Logic | COUNT_VARARGS | _GET_NTH_ARG
LOGIC_T
OR | _OR_NR | SI_0
SI_0

These macros depend on me:

PushButton2I_0_3 | PushButton2I_RGB_0_3
PushButton2I_w_LED_BL_0_3

### PushButton2I_0_4 [References: 0] Defined? True

#define PushButton2I_0_4(InCh,InCh2,LocInCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout) \
Logic(LocInCh, InCh+1 OR InCh2==SI_0?InCh+1:InCh2) \
Counter((Rotate?CF_ROTATE:0)|(Use0?0:CF_SKIP0)|(ResetLong?CF_RESET_LONG:0)|OptCtrPar|CF_INV_ENABLE, \
LocInCh, InCh, Timeout, TmpNr+0, TmpNr+1, TmpNr+2, TmpNr+3, TmpNr+4) InCh_to_TmpVar(TmpNr, \
4+1)

`defined @` MobaLedLib.h#471

I depend on these macros:

PushButton2I_0_4 | CF_INV_ENABLE
CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
Logic | COUNT_VARARGS | _GET_NTH_ARG
LOGIC_T
OR | _OR_NR | SI_0
SI_0

These macros depend on me:

PushButton2I_0_4 | PushButton2I_RGB_0_4
PushButton2I_w_LED_BL_0_4

### PushButton2I_0_5 [References: 0] Defined? True

#define PushButton2I_0_5(InCh,InCh2,LocInCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout) \
Logic(LocInCh, InCh+1 OR InCh2==SI_0?InCh+1:InCh2) \
Counter((Rotate?CF_ROTATE:0)|(Use0?0:CF_SKIP0)|(ResetLong?CF_RESET_LONG:0)|OptCtrPar|CF_INV_ENABLE, \
LocInCh, InCh, Timeout, TmpNr+0, TmpNr+1, TmpNr+2, TmpNr+3, TmpNr+4, TmpNr+5) \
InCh_to_TmpVar(TmpNr, 5+1)

`defined @` MobaLedLib.h#476

I depend on these macros:

PushButton2I_0_5 | CF_INV_ENABLE
CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
Logic | COUNT_VARARGS | _GET_NTH_ARG
LOGIC_T
OR | _OR_NR | SI_0
SI_0

These macros depend on me:

PushButton2I_0_5 | PushButton2I_RGB_0_5
PushButton2I_w_LED_BL_0_5

### PushButton2I_RGB_0_1 [References: 0] Defined? True

#define PushButton2I_RGB_0_1(B_LED,InCh,InCh2,LocInCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,R0,G0,B0,R10,G10,B10,R11,G11,B11) \
PushButton2I_0_1(InCh, InCh2, LocInCh, TmpNr, Rotate, Use0, ResetLong, OptCtrPar, \
Timeout) Status_Button_RGB_0_1(B_LED, R0,G0,B0,R10,G10,B10,R11,G11,B11)

`defined @` MobaLedLib.h#567

I depend on these macros:

PushButton2I_RGB_0_1 | PushButton2I_0_1 | CF_INV_ENABLE
CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
Logic | COUNT_VARARGS | _GET_NTH_ARG
LOGIC_T
OR | _OR_NR | SI_0
SI_0
Status_Button_RGB_0_1 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec

### PushButton2I_RGB_0_2 [References: 0] Defined? True

#define PushButton2I_RGB_0_2(B_LED,InCh,InCh2,LocInCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21) 1,B21) PushButton2I_0_2(InCh, InCh2, LocInCh, TmpNr, Rotate, Use0, \
ResetLong, OptCtrPar, Timeout) Status_Button_RGB_0_2(B_LED, \
R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21)

`defined @` MobaLedLib.h#571

I depend on these macros:

PushButton2I_RGB_0_2 | PushButton2I_0_2 | CF_INV_ENABLE
CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
Logic | COUNT_VARARGS | _GET_NTH_ARG
LOGIC_T
OR | _OR_NR | SI_0
SI_0
Status_Button_RGB_0_2 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec

### PushButton2I_RGB_0_3 [References: 0] Defined? True

#define PushButton2I_RGB_0_3(B_LED,InCh,InCh2,LocInCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21,R30,G30,B30,R31,G31,B31) 1,B31) PushButton2I_0_3(InCh, InCh2, LocInCh, \
TmpNr, Rotate, Use0, ResetLong, OptCtrPar, Timeout) Status_Button_RGB_0_3(B_LED, \
R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21,R30,G30,B30,R31,G31,B31) \

`defined @` MobaLedLib.h#575

I depend on these macros:

PushButton2I_RGB_0_3 | PushButton2I_0_3 | CF_INV_ENABLE
CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
Logic | COUNT_VARARGS | _GET_NTH_ARG
LOGIC_T
OR | _OR_NR | SI_0
SI_0
Status_Button_RGB_0_3 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec

### PushButton2I_RGB_0_4 [References: 0] Defined? True

#define PushButton2I_RGB_0_4(B_LED,InCh,InCh2,LocInCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21,R30,G30,B30,R31,G31,B31,R40,G40,B40,R41,G41,B41) 1,B41) PushButton2I_0_4(InCh, \
InCh2, LocInCh, TmpNr, Rotate, Use0, ResetLong, OptCtrPar, Timeout) \
Status_Button_RGB_0_4(B_LED, \
R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21,R30,G30,B30,R31,G31,B31,R40,G40,B40,R41,G41,B41) \

`defined @` MobaLedLib.h#579

I depend on these macros:

PushButton2I_RGB_0_4 | PushButton2I_0_4 | CF_INV_ENABLE
CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
Logic | COUNT_VARARGS | _GET_NTH_ARG
LOGIC_T
OR | _OR_NR | SI_0
SI_0
Status_Button_RGB_0_4 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec

### PushButton2I_RGB_0_5 [References: 0] Defined? True

#define PushButton2I_RGB_0_5(B_LED,InCh,InCh2,LocInCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21,R30,G30,B30,R31,G31,B31,R40,G40,B40,R41,G41,B41,R50,G50,B50,R51,G51,B51) 1,B51) \
PushButton2I_0_5(InCh, InCh2, LocInCh, TmpNr, Rotate, Use0, ResetLong, OptCtrPar, \
Timeout) Status_Button_RGB_0_5(B_LED, \
R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21,R30,G30,B30,R31,G31,B31,R40,G40,B40,R41,G41,B41,R50,G50,B50,R51,G51,B51) \

`defined @` MobaLedLib.h#583

I depend on these macros:

PushButton2I_RGB_0_5 | PushButton2I_0_5 | CF_INV_ENABLE
CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
Logic | COUNT_VARARGS | _GET_NTH_ARG
LOGIC_T
OR | _OR_NR | SI_0
SI_0
Status_Button_RGB_0_5 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec

### PushButton2I_w_LED_BL_0_1 [References: 0] Defined? True

#define PushButton2I_w_LED_BL_0_1(B_LED,B_LED_Cx,InCh,InCh2,LocInCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,Val1,BackLight) \
PushButton2I_0_1(InCh, InCh2, LocInCh, TmpNr, Rotate, Use0, ResetLong, OptCtrPar, \
Timeout) Status_ButtonBL_0_1(B_LED, B_LED_Cx, Val1, BackLight)

`defined @` MobaLedLib.h#546

I depend on these macros:

PushButton2I_w_LED_BL_0_1 | PushButton2I_0_1 | CF_INV_ENABLE
CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
Logic | COUNT_VARARGS | _GET_NTH_ARG
LOGIC_T
OR | _OR_NR | SI_0
SI_0
Status_ButtonBL_0_1 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec
_Cx2StCh

### PushButton2I_w_LED_BL_0_2 [References: 0] Defined? True

#define PushButton2I_w_LED_BL_0_2(B_LED,B_LED_Cx,InCh,InCh2,LocInCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,Val1,BackLight) \
PushButton2I_0_2(InCh, InCh2, LocInCh, TmpNr, Rotate, Use0, ResetLong, OptCtrPar, \
Timeout) Status_ButtonBL_0_2(B_LED, B_LED_Cx, Val1, BackLight)

`defined @` MobaLedLib.h#550

I depend on these macros:

PushButton2I_w_LED_BL_0_2 | PushButton2I_0_2 | CF_INV_ENABLE
CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
Logic | COUNT_VARARGS | _GET_NTH_ARG
LOGIC_T
OR | _OR_NR | SI_0
SI_0
Status_ButtonBL_0_2 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec
_Cx2StCh

### PushButton2I_w_LED_BL_0_3 [References: 0] Defined? True

#define PushButton2I_w_LED_BL_0_3(B_LED,B_LED_Cx,InCh,InCh2,LocInCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,Val1,BackLight) \
PushButton2I_0_3(InCh, InCh2, LocInCh, TmpNr, Rotate, Use0, ResetLong, OptCtrPar, \
Timeout) Status_ButtonBL_0_3(B_LED, B_LED_Cx, Val1, BackLight)

`defined @` MobaLedLib.h#554

I depend on these macros:

PushButton2I_w_LED_BL_0_3 | PushButton2I_0_3 | CF_INV_ENABLE
CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
Logic | COUNT_VARARGS | _GET_NTH_ARG
LOGIC_T
OR | _OR_NR | SI_0
SI_0
Status_ButtonBL_0_3 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec
_Cx2StCh

### PushButton2I_w_LED_BL_0_4 [References: 0] Defined? True

#define PushButton2I_w_LED_BL_0_4(B_LED,B_LED_Cx,InCh,InCh2,LocInCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,Val1,BackLight) \
PushButton2I_0_4(InCh, InCh2, LocInCh, TmpNr, Rotate, Use0, ResetLong, OptCtrPar, \
Timeout) Status_ButtonBL_0_4(B_LED, B_LED_Cx, Val1, BackLight)

`defined @` MobaLedLib.h#558

I depend on these macros:

PushButton2I_w_LED_BL_0_4 | PushButton2I_0_4 | CF_INV_ENABLE
CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
Logic | COUNT_VARARGS | _GET_NTH_ARG
LOGIC_T
OR | _OR_NR | SI_0
SI_0
Status_ButtonBL_0_4 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec
_Cx2StCh

### PushButton2I_w_LED_BL_0_5 [References: 0] Defined? True

#define PushButton2I_w_LED_BL_0_5(B_LED,B_LED_Cx,InCh,InCh2,LocInCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,Val1,BackLight) \
PushButton2I_0_5(InCh, InCh2, LocInCh, TmpNr, Rotate, Use0, ResetLong, OptCtrPar, \
Timeout) Status_ButtonBL_0_5(B_LED, B_LED_Cx, Val1, BackLight)

`defined @` MobaLedLib.h#562

I depend on these macros:

PushButton2I_w_LED_BL_0_5 | PushButton2I_0_5 | CF_INV_ENABLE
CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
Logic | COUNT_VARARGS | _GET_NTH_ARG
LOGIC_T
OR | _OR_NR | SI_0
SI_0
Status_ButtonBL_0_5 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec
_Cx2StCh

### PushButton_0_1 [References: 0] Defined? True

#define PushButton_0_1(InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout) \
Counter((Rotate?CF_ROTATE:0)|(Use0?0:CF_SKIP0)|(ResetLong?CF_RESET_LONG:0)|OptCtrPar, \
InCh, SI_1, Timeout, TmpNr+0, TmpNr+1) InCh_to_TmpVar(TmpNr, 1+1)

`defined @` MobaLedLib.h#435

I depend on these macros:

PushButton_0_1 | CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_1

These macros depend on me:

PushButton_0_1 | PushButton_RGB_0_1
PushButton_w_LED_0_1
PushButton_w_LED_BL_0_1

### PushButton_0_2 [References: 0] Defined? True

#define PushButton_0_2(InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout) \
Counter((Rotate?CF_ROTATE:0)|(Use0?0:CF_SKIP0)|(ResetLong?CF_RESET_LONG:0)|OptCtrPar, \
InCh, SI_1, Timeout, TmpNr+0, TmpNr+1, TmpNr+2) InCh_to_TmpVar(TmpNr, 2+1)

`defined @` MobaLedLib.h#439

I depend on these macros:

PushButton_0_2 | CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_1

These macros depend on me:

PushButton_0_2 | PushButton_RGB_0_2
PushButton_w_LED_0_2
PushButton_w_LED_BL_0_2

### PushButton_0_3 [References: 0] Defined? True

#define PushButton_0_3(InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout) \
Counter((Rotate?CF_ROTATE:0)|(Use0?0:CF_SKIP0)|(ResetLong?CF_RESET_LONG:0)|OptCtrPar, \
InCh, SI_1, Timeout, TmpNr+0, TmpNr+1, TmpNr+2, TmpNr+3) InCh_to_TmpVar(TmpNr, \
3+1)

`defined @` MobaLedLib.h#443

I depend on these macros:

PushButton_0_3 | CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_1

These macros depend on me:

PushButton_0_3 | PushButton_RGB_0_3
PushButton_w_LED_0_3
PushButton_w_LED_BL_0_3

### PushButton_0_4 [References: 0] Defined? True

#define PushButton_0_4(InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout) \
Counter((Rotate?CF_ROTATE:0)|(Use0?0:CF_SKIP0)|(ResetLong?CF_RESET_LONG:0)|OptCtrPar, \
InCh, SI_1, Timeout, TmpNr+0, TmpNr+1, TmpNr+2, TmpNr+3, TmpNr+4) InCh_to_TmpVar(TmpNr, \
4+1)

`defined @` MobaLedLib.h#447

I depend on these macros:

PushButton_0_4 | CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_1

These macros depend on me:

PushButton_0_4 | PushButton_RGB_0_4
PushButton_w_LED_0_4
PushButton_w_LED_BL_0_4

### PushButton_0_5 [References: 0] Defined? True

#define PushButton_0_5(InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout) \
Counter((Rotate?CF_ROTATE:0)|(Use0?0:CF_SKIP0)|(ResetLong?CF_RESET_LONG:0)|OptCtrPar, \
InCh, SI_1, Timeout, TmpNr+0, TmpNr+1, TmpNr+2, TmpNr+3, TmpNr+4, TmpNr+5) \
InCh_to_TmpVar(TmpNr, 5+1)

`defined @` MobaLedLib.h#451

I depend on these macros:

PushButton_0_5 | CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_1

These macros depend on me:

PushButton_0_5 | PushButton_RGB_0_5
PushButton_w_LED_0_5
PushButton_w_LED_BL_0_5

### PushButton_RGB_0_1 [References: 0] Defined? True

#define PushButton_RGB_0_1(B_LED,InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,R0,G0,B0,R10,G10,B10,R11,G11,B11) \
PushButton_0_1(InCh, TmpNr, Rotate, Use0, ResetLong, OptCtrPar, Timeout) \
Status_Button_RGB_0_1(B_LED, R0,G0,B0,R10,G10,B10,R11,G11,B11)

`defined @` MobaLedLib.h#525

I depend on these macros:

PushButton_RGB_0_1 | PushButton_0_1 | CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_1
Status_Button_RGB_0_1 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec

### PushButton_RGB_0_2 [References: 0] Defined? True

#define PushButton_RGB_0_2(B_LED,InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21)
) PushButton_0_2(InCh, TmpNr, Rotate, Use0, ResetLong, OptCtrPar, Timeout) \
Status_Button_RGB_0_2(B_LED, R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21) \

`defined @` MobaLedLib.h#529

I depend on these macros:

PushButton_RGB_0_2 | PushButton_0_2 | CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_1
Status_Button_RGB_0_2 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec

### PushButton_RGB_0_3 [References: 0] Defined? True

#define PushButton_RGB_0_3(B_LED,InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21,R30,G30,B30,R31,G31,B31) 1,B31) PushButton_0_3(InCh, TmpNr, Rotate, Use0, ResetLong, \
OptCtrPar, Timeout) Status_Button_RGB_0_3(B_LED, \
R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21,R30,G30,B30,R31,G31,B31) \

`defined @` MobaLedLib.h#533

I depend on these macros:

PushButton_RGB_0_3 | PushButton_0_3 | CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_1
Status_Button_RGB_0_3 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec

### PushButton_RGB_0_4 [References: 0] Defined? True

#define PushButton_RGB_0_4(B_LED,InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21,R30,G30,B30,R31,G31,B31,R40,G40,B40,R41,G41,B41) 1,B41) PushButton_0_4(InCh, TmpNr, \
Rotate, Use0, ResetLong, OptCtrPar, Timeout) Status_Button_RGB_0_4(B_LED, \
R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21,R30,G30,B30,R31,G31,B31,R40,G40,B40,R41,G41,B41) \

`defined @` MobaLedLib.h#537

I depend on these macros:

PushButton_RGB_0_4 | PushButton_0_4 | CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_1
Status_Button_RGB_0_4 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec

### PushButton_RGB_0_5 [References: 0] Defined? True

#define PushButton_RGB_0_5(B_LED,InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21,R30,G30,B30,R31,G31,B31,R40,G40,B40,R41,G41,B41,R50,G50,B50,R51,G51,B51) 1,B51) \
PushButton_0_5(InCh, TmpNr, Rotate, Use0, ResetLong, OptCtrPar, Timeout) \
Status_Button_RGB_0_5(B_LED, \
R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21,R30,G30,B30,R31,G31,B31,R40,G40,B40,R41,G41,B41,R50,G50,B50,R51,G51,B51) \

`defined @` MobaLedLib.h#541

I depend on these macros:

PushButton_RGB_0_5 | PushButton_0_5 | CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_1
Status_Button_RGB_0_5 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec

### PushButton_w_LED_0_1 [References: 0] Defined? True

#define PushButton_w_LED_0_1(B_LED,B_LED_Cx,InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout) \
PushButton_0_1(InCh, TmpNr, Rotate, Use0, ResetLong, OptCtrPar, Timeout) \
Status_Button_0_1(B_LED, B_LED_Cx, 255)

`defined @` MobaLedLib.h#483

I depend on these macros:

PushButton_w_LED_0_1 | PushButton_0_1 | CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_1
Status_Button_0_1 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec
_Cx2StCh

### PushButton_w_LED_0_2 [References: 0] Defined? True

#define PushButton_w_LED_0_2(B_LED,B_LED_Cx,InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout) \
PushButton_0_2(InCh, TmpNr, Rotate, Use0, ResetLong, OptCtrPar, Timeout) \
Status_Button_0_2(B_LED, B_LED_Cx, 255)

`defined @` MobaLedLib.h#487

I depend on these macros:

PushButton_w_LED_0_2 | PushButton_0_2 | CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_1
Status_Button_0_2 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec
_Cx2StCh

### PushButton_w_LED_0_3 [References: 0] Defined? True

#define PushButton_w_LED_0_3(B_LED,B_LED_Cx,InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout) \
PushButton_0_3(InCh, TmpNr, Rotate, Use0, ResetLong, OptCtrPar, Timeout) \
Status_Button_0_3(B_LED, B_LED_Cx,255)

`defined @` MobaLedLib.h#491

I depend on these macros:

PushButton_w_LED_0_3 | PushButton_0_3 | CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_1
Status_Button_0_3 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec
_Cx2StCh

### PushButton_w_LED_0_4 [References: 0] Defined? True

#define PushButton_w_LED_0_4(B_LED,B_LED_Cx,InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout) \
PushButton_0_4(InCh, TmpNr, Rotate, Use0, ResetLong, OptCtrPar, Timeout) \
Status_Button_0_4(B_LED, B_LED_Cx,255)

`defined @` MobaLedLib.h#495

I depend on these macros:

PushButton_w_LED_0_4 | PushButton_0_4 | CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_1
Status_Button_0_4 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec
_Cx2StCh

### PushButton_w_LED_0_5 [References: 0] Defined? True

#define PushButton_w_LED_0_5(B_LED,B_LED_Cx,InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout) \
PushButton_0_5(InCh, TmpNr, Rotate, Use0, ResetLong, OptCtrPar, Timeout) \
Status_Button_0_5(B_LED, B_LED_Cx,255)

`defined @` MobaLedLib.h#499

I depend on these macros:

PushButton_w_LED_0_5 | PushButton_0_5 | CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_1
Status_Button_0_5 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec
_Cx2StCh

### PushButton_w_LED_BL_0_1 [References: 0] Defined? True

#define PushButton_w_LED_BL_0_1(B_LED,B_LED_Cx,InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,Val1,BackLight) \
PushButton_0_1(InCh, TmpNr, Rotate, Use0, ResetLong, OptCtrPar, Timeout) \
Status_ButtonBL_0_1(B_LED, B_LED_Cx, Val1, BackLight)

`defined @` MobaLedLib.h#504

I depend on these macros:

PushButton_w_LED_BL_0_1 | PushButton_0_1 | CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_1
Status_ButtonBL_0_1 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec
_Cx2StCh

### PushButton_w_LED_BL_0_2 [References: 0] Defined? True

#define PushButton_w_LED_BL_0_2(B_LED,B_LED_Cx,InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,Val1,BackLight) \
PushButton_0_2(InCh, TmpNr, Rotate, Use0, ResetLong, OptCtrPar, Timeout) \
Status_ButtonBL_0_2(B_LED, B_LED_Cx, Val1, BackLight)

`defined @` MobaLedLib.h#508

I depend on these macros:

PushButton_w_LED_BL_0_2 | PushButton_0_2 | CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_1
Status_ButtonBL_0_2 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec
_Cx2StCh

### PushButton_w_LED_BL_0_3 [References: 0] Defined? True

#define PushButton_w_LED_BL_0_3(B_LED,B_LED_Cx,InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,Val1,BackLight) \
PushButton_0_3(InCh, TmpNr, Rotate, Use0, ResetLong, OptCtrPar, Timeout) \
Status_ButtonBL_0_3(B_LED, B_LED_Cx, Val1, BackLight)

`defined @` MobaLedLib.h#512

I depend on these macros:

PushButton_w_LED_BL_0_3 | PushButton_0_3 | CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_1
Status_ButtonBL_0_3 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec
_Cx2StCh

### PushButton_w_LED_BL_0_4 [References: 0] Defined? True

#define PushButton_w_LED_BL_0_4(B_LED,B_LED_Cx,InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,Val1,BackLight) \
PushButton_0_4(InCh, TmpNr, Rotate, Use0, ResetLong, OptCtrPar, Timeout) \
Status_ButtonBL_0_4(B_LED, B_LED_Cx, Val1, BackLight)

`defined @` MobaLedLib.h#516

I depend on these macros:

PushButton_w_LED_BL_0_4 | PushButton_0_4 | CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_1
Status_ButtonBL_0_4 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec
_Cx2StCh

### PushButton_w_LED_BL_0_5 [References: 0] Defined? True

#define PushButton_w_LED_BL_0_5(B_LED,B_LED_Cx,InCh,TmpNr,Rotate,Use0,ResetLong,OptCtrPar,Timeout,Val1,BackLight) \
PushButton_0_5(InCh, TmpNr, Rotate, Use0, ResetLong, OptCtrPar, Timeout) \
Status_ButtonBL_0_5(B_LED, B_LED_Cx, Val1, BackLight)

`defined @` MobaLedLib.h#520

I depend on these macros:

PushButton_w_LED_BL_0_5 | PushButton_0_5 | CF_RESET_LONG
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_1
Status_ButtonBL_0_5 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec
_Cx2StCh

### RAM0 [References: 0] Defined? True

#define RAM0 0

`defined @` Macros.h#708

### RAM10 [References: 0] Defined? True

#define RAM10 RAM9+RAM1

`defined @` Macros.h#718

I depend on these macros:

RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM10 | RAM11 | RAM12 | RAM13 | RAM14 | RAM15 | RAM16 | RAM17 | RAM18 | RAM19 | RAM20 | RAM21 | RAM22 | RAM23 | RAM24 | RAM25 | RAM26 | RAM27 | RAM28 | RAM29 | RAM30 | RAM31 | RAM32 | RAM33 | RAM34 | RAM35 | RAM36 | RAM37 | RAM38 | RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM100 [References: 0] Defined? True

#define RAM100 RAM99+RAM1

`defined @` Macros.h#808

I depend on these macros:

RAM100 | RAM1
RAM99 | RAM1
RAM98 | RAM1
RAM97 | RAM1
RAM96 | RAM1
RAM95 | RAM1
RAM94 | RAM1
RAM93 | RAM1
RAM92 | RAM1
RAM91 | RAM1
RAM90 | RAM1
RAM89 | RAM1
RAM88 | RAM1
RAM87 | RAM1
RAM86 | RAM1
RAM85 | RAM1
RAM84 | RAM1
RAM83 | RAM1
RAM82 | RAM1
RAM81 | RAM1
RAM80 | RAM1
RAM79 | RAM1
RAM78 | RAM1
RAM77 | RAM1
RAM76 | RAM1
RAM75 | RAM1
RAM74 | RAM1
RAM73 | RAM1
RAM72 | RAM1
RAM71 | RAM1
RAM70 | RAM1
RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

### RAM11 [References: 0] Defined? True

#define RAM11 RAM10+RAM1

`defined @` Macros.h#719

I depend on these macros:

RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM11 | RAM12 | RAM13 | RAM14 | RAM15 | RAM16 | RAM17 | RAM18 | RAM19 | RAM20 | RAM21 | RAM22 | RAM23 | RAM24 | RAM25 | RAM26 | RAM27 | RAM28 | RAM29 | RAM30 | RAM31 | RAM32 | RAM33 | RAM34 | RAM35 | RAM36 | RAM37 | RAM38 | RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM12 [References: 0] Defined? True

#define RAM12 RAM11+RAM1

`defined @` Macros.h#720

I depend on these macros:

RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM12 | RAM13 | RAM14 | RAM15 | RAM16 | RAM17 | RAM18 | RAM19 | RAM20 | RAM21 | RAM22 | RAM23 | RAM24 | RAM25 | RAM26 | RAM27 | RAM28 | RAM29 | RAM30 | RAM31 | RAM32 | RAM33 | RAM34 | RAM35 | RAM36 | RAM37 | RAM38 | RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM13 [References: 0] Defined? True

#define RAM13 RAM12+RAM1

`defined @` Macros.h#721

I depend on these macros:

RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM13 | RAM14 | RAM15 | RAM16 | RAM17 | RAM18 | RAM19 | RAM20 | RAM21 | RAM22 | RAM23 | RAM24 | RAM25 | RAM26 | RAM27 | RAM28 | RAM29 | RAM30 | RAM31 | RAM32 | RAM33 | RAM34 | RAM35 | RAM36 | RAM37 | RAM38 | RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM14 [References: 0] Defined? True

#define RAM14 RAM13+RAM1

`defined @` Macros.h#722

I depend on these macros:

RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM14 | RAM15 | RAM16 | RAM17 | RAM18 | RAM19 | RAM20 | RAM21 | RAM22 | RAM23 | RAM24 | RAM25 | RAM26 | RAM27 | RAM28 | RAM29 | RAM30 | RAM31 | RAM32 | RAM33 | RAM34 | RAM35 | RAM36 | RAM37 | RAM38 | RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM15 [References: 0] Defined? True

#define RAM15 RAM14+RAM1

`defined @` Macros.h#723

I depend on these macros:

RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM15 | RAM16 | RAM17 | RAM18 | RAM19 | RAM20 | RAM21 | RAM22 | RAM23 | RAM24 | RAM25 | RAM26 | RAM27 | RAM28 | RAM29 | RAM30 | RAM31 | RAM32 | RAM33 | RAM34 | RAM35 | RAM36 | RAM37 | RAM38 | RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM16 [References: 0] Defined? True

#define RAM16 RAM15+RAM1

`defined @` Macros.h#724

I depend on these macros:

RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM16 | RAM17 | RAM18 | RAM19 | RAM20 | RAM21 | RAM22 | RAM23 | RAM24 | RAM25 | RAM26 | RAM27 | RAM28 | RAM29 | RAM30 | RAM31 | RAM32 | RAM33 | RAM34 | RAM35 | RAM36 | RAM37 | RAM38 | RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM17 [References: 0] Defined? True

#define RAM17 RAM16+RAM1

`defined @` Macros.h#725

I depend on these macros:

RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM17 | RAM18 | RAM19 | RAM20 | RAM21 | RAM22 | RAM23 | RAM24 | RAM25 | RAM26 | RAM27 | RAM28 | RAM29 | RAM30 | RAM31 | RAM32 | RAM33 | RAM34 | RAM35 | RAM36 | RAM37 | RAM38 | RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM18 [References: 0] Defined? True

#define RAM18 RAM17+RAM1

`defined @` Macros.h#726

I depend on these macros:

RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM18 | RAM19 | RAM20 | RAM21 | RAM22 | RAM23 | RAM24 | RAM25 | RAM26 | RAM27 | RAM28 | RAM29 | RAM30 | RAM31 | RAM32 | RAM33 | RAM34 | RAM35 | RAM36 | RAM37 | RAM38 | RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM19 [References: 0] Defined? True

#define RAM19 RAM18+RAM1

`defined @` Macros.h#727

I depend on these macros:

RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM19 | RAM20 | RAM21 | RAM22 | RAM23 | RAM24 | RAM25 | RAM26 | RAM27 | RAM28 | RAM29 | RAM30 | RAM31 | RAM32 | RAM33 | RAM34 | RAM35 | RAM36 | RAM37 | RAM38 | RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM20 [References: 0] Defined? True

#define RAM20 RAM19+RAM1

`defined @` Macros.h#728

I depend on these macros:

RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM20 | RAM21 | RAM22 | RAM23 | RAM24 | RAM25 | RAM26 | RAM27 | RAM28 | RAM29 | RAM30 | RAM31 | RAM32 | RAM33 | RAM34 | RAM35 | RAM36 | RAM37 | RAM38 | RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM21 [References: 0] Defined? True

#define RAM21 RAM20+RAM1

`defined @` Macros.h#729

I depend on these macros:

RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM21 | RAM22 | RAM23 | RAM24 | RAM25 | RAM26 | RAM27 | RAM28 | RAM29 | RAM30 | RAM31 | RAM32 | RAM33 | RAM34 | RAM35 | RAM36 | RAM37 | RAM38 | RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM22 [References: 0] Defined? True

#define RAM22 RAM21+RAM1

`defined @` Macros.h#730

I depend on these macros:

RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM22 | RAM23 | RAM24 | RAM25 | RAM26 | RAM27 | RAM28 | RAM29 | RAM30 | RAM31 | RAM32 | RAM33 | RAM34 | RAM35 | RAM36 | RAM37 | RAM38 | RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM23 [References: 0] Defined? True

#define RAM23 RAM22+RAM1

`defined @` Macros.h#731

I depend on these macros:

RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM23 | RAM24 | RAM25 | RAM26 | RAM27 | RAM28 | RAM29 | RAM30 | RAM31 | RAM32 | RAM33 | RAM34 | RAM35 | RAM36 | RAM37 | RAM38 | RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM24 [References: 0] Defined? True

#define RAM24 RAM23+RAM1

`defined @` Macros.h#732

I depend on these macros:

RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM24 | RAM25 | RAM26 | RAM27 | RAM28 | RAM29 | RAM30 | RAM31 | RAM32 | RAM33 | RAM34 | RAM35 | RAM36 | RAM37 | RAM38 | RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM25 [References: 0] Defined? True

#define RAM25 RAM24+RAM1

`defined @` Macros.h#733

I depend on these macros:

RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM25 | RAM26 | RAM27 | RAM28 | RAM29 | RAM30 | RAM31 | RAM32 | RAM33 | RAM34 | RAM35 | RAM36 | RAM37 | RAM38 | RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM26 [References: 0] Defined? True

#define RAM26 RAM25+RAM1

`defined @` Macros.h#734

I depend on these macros:

RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM26 | RAM27 | RAM28 | RAM29 | RAM30 | RAM31 | RAM32 | RAM33 | RAM34 | RAM35 | RAM36 | RAM37 | RAM38 | RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM27 [References: 0] Defined? True

#define RAM27 RAM26+RAM1

`defined @` Macros.h#735

I depend on these macros:

RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM27 | RAM28 | RAM29 | RAM30 | RAM31 | RAM32 | RAM33 | RAM34 | RAM35 | RAM36 | RAM37 | RAM38 | RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM28 [References: 0] Defined? True

#define RAM28 RAM27+RAM1

`defined @` Macros.h#736

I depend on these macros:

RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM28 | RAM29 | RAM30 | RAM31 | RAM32 | RAM33 | RAM34 | RAM35 | RAM36 | RAM37 | RAM38 | RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM29 [References: 0] Defined? True

#define RAM29 RAM28+RAM1

`defined @` Macros.h#737

I depend on these macros:

RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM29 | RAM30 | RAM31 | RAM32 | RAM33 | RAM34 | RAM35 | RAM36 | RAM37 | RAM38 | RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM30 [References: 0] Defined? True

#define RAM30 RAM29+RAM1

`defined @` Macros.h#738

I depend on these macros:

RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM30 | RAM31 | RAM32 | RAM33 | RAM34 | RAM35 | RAM36 | RAM37 | RAM38 | RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM31 [References: 0] Defined? True

#define RAM31 RAM30+RAM1

`defined @` Macros.h#739

I depend on these macros:

RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM31 | RAM32 | RAM33 | RAM34 | RAM35 | RAM36 | RAM37 | RAM38 | RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM32 [References: 0] Defined? True

#define RAM32 RAM31+RAM1

`defined @` Macros.h#740

I depend on these macros:

RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM32 | RAM33 | RAM34 | RAM35 | RAM36 | RAM37 | RAM38 | RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM33 [References: 0] Defined? True

#define RAM33 RAM32+RAM1

`defined @` Macros.h#741

I depend on these macros:

RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM33 | RAM34 | RAM35 | RAM36 | RAM37 | RAM38 | RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM34 [References: 0] Defined? True

#define RAM34 RAM33+RAM1

`defined @` Macros.h#742

I depend on these macros:

RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM34 | RAM35 | RAM36 | RAM37 | RAM38 | RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM35 [References: 0] Defined? True

#define RAM35 RAM34+RAM1

`defined @` Macros.h#743

I depend on these macros:

RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM35 | RAM36 | RAM37 | RAM38 | RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM36 [References: 0] Defined? True

#define RAM36 RAM35+RAM1

`defined @` Macros.h#744

I depend on these macros:

RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM36 | RAM37 | RAM38 | RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM37 [References: 0] Defined? True

#define RAM37 RAM36+RAM1

`defined @` Macros.h#745

I depend on these macros:

RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM37 | RAM38 | RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM38 [References: 0] Defined? True

#define RAM38 RAM37+RAM1

`defined @` Macros.h#746

I depend on these macros:

RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM38 | RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM39 [References: 0] Defined? True

#define RAM39 RAM38+RAM1

`defined @` Macros.h#747

I depend on these macros:

RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM40 [References: 0] Defined? True

#define RAM40 RAM39+RAM1

`defined @` Macros.h#748

I depend on these macros:

RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM41 [References: 0] Defined? True

#define RAM41 RAM40+RAM1

`defined @` Macros.h#749

I depend on these macros:

RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM42 [References: 0] Defined? True

#define RAM42 RAM41+RAM1

`defined @` Macros.h#750

I depend on these macros:

RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM43 [References: 0] Defined? True

#define RAM43 RAM42+RAM1

`defined @` Macros.h#751

I depend on these macros:

RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM44 [References: 0] Defined? True

#define RAM44 RAM43+RAM1

`defined @` Macros.h#752

I depend on these macros:

RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM45 [References: 0] Defined? True

#define RAM45 RAM44+RAM1

`defined @` Macros.h#753

I depend on these macros:

RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM46 [References: 0] Defined? True

#define RAM46 RAM45+RAM1

`defined @` Macros.h#754

I depend on these macros:

RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM47 [References: 0] Defined? True

#define RAM47 RAM46+RAM1

`defined @` Macros.h#755

I depend on these macros:

RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM48 [References: 0] Defined? True

#define RAM48 RAM47+RAM1

`defined @` Macros.h#756

I depend on these macros:

RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM49 [References: 0] Defined? True

#define RAM49 RAM48+RAM1

`defined @` Macros.h#757

I depend on these macros:

RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM50 [References: 0] Defined? True

#define RAM50 RAM49+RAM1

`defined @` Macros.h#758

I depend on these macros:

RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM51 [References: 0] Defined? True

#define RAM51 RAM50+RAM1

`defined @` Macros.h#759

I depend on these macros:

RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM52 [References: 0] Defined? True

#define RAM52 RAM51+RAM1

`defined @` Macros.h#760

I depend on these macros:

RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM53 [References: 0] Defined? True

#define RAM53 RAM52+RAM1

`defined @` Macros.h#761

I depend on these macros:

RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM54 [References: 0] Defined? True

#define RAM54 RAM53+RAM1

`defined @` Macros.h#762

I depend on these macros:

RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM55 [References: 0] Defined? True

#define RAM55 RAM54+RAM1

`defined @` Macros.h#763

I depend on these macros:

RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM56 [References: 0] Defined? True

#define RAM56 RAM55+RAM1

`defined @` Macros.h#764

I depend on these macros:

RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM57 [References: 0] Defined? True

#define RAM57 RAM56+RAM1

`defined @` Macros.h#765

I depend on these macros:

RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM58 [References: 0] Defined? True

#define RAM58 RAM57+RAM1

`defined @` Macros.h#766

I depend on these macros:

RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM59 [References: 0] Defined? True

#define RAM59 RAM58+RAM1

`defined @` Macros.h#767

I depend on these macros:

RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM60 [References: 0] Defined? True

#define RAM60 RAM59+RAM1

`defined @` Macros.h#768

I depend on these macros:

RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM61 [References: 0] Defined? True

#define RAM61 RAM60+RAM1

`defined @` Macros.h#769

I depend on these macros:

RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM62 [References: 0] Defined? True

#define RAM62 RAM61+RAM1

`defined @` Macros.h#770

I depend on these macros:

RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM63 [References: 0] Defined? True

#define RAM63 RAM62+RAM1

`defined @` Macros.h#771

I depend on these macros:

RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM64 [References: 0] Defined? True

#define RAM64 RAM63+RAM1

`defined @` Macros.h#772

I depend on these macros:

RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM65 [References: 0] Defined? True

#define RAM65 RAM64+RAM1

`defined @` Macros.h#773

I depend on these macros:

RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM66 [References: 0] Defined? True

#define RAM66 RAM65+RAM1

`defined @` Macros.h#774

I depend on these macros:

RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM67 [References: 0] Defined? True

#define RAM67 RAM66+RAM1

`defined @` Macros.h#775

I depend on these macros:

RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM68 [References: 0] Defined? True

#define RAM68 RAM67+RAM1

`defined @` Macros.h#776

I depend on these macros:

RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM69 [References: 0] Defined? True

#define RAM69 RAM68+RAM1

`defined @` Macros.h#777

I depend on these macros:

RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM70 [References: 0] Defined? True

#define RAM70 RAM69+RAM1

`defined @` Macros.h#778

I depend on these macros:

RAM70 | RAM1
RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM71 [References: 0] Defined? True

#define RAM71 RAM70+RAM1

`defined @` Macros.h#779

I depend on these macros:

RAM71 | RAM1
RAM70 | RAM1
RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM72 [References: 0] Defined? True

#define RAM72 RAM71+RAM1

`defined @` Macros.h#780

I depend on these macros:

RAM72 | RAM1
RAM71 | RAM1
RAM70 | RAM1
RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM73 [References: 0] Defined? True

#define RAM73 RAM72+RAM1

`defined @` Macros.h#781

I depend on these macros:

RAM73 | RAM1
RAM72 | RAM1
RAM71 | RAM1
RAM70 | RAM1
RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM74 [References: 0] Defined? True

#define RAM74 RAM73+RAM1

`defined @` Macros.h#782

I depend on these macros:

RAM74 | RAM1
RAM73 | RAM1
RAM72 | RAM1
RAM71 | RAM1
RAM70 | RAM1
RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM75 [References: 0] Defined? True

#define RAM75 RAM74+RAM1

`defined @` Macros.h#783

I depend on these macros:

RAM75 | RAM1
RAM74 | RAM1
RAM73 | RAM1
RAM72 | RAM1
RAM71 | RAM1
RAM70 | RAM1
RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM76 [References: 0] Defined? True

#define RAM76 RAM75+RAM1

`defined @` Macros.h#784

I depend on these macros:

RAM76 | RAM1
RAM75 | RAM1
RAM74 | RAM1
RAM73 | RAM1
RAM72 | RAM1
RAM71 | RAM1
RAM70 | RAM1
RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM77 [References: 0] Defined? True

#define RAM77 RAM76+RAM1

`defined @` Macros.h#785

I depend on these macros:

RAM77 | RAM1
RAM76 | RAM1
RAM75 | RAM1
RAM74 | RAM1
RAM73 | RAM1
RAM72 | RAM1
RAM71 | RAM1
RAM70 | RAM1
RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM78 [References: 0] Defined? True

#define RAM78 RAM77+RAM1

`defined @` Macros.h#786

I depend on these macros:

RAM78 | RAM1
RAM77 | RAM1
RAM76 | RAM1
RAM75 | RAM1
RAM74 | RAM1
RAM73 | RAM1
RAM72 | RAM1
RAM71 | RAM1
RAM70 | RAM1
RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM79 [References: 0] Defined? True

#define RAM79 RAM78+RAM1

`defined @` Macros.h#787

I depend on these macros:

RAM79 | RAM1
RAM78 | RAM1
RAM77 | RAM1
RAM76 | RAM1
RAM75 | RAM1
RAM74 | RAM1
RAM73 | RAM1
RAM72 | RAM1
RAM71 | RAM1
RAM70 | RAM1
RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM8 [References: 0] Defined? True

#define RAM8 RAM7+RAM1

`defined @` Macros.h#716

I depend on these macros:

RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM8 | RAM9 | RAM10 | RAM11 | RAM12 | RAM13 | RAM14 | RAM15 | RAM16 | RAM17 | RAM18 | RAM19 | RAM20 | RAM21 | RAM22 | RAM23 | RAM24 | RAM25 | RAM26 | RAM27 | RAM28 | RAM29 | RAM30 | RAM31 | RAM32 | RAM33 | RAM34 | RAM35 | RAM36 | RAM37 | RAM38 | RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM80 [References: 0] Defined? True

#define RAM80 RAM79+RAM1

`defined @` Macros.h#788

I depend on these macros:

RAM80 | RAM1
RAM79 | RAM1
RAM78 | RAM1
RAM77 | RAM1
RAM76 | RAM1
RAM75 | RAM1
RAM74 | RAM1
RAM73 | RAM1
RAM72 | RAM1
RAM71 | RAM1
RAM70 | RAM1
RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM81 [References: 0] Defined? True

#define RAM81 RAM80+RAM1

`defined @` Macros.h#789

I depend on these macros:

RAM81 | RAM1
RAM80 | RAM1
RAM79 | RAM1
RAM78 | RAM1
RAM77 | RAM1
RAM76 | RAM1
RAM75 | RAM1
RAM74 | RAM1
RAM73 | RAM1
RAM72 | RAM1
RAM71 | RAM1
RAM70 | RAM1
RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM82 [References: 0] Defined? True

#define RAM82 RAM81+RAM1

`defined @` Macros.h#790

I depend on these macros:

RAM82 | RAM1
RAM81 | RAM1
RAM80 | RAM1
RAM79 | RAM1
RAM78 | RAM1
RAM77 | RAM1
RAM76 | RAM1
RAM75 | RAM1
RAM74 | RAM1
RAM73 | RAM1
RAM72 | RAM1
RAM71 | RAM1
RAM70 | RAM1
RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM83 [References: 0] Defined? True

#define RAM83 RAM82+RAM1

`defined @` Macros.h#791

I depend on these macros:

RAM83 | RAM1
RAM82 | RAM1
RAM81 | RAM1
RAM80 | RAM1
RAM79 | RAM1
RAM78 | RAM1
RAM77 | RAM1
RAM76 | RAM1
RAM75 | RAM1
RAM74 | RAM1
RAM73 | RAM1
RAM72 | RAM1
RAM71 | RAM1
RAM70 | RAM1
RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM84 [References: 0] Defined? True

#define RAM84 RAM83+RAM1

`defined @` Macros.h#792

I depend on these macros:

RAM84 | RAM1
RAM83 | RAM1
RAM82 | RAM1
RAM81 | RAM1
RAM80 | RAM1
RAM79 | RAM1
RAM78 | RAM1
RAM77 | RAM1
RAM76 | RAM1
RAM75 | RAM1
RAM74 | RAM1
RAM73 | RAM1
RAM72 | RAM1
RAM71 | RAM1
RAM70 | RAM1
RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM85 [References: 0] Defined? True

#define RAM85 RAM84+RAM1

`defined @` Macros.h#793

I depend on these macros:

RAM85 | RAM1
RAM84 | RAM1
RAM83 | RAM1
RAM82 | RAM1
RAM81 | RAM1
RAM80 | RAM1
RAM79 | RAM1
RAM78 | RAM1
RAM77 | RAM1
RAM76 | RAM1
RAM75 | RAM1
RAM74 | RAM1
RAM73 | RAM1
RAM72 | RAM1
RAM71 | RAM1
RAM70 | RAM1
RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM86 [References: 0] Defined? True

#define RAM86 RAM85+RAM1

`defined @` Macros.h#794

I depend on these macros:

RAM86 | RAM1
RAM85 | RAM1
RAM84 | RAM1
RAM83 | RAM1
RAM82 | RAM1
RAM81 | RAM1
RAM80 | RAM1
RAM79 | RAM1
RAM78 | RAM1
RAM77 | RAM1
RAM76 | RAM1
RAM75 | RAM1
RAM74 | RAM1
RAM73 | RAM1
RAM72 | RAM1
RAM71 | RAM1
RAM70 | RAM1
RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM87 [References: 0] Defined? True

#define RAM87 RAM86+RAM1

`defined @` Macros.h#795

I depend on these macros:

RAM87 | RAM1
RAM86 | RAM1
RAM85 | RAM1
RAM84 | RAM1
RAM83 | RAM1
RAM82 | RAM1
RAM81 | RAM1
RAM80 | RAM1
RAM79 | RAM1
RAM78 | RAM1
RAM77 | RAM1
RAM76 | RAM1
RAM75 | RAM1
RAM74 | RAM1
RAM73 | RAM1
RAM72 | RAM1
RAM71 | RAM1
RAM70 | RAM1
RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM88 [References: 0] Defined? True

#define RAM88 RAM87+RAM1

`defined @` Macros.h#796

I depend on these macros:

RAM88 | RAM1
RAM87 | RAM1
RAM86 | RAM1
RAM85 | RAM1
RAM84 | RAM1
RAM83 | RAM1
RAM82 | RAM1
RAM81 | RAM1
RAM80 | RAM1
RAM79 | RAM1
RAM78 | RAM1
RAM77 | RAM1
RAM76 | RAM1
RAM75 | RAM1
RAM74 | RAM1
RAM73 | RAM1
RAM72 | RAM1
RAM71 | RAM1
RAM70 | RAM1
RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM89 [References: 0] Defined? True

#define RAM89 RAM88+RAM1

`defined @` Macros.h#797

I depend on these macros:

RAM89 | RAM1
RAM88 | RAM1
RAM87 | RAM1
RAM86 | RAM1
RAM85 | RAM1
RAM84 | RAM1
RAM83 | RAM1
RAM82 | RAM1
RAM81 | RAM1
RAM80 | RAM1
RAM79 | RAM1
RAM78 | RAM1
RAM77 | RAM1
RAM76 | RAM1
RAM75 | RAM1
RAM74 | RAM1
RAM73 | RAM1
RAM72 | RAM1
RAM71 | RAM1
RAM70 | RAM1
RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM9 [References: 0] Defined? True

#define RAM9 RAM8+RAM1

`defined @` Macros.h#717

I depend on these macros:

RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM9 | RAM10 | RAM11 | RAM12 | RAM13 | RAM14 | RAM15 | RAM16 | RAM17 | RAM18 | RAM19 | RAM20 | RAM21 | RAM22 | RAM23 | RAM24 | RAM25 | RAM26 | RAM27 | RAM28 | RAM29 | RAM30 | RAM31 | RAM32 | RAM33 | RAM34 | RAM35 | RAM36 | RAM37 | RAM38 | RAM39 | RAM40 | RAM41 | RAM42 | RAM43 | RAM44 | RAM45 | RAM46 | RAM47 | RAM48 | RAM49 | RAM50 | RAM51 | RAM52 | RAM53 | RAM54 | RAM55 | RAM56 | RAM57 | RAM58 | RAM59 | RAM60 | RAM61 | RAM62 | RAM63 | RAM64 | RAM65 | RAM66 | RAM67 | RAM68 | RAM69 | RAM70 | RAM71 | RAM72 | RAM73 | RAM74 | RAM75 | RAM76 | RAM77 | RAM78 | RAM79 | RAM80 | RAM81 | RAM82 | RAM83 | RAM84 | RAM85 | RAM86 | RAM87 | RAM88 | RAM89 | RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM90 [References: 0] Defined? True

#define RAM90 RAM89+RAM1

`defined @` Macros.h#798

I depend on these macros:

RAM90 | RAM1
RAM89 | RAM1
RAM88 | RAM1
RAM87 | RAM1
RAM86 | RAM1
RAM85 | RAM1
RAM84 | RAM1
RAM83 | RAM1
RAM82 | RAM1
RAM81 | RAM1
RAM80 | RAM1
RAM79 | RAM1
RAM78 | RAM1
RAM77 | RAM1
RAM76 | RAM1
RAM75 | RAM1
RAM74 | RAM1
RAM73 | RAM1
RAM72 | RAM1
RAM71 | RAM1
RAM70 | RAM1
RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM90 | RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM91 [References: 0] Defined? True

#define RAM91 RAM90+RAM1

`defined @` Macros.h#799

I depend on these macros:

RAM91 | RAM1
RAM90 | RAM1
RAM89 | RAM1
RAM88 | RAM1
RAM87 | RAM1
RAM86 | RAM1
RAM85 | RAM1
RAM84 | RAM1
RAM83 | RAM1
RAM82 | RAM1
RAM81 | RAM1
RAM80 | RAM1
RAM79 | RAM1
RAM78 | RAM1
RAM77 | RAM1
RAM76 | RAM1
RAM75 | RAM1
RAM74 | RAM1
RAM73 | RAM1
RAM72 | RAM1
RAM71 | RAM1
RAM70 | RAM1
RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM91 | RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM92 [References: 0] Defined? True

#define RAM92 RAM91+RAM1

`defined @` Macros.h#800

I depend on these macros:

RAM92 | RAM1
RAM91 | RAM1
RAM90 | RAM1
RAM89 | RAM1
RAM88 | RAM1
RAM87 | RAM1
RAM86 | RAM1
RAM85 | RAM1
RAM84 | RAM1
RAM83 | RAM1
RAM82 | RAM1
RAM81 | RAM1
RAM80 | RAM1
RAM79 | RAM1
RAM78 | RAM1
RAM77 | RAM1
RAM76 | RAM1
RAM75 | RAM1
RAM74 | RAM1
RAM73 | RAM1
RAM72 | RAM1
RAM71 | RAM1
RAM70 | RAM1
RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM92 | RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM93 [References: 0] Defined? True

#define RAM93 RAM92+RAM1

`defined @` Macros.h#801

I depend on these macros:

RAM93 | RAM1
RAM92 | RAM1
RAM91 | RAM1
RAM90 | RAM1
RAM89 | RAM1
RAM88 | RAM1
RAM87 | RAM1
RAM86 | RAM1
RAM85 | RAM1
RAM84 | RAM1
RAM83 | RAM1
RAM82 | RAM1
RAM81 | RAM1
RAM80 | RAM1
RAM79 | RAM1
RAM78 | RAM1
RAM77 | RAM1
RAM76 | RAM1
RAM75 | RAM1
RAM74 | RAM1
RAM73 | RAM1
RAM72 | RAM1
RAM71 | RAM1
RAM70 | RAM1
RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM93 | RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM94 [References: 0] Defined? True

#define RAM94 RAM93+RAM1

`defined @` Macros.h#802

I depend on these macros:

RAM94 | RAM1
RAM93 | RAM1
RAM92 | RAM1
RAM91 | RAM1
RAM90 | RAM1
RAM89 | RAM1
RAM88 | RAM1
RAM87 | RAM1
RAM86 | RAM1
RAM85 | RAM1
RAM84 | RAM1
RAM83 | RAM1
RAM82 | RAM1
RAM81 | RAM1
RAM80 | RAM1
RAM79 | RAM1
RAM78 | RAM1
RAM77 | RAM1
RAM76 | RAM1
RAM75 | RAM1
RAM74 | RAM1
RAM73 | RAM1
RAM72 | RAM1
RAM71 | RAM1
RAM70 | RAM1
RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM94 | RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM95 [References: 0] Defined? True

#define RAM95 RAM94+RAM1

`defined @` Macros.h#803

I depend on these macros:

RAM95 | RAM1
RAM94 | RAM1
RAM93 | RAM1
RAM92 | RAM1
RAM91 | RAM1
RAM90 | RAM1
RAM89 | RAM1
RAM88 | RAM1
RAM87 | RAM1
RAM86 | RAM1
RAM85 | RAM1
RAM84 | RAM1
RAM83 | RAM1
RAM82 | RAM1
RAM81 | RAM1
RAM80 | RAM1
RAM79 | RAM1
RAM78 | RAM1
RAM77 | RAM1
RAM76 | RAM1
RAM75 | RAM1
RAM74 | RAM1
RAM73 | RAM1
RAM72 | RAM1
RAM71 | RAM1
RAM70 | RAM1
RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM95 | RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM96 [References: 0] Defined? True

#define RAM96 RAM95+RAM1

`defined @` Macros.h#804

I depend on these macros:

RAM96 | RAM1
RAM95 | RAM1
RAM94 | RAM1
RAM93 | RAM1
RAM92 | RAM1
RAM91 | RAM1
RAM90 | RAM1
RAM89 | RAM1
RAM88 | RAM1
RAM87 | RAM1
RAM86 | RAM1
RAM85 | RAM1
RAM84 | RAM1
RAM83 | RAM1
RAM82 | RAM1
RAM81 | RAM1
RAM80 | RAM1
RAM79 | RAM1
RAM78 | RAM1
RAM77 | RAM1
RAM76 | RAM1
RAM75 | RAM1
RAM74 | RAM1
RAM73 | RAM1
RAM72 | RAM1
RAM71 | RAM1
RAM70 | RAM1
RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM96 | RAM97 | RAM98 | RAM99 | RAM100

### RAM97 [References: 0] Defined? True

#define RAM97 RAM96+RAM1

`defined @` Macros.h#805

I depend on these macros:

RAM97 | RAM1
RAM96 | RAM1
RAM95 | RAM1
RAM94 | RAM1
RAM93 | RAM1
RAM92 | RAM1
RAM91 | RAM1
RAM90 | RAM1
RAM89 | RAM1
RAM88 | RAM1
RAM87 | RAM1
RAM86 | RAM1
RAM85 | RAM1
RAM84 | RAM1
RAM83 | RAM1
RAM82 | RAM1
RAM81 | RAM1
RAM80 | RAM1
RAM79 | RAM1
RAM78 | RAM1
RAM77 | RAM1
RAM76 | RAM1
RAM75 | RAM1
RAM74 | RAM1
RAM73 | RAM1
RAM72 | RAM1
RAM71 | RAM1
RAM70 | RAM1
RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM97 | RAM98 | RAM99 | RAM100

### RAM98 [References: 0] Defined? True

#define RAM98 RAM97+RAM1

`defined @` Macros.h#806

I depend on these macros:

RAM98 | RAM1
RAM97 | RAM1
RAM96 | RAM1
RAM95 | RAM1
RAM94 | RAM1
RAM93 | RAM1
RAM92 | RAM1
RAM91 | RAM1
RAM90 | RAM1
RAM89 | RAM1
RAM88 | RAM1
RAM87 | RAM1
RAM86 | RAM1
RAM85 | RAM1
RAM84 | RAM1
RAM83 | RAM1
RAM82 | RAM1
RAM81 | RAM1
RAM80 | RAM1
RAM79 | RAM1
RAM78 | RAM1
RAM77 | RAM1
RAM76 | RAM1
RAM75 | RAM1
RAM74 | RAM1
RAM73 | RAM1
RAM72 | RAM1
RAM71 | RAM1
RAM70 | RAM1
RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM98 | RAM99 | RAM100

### RAM99 [References: 0] Defined? True

#define RAM99 RAM98+RAM1

`defined @` Macros.h#807

I depend on these macros:

RAM99 | RAM1
RAM98 | RAM1
RAM97 | RAM1
RAM96 | RAM1
RAM95 | RAM1
RAM94 | RAM1
RAM93 | RAM1
RAM92 | RAM1
RAM91 | RAM1
RAM90 | RAM1
RAM89 | RAM1
RAM88 | RAM1
RAM87 | RAM1
RAM86 | RAM1
RAM85 | RAM1
RAM84 | RAM1
RAM83 | RAM1
RAM82 | RAM1
RAM81 | RAM1
RAM80 | RAM1
RAM79 | RAM1
RAM78 | RAM1
RAM77 | RAM1
RAM76 | RAM1
RAM75 | RAM1
RAM74 | RAM1
RAM73 | RAM1
RAM72 | RAM1
RAM71 | RAM1
RAM70 | RAM1
RAM69 | RAM1
RAM68 | RAM1
RAM67 | RAM1
RAM66 | RAM1
RAM65 | RAM1
RAM64 | RAM1
RAM63 | RAM1
RAM62 | RAM1
RAM61 | RAM1
RAM60 | RAM1
RAM59 | RAM1
RAM58 | RAM1
RAM57 | RAM1
RAM56 | RAM1
RAM55 | RAM1
RAM54 | RAM1
RAM53 | RAM1
RAM52 | RAM1
RAM51 | RAM1
RAM50 | RAM1
RAM49 | RAM1
RAM48 | RAM1
RAM47 | RAM1
RAM46 | RAM1
RAM45 | RAM1
RAM44 | RAM1
RAM43 | RAM1
RAM42 | RAM1
RAM41 | RAM1
RAM40 | RAM1
RAM39 | RAM1
RAM38 | RAM1
RAM37 | RAM1
RAM36 | RAM1
RAM35 | RAM1
RAM34 | RAM1
RAM33 | RAM1
RAM32 | RAM1
RAM31 | RAM1
RAM30 | RAM1
RAM29 | RAM1
RAM28 | RAM1
RAM27 | RAM1
RAM26 | RAM1
RAM25 | RAM1
RAM24 | RAM1
RAM23 | RAM1
RAM22 | RAM1
RAM21 | RAM1
RAM20 | RAM1
RAM19 | RAM1
RAM18 | RAM1
RAM17 | RAM1
RAM16 | RAM1
RAM15 | RAM1
RAM14 | RAM1
RAM13 | RAM1
RAM12 | RAM1
RAM11 | RAM1
RAM10 | RAM1
RAM9 | RAM1
RAM8 | RAM1
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1

These macros depend on me:

RAM99 | RAM100

### RAMN [References: 0] Defined? True

#define RAMN(n) RAM ## n

`defined @` Macros.h#810

These macros depend on me:

RAMN | Fire
XPatternT1 | DepSignal4
DepSignal4Bin
DepSignal4Bin_RGB
DepSignal4_RGB
EntrySignal3
EntrySignal3Bin
EntrySignal3Bin_RGB
EntrySignal3_RGB_BT | EntrySignal3_RGB
EntrySignal3_RGB_B
EntrySignal3_RGB_T
GleissperrsignalBin_RGB
Gleissperrsignal_RGB
HP_2_2Bin_RGB
HP_2_2_RGB
HS_5_PlusBin_RGB
HS_5_Plus_RGB
HS_5lBin_RGB
HS_5l_RGB
HS_5rBin_RGB
HS_5r_RGB
HS_EinfachBin_RGB
HS_Einfach_RGB
SingleLedSignal
SingleLedSignalEx
VorsignalBin_RGB
Vorsignal_RGB
XPatternT10
XPatternT11 | KS_Hauptsignal_Zs3_Zs1
KS_Hauptsignal_Zs3_Zs1Bin
KS_Hauptsignal_Zs3_Zs1Bin_RGB
KS_Hauptsignal_Zs3_Zs1_RGB
KS_Hauptsignal_Zs3_Zs6_Zs1
KS_Hauptsignal_Zs3_Zs6_Zs1Bin
KS_Hauptsignal_Zs3_Zs6_Zs1Bin_RGB
KS_Hauptsignal_Zs3_Zs6_Zs1_RGB
XPatternT12
XPatternT13
XPatternT14
XPatternT15
XPatternT16
XPatternT17
XPatternT18
XPatternT19
XPatternT2
XPatternT20
XPatternT21
XPatternT22
XPatternT23
XPatternT24
XPatternT25
XPatternT26
XPatternT27
XPatternT28
XPatternT29
XPatternT3
XPatternT30
XPatternT31
XPatternT32
XPatternT33
XPatternT34
XPatternT35
XPatternT36
XPatternT37
XPatternT38
XPatternT39
XPatternT4
XPatternT40
XPatternT41
XPatternT42
XPatternT43
XPatternT44
XPatternT45
XPatternT46
XPatternT47
XPatternT48
XPatternT49
XPatternT5
XPatternT50
XPatternT51
XPatternT52
XPatternT53
XPatternT54
XPatternT55
XPatternT56
XPatternT57
XPatternT58
XPatternT59
XPatternT6
XPatternT60
XPatternT61
XPatternT62
XPatternT63
XPatternT64
XPatternT7
XPatternT8
XPatternT9 | AndreaskrLT
AndreaskrLT3
AndreaskrLT3_RGB
AndreaskrLT_RGB
KS_Vorsignal_Zs3V
KS_Vorsignal_Zs3VBin
KS_Vorsignal_Zs3VBin_RGB
KS_Vorsignal_Zs3V_RGB
XPatternTE1
XPatternTE10
XPatternTE11
XPatternTE12
XPatternTE13
XPatternTE14
XPatternTE15
XPatternTE16
XPatternTE17
XPatternTE18
XPatternTE19
XPatternTE2
XPatternTE20
XPatternTE21
XPatternTE22
XPatternTE23
XPatternTE24
XPatternTE25
XPatternTE26
XPatternTE27
XPatternTE28
XPatternTE29
XPatternTE3
XPatternTE30
XPatternTE31
XPatternTE32
XPatternTE33
XPatternTE34
XPatternTE35
XPatternTE36
XPatternTE37
XPatternTE38
XPatternTE39
XPatternTE4
XPatternTE40
XPatternTE41
XPatternTE42
XPatternTE43
XPatternTE44
XPatternTE45
XPatternTE46
XPatternTE47
XPatternTE48
XPatternTE49
XPatternTE5
XPatternTE50
XPatternTE51
XPatternTE52
XPatternTE53
XPatternTE54
XPatternTE55
XPatternTE56
XPatternTE57
XPatternTE58
XPatternTE59
XPatternTE6
XPatternTE60
XPatternTE61
XPatternTE62
XPatternTE63
XPatternTE64
XPatternTE7
XPatternTE8
XPatternTE9

### RANDMUX_T [References: 0] Defined? True

#define RANDMUX_T 2

`defined @` Macros.h#516

These macros depend on me:

RANDMUX_T | RandMux | RandCntMux

### RANDOM_T [References: 0] Defined? True

#define RANDOM_T 140

`defined @` Macros.h#654

These macros depend on me:

RANDOM_T | Random | ButtonFunc
Def_Neon_Misha
Flash
RandWelding

### RECEIVE_LED_COLOR_PER_RS232 [References: 0] Defined? True

#define RECEIVE_LED_COLOR_PER_RS232

`defined @` leds_autoprog.h#26

### RF_NOT_SAME [References: 0] Defined? True

#define RF_NOT_SAME 0b00001000

`defined @` MobaLedLib.h#1050

These macros depend on me:

RF_NOT_SAME | _CHECK_MODE_RF_NOT_SAME | RandMux | RandCntMux

### RF_SEQ [References: 0] Defined? True

#define RF_SEQ 0b00000010

`defined @` MobaLedLib.h#1047

These macros depend on me:

RF_SEQ | RandCntMux

### RF_SLOW [References: 0] Defined? True

#define RF_SLOW 0b00000001

`defined @` MobaLedLib.h#1046

These macros depend on me:

RF_SLOW | _RAND_MODE2 | RandMux | RandCntMux
_RAND_MODE4 | Random | ButtonFunc
Def_Neon_Misha
Flash
RandWelding

### RF_STAY_ON [References: 0] Defined? True

#define RF_STAY_ON 0b00000100

`defined @` MobaLedLib.h#1048

These macros depend on me:

RF_STAY_ON | ButtonFunc

### RGB_AmpelX [References: 0] Defined? True

#define RGB_AmpelX(LED,InCh) PatternT4(LED,0,InCh,18,0,255,0,0,3 Sec,1 Sec,10 Sec,3 \
Sec,1,2,100,8,0,40,0,134,0,1,2,4,200,16,0,80,0,12)

`defined @` MobaLedLib.h#181

I depend on these macros:

RGB_AmpelX | PatternT4 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT4_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
Sec

### RGB_AmpelXFade [References: 0] Defined? True

#define RGB_AmpelXFade(LED,InCh) APatternT8(LED,0,InCh,18,0,255,0,0,200,2 Sec,200,1 \
Sec,200,10 Sec,200,3 Sec,1,2,4,8,144,33,64,134,0,128,2,0,10,128,33,0,134,0,1,2,4,8,16,32,67,128,12,1,0,5,0,20,0,67,0,12) \

`defined @` MobaLedLib.h#182

I depend on these macros:

RGB_AmpelXFade | APatternT8 | APATTERNT8_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
Sec

### RGB_AmpelX_A [References: 0] Defined? True

#define RGB_AmpelX_A(LED,InCh) PatternT12(LED,0,InCh,17,0,255,0,0,2 Sec,2 sec,10 \
Sec,500,500,500,500,500,500,500,500,2 \
Sec,1,2,50,4,0,10,0,16,0,40,0,64,0,160,0,0,1,128,2,0,4,0,10,192,16,16,32,32,64,70,0,192,0,0,1,0,3,0,4,0,12,0,16,0,48,0,64,0,192,0,24\
)

`defined @` MobaLedLib.h#183

I depend on these macros:

RGB_AmpelX_A | PatternT12 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT12_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
Sec
sec | Sec

### RGB_Heartbeat2 [References: 0] Defined? True

#define RGB_Heartbeat2(LED,MinBrightness,MaxBrightness) New_HSV_Group() \
APatternT2(LED,192,SI_1,1,0,255,0,PM_HSV,60 Sek,0 ms,1) APatternT1(LED, \
194,SI_1,1,MinBrightness,MaxBrightness,0,PM_HSV|PF_EASEINOUT,1 Sek,1)

`defined @` MobaLedLib.h#384

I depend on these macros:

RGB_Heartbeat2 | APatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
APatternT2 | APATTERNT2_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
New_HSV_Group | NEW_HSV_GROUP_T
RAM3 | RAM1
RAM2 | RAM1
PF_EASEINOUT
PM_HSV
SI_1
Sek | Sec
ms

### RGB_Heartbeat_Color [References: 0] Defined? True

#define RGB_Heartbeat_Color(LED,MinBrightness,MaxBrightness,Color,Duration) New_HSV_Group() \
APatternT1(LED,224,SI_1,1,Color,Color,0,PM_HSV,0 ms,1) APatternT1(LED, \
194,SI_1,1,MinBrightness,MaxBrightness,0,PM_HSV|PF_EASEINOUT,Duration,1)

`defined @` MobaLedLib.h#389

I depend on these macros:

RGB_Heartbeat_Color | APatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
New_HSV_Group | NEW_HSV_GROUP_T
RAM3 | RAM1
RAM2 | RAM1
PF_EASEINOUT
PM_HSV
SI_1
ms

### RGB_Ring [References: 0] Defined? True

#define RGB_Ring(LED,InCh,Brightness,Duration) \
APatternT1(LED,4,InCh,36,0,Brightness,0,0,Duration,137,98,8,162,28,195,52,142,34,72,162, \
24,130,40,199,48,141,163,40,146,40,134,32,202,49,76,227,56,138,36,138,33,136,114,12,211, \
52,142,34,137,98,8,162,28,195,48,141,163,72,162,24,130,40,199,49,76,227,40,146,40,134,32, \
202,114,12,211,56,138,36,138,33,136,162,28,195,52,142,34,137,98,8,130,40,199,48,141,163, \
72,162,24,134,32,202,49,76,227,40,146,40,138,33,136,114,12,211,56,138,36)

`defined @` MobaLedLib.h#394

I depend on these macros:

RGB_Ring | APatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B

### RM_NORMAL [References: 0] Defined? True

#define RM_NORMAL 0b00000000

`defined @` MobaLedLib.h#1045

These macros depend on me:

RM_NORMAL | Def_Neon_Misha
Flash
RandWelding

### ROOM_BRIGHT [References: 0] Defined? True

#define ROOM_BRIGHT 1

`defined @` MobaLedLib.h#1081

### ROOM_COL0 [References: 0] Defined? True

#define ROOM_COL0 5

`defined @` MobaLedLib.h#1085

### ROOM_COL1 [References: 0] Defined? True

#define ROOM_COL1 6

`defined @` MobaLedLib.h#1086

### ROOM_COL2 [References: 0] Defined? True

#define ROOM_COL2 7

`defined @` MobaLedLib.h#1087

### ROOM_COL3 [References: 0] Defined? True

#define ROOM_COL3 8

`defined @` MobaLedLib.h#1088

### ROOM_COL345 [References: 0] Defined? True

#define ROOM_COL345 11

`defined @` MobaLedLib.h#1091

### ROOM_COL4 [References: 0] Defined? True

#define ROOM_COL4 9

`defined @` MobaLedLib.h#1089

### ROOM_COL5 [References: 0] Defined? True

#define ROOM_COL5 10

`defined @` MobaLedLib.h#1090

### ROOM_COL_CNT [References: 0] Defined? True

#define ROOM_COL_CNT 17

`defined @` MobaLedLib.h#1273

### ROOM_D_RED [References: 0] Defined? True

#define ROOM_D_RED 4

`defined @` MobaLedLib.h#1084

### ROOM_TV0 [References: 0] Defined? True

#define ROOM_TV0 19

`defined @` MobaLedLib.h#1099

### ROOM_TV1 [References: 0] Defined? True

#define ROOM_TV1 23

`defined @` MobaLedLib.h#1103

### RS_FlipFlop [References: 0] Defined? True

#define RS_FlipFlop(DstVar,R_InCh,S_InCh) Counter(_CM_RS_FlipFlop1, S_InCh, R_InCh, 0, \
DstVar)

`defined @` MobaLedLib.h#358

I depend on these macros:

RS_FlipFlop | Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
_CM_RS_FlipFlop1 | CF_BINARY
CF_UP_DOWN

These macros depend on me:

RS_FlipFlop | _Herz_MoRelais_RS | Herz_MoRelais
Herz_MoRelais_I

### RS_FlipFlop2 [References: 0] Defined? True

#define RS_FlipFlop2(DstVar0,DstVar1,R_InCh,S_InCh) Counter(_CM_RS_FlipFlop2, S_InCh, \
R_InCh, 0, DstVar0, DstVar1)

`defined @` MobaLedLib.h#374

I depend on these macros:

RS_FlipFlop2 | Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
_CM_RS_FlipFlop2 | CF_UP_DOWN

### RS_FlipFlop2Timeout [References: 0] Defined? True

#define RS_FlipFlop2Timeout(DstVar0,DstVar1,R_InCh,S_InCh,Timeout) Counter(_CM_RS_FlipFlop2, \
S_InCh, R_InCh, Timeout, DstVar0, DstVar1)

`defined @` MobaLedLib.h#375

I depend on these macros:

RS_FlipFlop2Timeout | Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
_CM_RS_FlipFlop2 | CF_UP_DOWN

### RS_FlipFlopInv [References: 0] Defined? True

#define RS_FlipFlopInv(DstVar,R_InCh,S_InCh) Counter(_CM_RS_FlipFlop2, S_InCh, R_InCh, 0, \
DstVar, DstVar)

`defined @` MobaLedLib.h#366

I depend on these macros:

RS_FlipFlopInv | Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
_CM_RS_FlipFlop2 | CF_UP_DOWN

### RS_FlipFlopInvTimeout [References: 0] Defined? True

#define RS_FlipFlopInvTimeout(DstVar,R_InCh,S_InCh,Timeout) Counter(_CM_RS_FlipFlop2, \
S_InCh, R_InCh, Timeout, DstVar, DstVar)

`defined @` MobaLedLib.h#367

I depend on these macros:

RS_FlipFlopInvTimeout | Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
_CM_RS_FlipFlop2 | CF_UP_DOWN

### RS_FlipFlopTimeout [References: 0] Defined? True

#define RS_FlipFlopTimeout(DstVar,R_InCh,S_InCh,Timeout) Counter(_CM_RS_FlipFlop1, S_InCh, \
R_InCh, Timeout, DstVar)

`defined @` MobaLedLib.h#359

I depend on these macros:

RS_FlipFlopTimeout | Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
_CM_RS_FlipFlop1 | CF_BINARY
CF_UP_DOWN

These macros depend on me:

RS_FlipFlopTimeout | _Herz_MoRelais_RS | Herz_MoRelais
Herz_MoRelais_I

### RandCntMux [References: 0] Defined? True

#define RandCntMux(DstVar1,DstVarN,InCh,Mode,MinTime,MaxTime) RandMux(DstVar1, DstVarN, \
InCh, Mode|RF_SEQ, MinTime, MaxTime)

`defined @` MobaLedLib.h#117

I depend on these macros:

RandCntMux | RF_SEQ
RandMux | RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RANDMUX_T
_CHECK_MODE_RF_NOT_SAME | RF_NOT_SAME
_RAND_MODE2 | RF_SLOW
_ALL_LT_MX2 | _LT_MX | _MAX_TIMER_VAL
_Tx2B2 | _RAND_DIV2 | _ALL_LT_MX2 | _LT_MX | _MAX_TIMER_VAL
_T2B | _W2B

### RandMux [References: 0] Defined? True

#define RandMux(DstVar1,DstVarN,InCh,Mode,MinTime,MaxTime) RANDMUX_T, DstVar1+RAM4, DstVarN, \
InCh, _CHECK_MODE_RF_NOT_SAME(Mode, DstVar1, DstVarN) | _RAND_MODE2((MinTime), \
(MaxTime)), _Tx2B2(MinTime, MaxTime), _Tx2B2(MaxTime, MinTime),

`defined @` MobaLedLib.h#116

I depend on these macros:

RandMux | RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RANDMUX_T
_CHECK_MODE_RF_NOT_SAME | RF_NOT_SAME
_RAND_MODE2 | RF_SLOW
_ALL_LT_MX2 | _LT_MX | _MAX_TIMER_VAL
_Tx2B2 | _RAND_DIV2 | _ALL_LT_MX2 | _LT_MX | _MAX_TIMER_VAL
_T2B | _W2B

These macros depend on me:

RandMux | RandCntMux

### RandWelding [References: 0] Defined? True

#define RandWelding(LED,InCh,Var,MinTime,MaxTime,MinOn,MaxOn) Random(Var, InCh, RM_NORMAL, \
MinTime, MaxTime, MinOn, MaxOn) Welding(LED, Var)

`defined @` MobaLedLib.h#121

I depend on these macros:

RandWelding | RM_NORMAL
Random | RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RANDOM_T
_RAND_MODE4 | RF_SLOW
_ALL_LT_MX4 | _ALL_LT_MX2 | _LT_MX | _MAX_TIMER_VAL
_Tx2B4 | _RAND_DIV4 | _ALL_LT_MX4 | _ALL_LT_MX2 | _LT_MX | _MAX_TIMER_VAL
_T2B | _W2B
Welding | RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
WELDING_T
_CHKL | NUM_LEDS
_ERR_LED_RANGE

### Random [References: 0] Defined? True

#define Random(DstVar,InCh,Mode,MinTime,MaxTime,MinOn,MaxOn) RANDOM_T, DstVar +RAM4, InCh, \
(Mode) | _RAND_MODE4((MinTime), (MaxTime), (MinOn), (MaxOn)), _Tx2B4(MinTime, \
MaxTime, MinOn, MaxOn), _Tx2B4(MaxTime, MinTime, MinOn, MaxOn), _Tx2B4(MinOn, \
MaxOn, MinTime, MaxTime), _Tx2B4(MaxOn, MinOn, MinTime, MaxTime),

`defined @` MobaLedLib.h#118

I depend on these macros:

Random | RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RANDOM_T
_RAND_MODE4 | RF_SLOW
_ALL_LT_MX4 | _ALL_LT_MX2 | _LT_MX | _MAX_TIMER_VAL
_Tx2B4 | _RAND_DIV4 | _ALL_LT_MX4 | _ALL_LT_MX2 | _LT_MX | _MAX_TIMER_VAL
_T2B | _W2B

These macros depend on me:

Random | ButtonFunc
Def_Neon_Misha
Flash
RandWelding

### SCHEDULE_T [References: 0] Defined? True

#define SCHEDULE_T 3

`defined @` Macros.h#517

These macros depend on me:

SCHEDULE_T | Schedule

### SETUP_FASTLED [References: 0] Defined? True

#define SETUP_FASTLED() CLEDController& controller0 = FastLED.addLeds<NEOPIXEL, 6>(leds+ \
0, 32); controller0.clearLeds(256); FastLED.setDither(DISABLE_DITHER);

`defined @` leds_autoprog.h#77

### SINGLE_LED1 [References: 0] Defined? True

#define SINGLE_LED1 55

`defined @` MobaLedLib.h#1135

### SINGLE_LED1D [References: 0] Defined? True

#define SINGLE_LED1D 58

`defined @` MobaLedLib.h#1138

### SINGLE_LED2 [References: 0] Defined? True

#define SINGLE_LED2 56

`defined @` MobaLedLib.h#1136

### SINGLE_LED2D [References: 0] Defined? True

#define SINGLE_LED2D 59

`defined @` MobaLedLib.h#1139

### SINGLE_LED3 [References: 0] Defined? True

#define SINGLE_LED3 57

`defined @` MobaLedLib.h#1137

### SINGLE_LED3D [References: 0] Defined? True

#define SINGLE_LED3D 60

`defined @` MobaLedLib.h#1140

### SI_Enable_Sound [References: 0] Defined? True

#define SI_Enable_Sound 253

`defined @` MobaLedLib.h#1157

These macros depend on me:

SI_Enable_Sound | Sound_ADKey | Sound_Loop
Sound_New_Loop
Sound_New_Next
Sound_New_PausePlay
Sound_New_PlayMode
Sound_New_Prev
Sound_New_Seq1
Sound_New_Seq10
Sound_New_Seq11
Sound_New_Seq12
Sound_New_Seq13
Sound_New_Seq14
Sound_New_Seq2
Sound_New_Seq3
Sound_New_Seq4
Sound_New_Seq5
Sound_New_Seq6
Sound_New_Seq7
Sound_New_Seq8
Sound_New_Seq9
Sound_New_USDSPI
Sound_Next
Sound_PausePlay
Sound_PlayMode
Sound_Prev
Sound_Seq1
Sound_Seq10
Sound_Seq11
Sound_Seq12
Sound_Seq13
Sound_Seq14
Sound_Seq2
Sound_Seq3
Sound_Seq4
Sound_Seq5
Sound_Seq6
Sound_Seq7
Sound_Seq8
Sound_Seq9
Sound_USDSPI
Sound_JQ6500_ADKey | Sound_JQ6500_BG_Next
Sound_JQ6500_BG_Prev
Sound_JQ6500_BG_Seq1
Sound_JQ6500_BG_Seq2
Sound_JQ6500_BG_Seq3
Sound_JQ6500_BG_Seq4
Sound_JQ6500_BG_Seq5
Sound_JQ6500_Next
Sound_JQ6500_Prev
Sound_JQ6500_Seq1
Sound_JQ6500_Seq2
Sound_JQ6500_Seq3
Sound_JQ6500_Seq4
Sound_JQ6500_Seq5

### SKIP_ROOM [References: 0] Defined? True

#define SKIP_ROOM 61

`defined @` MobaLedLib.h#1141

### SOUND_ADKEY1 [References: 0] Defined? True

#define SOUND_ADKEY1 255

`defined @` MobaLedLib.h#701

These macros depend on me:

SOUND_ADKEY1 | Sound_Seq1
Sound_Seq5
_LocalVar_Sound | Sound_Next_of_N_Reset | Sound_Next_of_N
Sound_PlayRandom

### SOUND_ADKEY10 [References: 0] Defined? True

#define SOUND_ADKEY10 11

`defined @` MobaLedLib.h#692

These macros depend on me:

SOUND_ADKEY10 | Sound_PlayMode
Sound_Seq14
_LocalVar_Sound | Sound_Next_of_N_Reset | Sound_Next_of_N
Sound_PlayRandom

### SOUND_ADKEY2 [References: 0] Defined? True

#define SOUND_ADKEY2 134

`defined @` MobaLedLib.h#700

These macros depend on me:

SOUND_ADKEY2 | Sound_Seq2
Sound_Seq6
_LocalVar_Sound | Sound_Next_of_N_Reset | Sound_Next_of_N
Sound_PlayRandom

### SOUND_ADKEY3 [References: 0] Defined? True

#define SOUND_ADKEY3 70

`defined @` MobaLedLib.h#699

These macros depend on me:

SOUND_ADKEY3 | Sound_Seq3
Sound_Seq7
_LocalVar_Sound | Sound_Next_of_N_Reset | Sound_Next_of_N
Sound_PlayRandom

### SOUND_ADKEY4 [References: 0] Defined? True

#define SOUND_ADKEY4 49

`defined @` MobaLedLib.h#698

These macros depend on me:

SOUND_ADKEY4 | Sound_Seq4
Sound_Seq8
_LocalVar_Sound | Sound_Next_of_N_Reset | Sound_Next_of_N
Sound_PlayRandom

### SOUND_ADKEY5 [References: 0] Defined? True

#define SOUND_ADKEY5 37

`defined @` MobaLedLib.h#697

These macros depend on me:

SOUND_ADKEY5 | Sound_DecVol
Sound_Prev
Sound_Seq9
_LocalVar_Sound | Sound_Next_of_N_Reset | Sound_Next_of_N
Sound_PlayRandom

### SOUND_ADKEY6 [References: 0] Defined? True

#define SOUND_ADKEY6 29

`defined @` MobaLedLib.h#696

These macros depend on me:

SOUND_ADKEY6 | Sound_IncVol
Sound_Next
Sound_Seq10
_LocalVar_Sound | Sound_Next_of_N_Reset | Sound_Next_of_N
Sound_PlayRandom

### SOUND_ADKEY7 [References: 0] Defined? True

#define SOUND_ADKEY7 25

`defined @` MobaLedLib.h#695

These macros depend on me:

SOUND_ADKEY7 | Sound_PausePlay
Sound_Seq11
_LocalVar_Sound | Sound_Next_of_N_Reset | Sound_Next_of_N
Sound_PlayRandom

### SOUND_ADKEY8 [References: 0] Defined? True

#define SOUND_ADKEY8 22

`defined @` MobaLedLib.h#694

These macros depend on me:

SOUND_ADKEY8 | Sound_Loop
Sound_Seq12
_LocalVar_Sound | Sound_Next_of_N_Reset | Sound_Next_of_N
Sound_PlayRandom

### SOUND_ADKEY9 [References: 0] Defined? True

#define SOUND_ADKEY9 17

`defined @` MobaLedLib.h#693

These macros depend on me:

SOUND_ADKEY9 | Sound_Seq13
Sound_USDSPI
_LocalVar_Sound | Sound_Next_of_N_Reset | Sound_Next_of_N
Sound_PlayRandom

### SOUND_JQ6500_ADKEY1_BG [References: 0] Defined? True

#define SOUND_JQ6500_ADKEY1_BG 32

`defined @` MobaLedLib.h#834

These macros depend on me:

SOUND_JQ6500_ADKEY1_BG | Sound_JQ6500_BG_Seq1
_LocalVar_Sound_JQ6500_BG | Sound_JQ6500_BG_Next_of_N_Reset | Sound_JQ6500_BG_Next_of_N
Sound_JQ6500_BG_PlayRandom

### SOUND_JQ6500_ADKEY1_N [References: 0] Defined? True

#define SOUND_JQ6500_ADKEY1_N 29

`defined @` MobaLedLib.h#825

These macros depend on me:

SOUND_JQ6500_ADKEY1_N | Sound_JQ6500_Seq1
_LocalVar_Sound_JQ6500 | Sound_JQ6500_Next_of_N_Reset | Sound_JQ6500_Next_of_N
Sound_JQ6500_PlayRandom

### SOUND_JQ6500_ADKEY2_BG [References: 0] Defined? True

#define SOUND_JQ6500_ADKEY2_BG 44

`defined @` MobaLedLib.h#835

These macros depend on me:

SOUND_JQ6500_ADKEY2_BG | Sound_JQ6500_BG_Seq2
_LocalVar_Sound_JQ6500_BG | Sound_JQ6500_BG_Next_of_N_Reset | Sound_JQ6500_BG_Next_of_N
Sound_JQ6500_BG_PlayRandom

### SOUND_JQ6500_ADKEY2_N [References: 0] Defined? True

#define SOUND_JQ6500_ADKEY2_N 40

`defined @` MobaLedLib.h#826

These macros depend on me:

SOUND_JQ6500_ADKEY2_N | Sound_JQ6500_Seq2
_LocalVar_Sound_JQ6500 | Sound_JQ6500_Next_of_N_Reset | Sound_JQ6500_Next_of_N
Sound_JQ6500_PlayRandom

### SOUND_JQ6500_ADKEY3_BG [References: 0] Defined? True

#define SOUND_JQ6500_ADKEY3_BG 56

`defined @` MobaLedLib.h#836

These macros depend on me:

SOUND_JQ6500_ADKEY3_BG | Sound_JQ6500_BG_Seq3
_LocalVar_Sound_JQ6500_BG | Sound_JQ6500_BG_Next_of_N_Reset | Sound_JQ6500_BG_Next_of_N
Sound_JQ6500_BG_PlayRandom

### SOUND_JQ6500_ADKEY3_N [References: 0] Defined? True

#define SOUND_JQ6500_ADKEY3_N 50

`defined @` MobaLedLib.h#827

These macros depend on me:

SOUND_JQ6500_ADKEY3_N | Sound_JQ6500_Seq3
_LocalVar_Sound_JQ6500 | Sound_JQ6500_Next_of_N_Reset | Sound_JQ6500_Next_of_N
Sound_JQ6500_PlayRandom

### SOUND_JQ6500_ADKEY4_BG [References: 0] Defined? True

#define SOUND_JQ6500_ADKEY4_BG 68

`defined @` MobaLedLib.h#837

These macros depend on me:

SOUND_JQ6500_ADKEY4_BG | Sound_JQ6500_BG_Seq4
_LocalVar_Sound_JQ6500_BG | Sound_JQ6500_BG_Next_of_N_Reset | Sound_JQ6500_BG_Next_of_N
Sound_JQ6500_BG_PlayRandom

### SOUND_JQ6500_ADKEY4_N [References: 0] Defined? True

#define SOUND_JQ6500_ADKEY4_N 60

`defined @` MobaLedLib.h#828

These macros depend on me:

SOUND_JQ6500_ADKEY4_N | Sound_JQ6500_Seq4
_LocalVar_Sound_JQ6500 | Sound_JQ6500_Next_of_N_Reset | Sound_JQ6500_Next_of_N
Sound_JQ6500_PlayRandom

### SOUND_JQ6500_ADKEY5_BG [References: 0] Defined? True

#define SOUND_JQ6500_ADKEY5_BG 90

`defined @` MobaLedLib.h#838

These macros depend on me:

SOUND_JQ6500_ADKEY5_BG | Sound_JQ6500_BG_Seq5
_LocalVar_Sound_JQ6500_BG | Sound_JQ6500_BG_Next_of_N_Reset | Sound_JQ6500_BG_Next_of_N
Sound_JQ6500_BG_PlayRandom

### SOUND_JQ6500_ADKEY5_N [References: 0] Defined? True

#define SOUND_JQ6500_ADKEY5_N 80

`defined @` MobaLedLib.h#829

These macros depend on me:

SOUND_JQ6500_ADKEY5_N | Sound_JQ6500_Seq5
_LocalVar_Sound_JQ6500 | Sound_JQ6500_Next_of_N_Reset | Sound_JQ6500_Next_of_N
Sound_JQ6500_PlayRandom

### SOUND_JQ6500_ADKEY6_BG [References: 0] Defined? True

#define SOUND_JQ6500_ADKEY6_BG 183

`defined @` MobaLedLib.h#839

These macros depend on me:

SOUND_JQ6500_ADKEY6_BG | Sound_JQ6500_BG_DecVol
Sound_JQ6500_BG_Prev

### SOUND_JQ6500_ADKEY6_N [References: 0] Defined? True

#define SOUND_JQ6500_ADKEY6_N 162

`defined @` MobaLedLib.h#830

These macros depend on me:

SOUND_JQ6500_ADKEY6_N | Sound_JQ6500_DecVol
Sound_JQ6500_Prev

### SOUND_JQ6500_ADKEY7_BG [References: 0] Defined? True

#define SOUND_JQ6500_ADKEY7_BG 238

`defined @` MobaLedLib.h#840

These macros depend on me:

SOUND_JQ6500_ADKEY7_BG | Sound_JQ6500_BG_IncVol
Sound_JQ6500_BG_Next

### SOUND_JQ6500_ADKEY7_N [References: 0] Defined? True

#define SOUND_JQ6500_ADKEY7_N 231

`defined @` MobaLedLib.h#831

These macros depend on me:

SOUND_JQ6500_ADKEY7_N | Sound_JQ6500_IncVol
Sound_JQ6500_Next

### SOUND_New_ADKEY1 [References: 0] Defined? True

#define SOUND_New_ADKEY1 255

`defined @` MobaLedLib.h#769

These macros depend on me:

SOUND_New_ADKEY1 | Sound_New_Seq1
Sound_New_Seq5
_LocalVar_New_Sound | Sound_New_Next_of_N_Reset | Sound_New_Next_of_N
Sound_New_PlayRandom

### SOUND_New_ADKEY10 [References: 0] Defined? True

#define SOUND_New_ADKEY10 11

`defined @` MobaLedLib.h#760

These macros depend on me:

SOUND_New_ADKEY10 | Sound_New_PlayMode
Sound_New_Seq14
_LocalVar_New_Sound | Sound_New_Next_of_N_Reset | Sound_New_Next_of_N
Sound_New_PlayRandom

### SOUND_New_ADKEY2 [References: 0] Defined? True

#define SOUND_New_ADKEY2 148

`defined @` MobaLedLib.h#768

These macros depend on me:

SOUND_New_ADKEY2 | Sound_New_Seq2
Sound_New_Seq6
_LocalVar_New_Sound | Sound_New_Next_of_N_Reset | Sound_New_Next_of_N
Sound_New_PlayRandom

### SOUND_New_ADKEY3 [References: 0] Defined? True

#define SOUND_New_ADKEY3 75

`defined @` MobaLedLib.h#767

These macros depend on me:

SOUND_New_ADKEY3 | Sound_New_Seq3
Sound_New_Seq7
_LocalVar_New_Sound | Sound_New_Next_of_N_Reset | Sound_New_Next_of_N
Sound_New_PlayRandom

### SOUND_New_ADKEY4 [References: 0] Defined? True

#define SOUND_New_ADKEY4 53

`defined @` MobaLedLib.h#766

These macros depend on me:

SOUND_New_ADKEY4 | Sound_New_Seq4
Sound_New_Seq8
_LocalVar_New_Sound | Sound_New_Next_of_N_Reset | Sound_New_Next_of_N
Sound_New_PlayRandom

### SOUND_New_ADKEY5 [References: 0] Defined? True

#define SOUND_New_ADKEY5 39

`defined @` MobaLedLib.h#765

These macros depend on me:

SOUND_New_ADKEY5 | Sound_New_DecVol
Sound_New_Prev
Sound_New_Seq9
_LocalVar_New_Sound | Sound_New_Next_of_N_Reset | Sound_New_Next_of_N
Sound_New_PlayRandom

### SOUND_New_ADKEY6 [References: 0] Defined? True

#define SOUND_New_ADKEY6 31

`defined @` MobaLedLib.h#764

These macros depend on me:

SOUND_New_ADKEY6 | Sound_New_IncVol
Sound_New_Next
Sound_New_Seq10
_LocalVar_New_Sound | Sound_New_Next_of_N_Reset | Sound_New_Next_of_N
Sound_New_PlayRandom

### SOUND_New_ADKEY7 [References: 0] Defined? True

#define SOUND_New_ADKEY7 27

`defined @` MobaLedLib.h#763

These macros depend on me:

SOUND_New_ADKEY7 | Sound_New_PausePlay
Sound_New_Seq11
_LocalVar_New_Sound | Sound_New_Next_of_N_Reset | Sound_New_Next_of_N
Sound_New_PlayRandom

### SOUND_New_ADKEY8 [References: 0] Defined? True

#define SOUND_New_ADKEY8 23

`defined @` MobaLedLib.h#762

These macros depend on me:

SOUND_New_ADKEY8 | Sound_New_Loop
Sound_New_Seq12
_LocalVar_New_Sound | Sound_New_Next_of_N_Reset | Sound_New_Next_of_N
Sound_New_PlayRandom

### SOUND_New_ADKEY9 [References: 0] Defined? True

#define SOUND_New_ADKEY9 18

`defined @` MobaLedLib.h#761

These macros depend on me:

SOUND_New_ADKEY9 | Sound_New_Seq13
Sound_New_USDSPI
_LocalVar_New_Sound | Sound_New_Next_of_N_Reset | Sound_New_Next_of_N
Sound_New_PlayRandom

### START_MSG [References: 0] Defined? True

#define START_MSG "LEDs_AutoProg Ver 3: AM328 3.3.2G 05.04.25 09:43"

`defined @` leds_autoprog.h#12

### START_SEND_INPUTS [References: 0] Defined? True

#define START_SEND_INPUTS 1

`defined @` leds_autoprog.h#69

### START_VARIABLES [References: 0] Defined? True

#define START_VARIABLES 1

`defined @` leds_autoprog.h#65

### Schedule [References: 0] Defined? True

#define Schedule(DstVar1,DstVarN,EnableCh,Start,End) SCHEDULE_T, DstVar1+RAM3, DstVarN, \
EnableCh, Start, End,

`defined @` MobaLedLib.h#130

I depend on these macros:

Schedule | RAM3 | RAM1
RAM2 | RAM1
SCHEDULE_T

### Servo2 [References: 0] Defined? True

#define Servo2(LED,InCh,Single_Cx,Servo1,Servo2,ServoT) InCh_to_TmpVar1(InCh, 2) \
PatternT1(LED,_Cx2StCh(Single_Cx)+28,SI_LocalVar,1,0,255,0,0,ServoT,0,Servo1,Servo2 \
,127,129,129)

`defined @` MobaLedLib.h#587

I depend on these macros:

Servo2 | InCh_to_TmpVar1 | INCH_TO_TMPVAR1_T
PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
_Cx2StCh

These macros depend on me:

Servo2 | Servo3 | Servo4 | Servo5
Servo5
Servo4 | Servo5
Servo5

### Servo3 [References: 0] Defined? True

#define Servo3(LED,InCh,Single_Cx,Servo1,Servo2,Servo3,ServoT) InCh_to_TmpVar1(InCh, 3) \
PatternT1(LED,_Cx2StCh(Single_Cx)+28,SI_LocalVar,1,0,255,0,0,ServoT,0,Servo1,Servo2,Servo3 \
,127,129,129,129)

`defined @` MobaLedLib.h#591

I depend on these macros:

Servo3 | InCh_to_TmpVar1 | INCH_TO_TMPVAR1_T
PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Servo2 | InCh_to_TmpVar1 | INCH_TO_TMPVAR1_T
PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
_Cx2StCh
_Cx2StCh

These macros depend on me:

Servo3 | Servo4 | Servo5
Servo5

### Servo4 [References: 0] Defined? True

#define Servo4(LED,InCh,Single_Cx,Servo1,Servo2,Servo3,Servo4,ServoT) InCh_to_TmpVar1(InCh, \
4) PatternT1(LED,_Cx2StCh(Single_Cx)+28,SI_LocalVar,1,0,255,0,0,ServoT,0,Servo1,Servo2,Servo3,Servo4 \
,127,129,129,129,129)

`defined @` MobaLedLib.h#595

I depend on these macros:

Servo4 | InCh_to_TmpVar1 | INCH_TO_TMPVAR1_T
PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Servo2 | InCh_to_TmpVar1 | INCH_TO_TMPVAR1_T
PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
_Cx2StCh
Servo3 | InCh_to_TmpVar1 | INCH_TO_TMPVAR1_T
PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Servo2 | InCh_to_TmpVar1 | INCH_TO_TMPVAR1_T
PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
_Cx2StCh
_Cx2StCh
_Cx2StCh

These macros depend on me:

Servo4 | Servo5

### Servo5 [References: 0] Defined? True

#define Servo5(LED,InCh,Single_Cx,Servo1,Servo2,Servo3,Servo4,Servo5,ServoT) InCh_to_TmpVar1(InCh, \
5) PatternT1(LED,_Cx2StCh(Single_Cx)+28,SI_LocalVar,1,0,255,0,0,10 \
Sec,0,Servo1,Servo2,Servo3,Servo4,Servo5 ,127,129,129,129,129,129)

`defined @` MobaLedLib.h#599

I depend on these macros:

Servo5 | InCh_to_TmpVar1 | INCH_TO_TMPVAR1_T
PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec
Servo2 | InCh_to_TmpVar1 | INCH_TO_TMPVAR1_T
PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
_Cx2StCh
Servo3 | InCh_to_TmpVar1 | INCH_TO_TMPVAR1_T
PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Servo2 | InCh_to_TmpVar1 | INCH_TO_TMPVAR1_T
PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
_Cx2StCh
_Cx2StCh
Servo4 | InCh_to_TmpVar1 | INCH_TO_TMPVAR1_T
PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Servo2 | InCh_to_TmpVar1 | INCH_TO_TMPVAR1_T
PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
_Cx2StCh
Servo3 | InCh_to_TmpVar1 | INCH_TO_TMPVAR1_T
PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Servo2 | InCh_to_TmpVar1 | INCH_TO_TMPVAR1_T
PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
_Cx2StCh
_Cx2StCh
_Cx2StCh
_Cx2StCh

These macros depend on me:

Servo5

### SingleLedSignal [References: 0] Defined? True

#define SingleLedSignal(LED,InCh,Single_Cx,FadeTime) InCh_to_LocalVar(InCh, 4) \
XPatternT1(LED,_Cx2StCh(Single_Cx)+64,SI_LocalVar,2,0,128,0,0,FadeTime,132,12 \
,0,63,128,63,128,63,191)

`defined @` MobaLedLib.h#340

I depend on these macros:

SingleLedSignal | SI_LocalVar | SI_0
XPatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
_Cx2StCh

### SingleLedSignalEx [References: 0] Defined? True

#define SingleLedSignalEx(LED,InCh,Single_Cx,FadeTime,State0_0,State0_1,State1_0,State1_1,State2_0,State2_1,State3_0,State3_1) \
InCh_to_LocalVar(InCh, 4) \
XPatternT1(LED,_Cx2StCh(Single_Cx)+28,SI_LocalVar,2,0,255,0,0,FadeTime,0,0,State0_0,State0_1,0,0,State1_0,State1_1,0,0,State2_0,Stat\
e2_1,0,0, State3_0,State3_1 ,0,63,128,63,128,63,128,63)

`defined @` MobaLedLib.h#342

I depend on these macros:

SingleLedSignalEx | SI_LocalVar | SI_0
XPatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
_Cx2StCh

### Sound_ADKey [References: 0] Defined? True

#define Sound_ADKey(LED,InCh,ADKey1,ADKey2) PatternTE2(LED,28,InCh,SI_Enable_Sound,2,0,255,0,PM_SEQUENZ_NO_RESTART,200 \
ms,10 ms,ADKey1,ADKey2,0,0)

`defined @` MobaLedLib.h#705

I depend on these macros:

Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

These macros depend on me:

Sound_ADKey | Sound_Loop
Sound_New_Loop
Sound_New_Next
Sound_New_PausePlay
Sound_New_PlayMode
Sound_New_Prev
Sound_New_Seq1
Sound_New_Seq10
Sound_New_Seq11
Sound_New_Seq12
Sound_New_Seq13
Sound_New_Seq14
Sound_New_Seq2
Sound_New_Seq3
Sound_New_Seq4
Sound_New_Seq5
Sound_New_Seq6
Sound_New_Seq7
Sound_New_Seq8
Sound_New_Seq9
Sound_New_USDSPI
Sound_Next
Sound_PausePlay
Sound_PlayMode
Sound_Prev
Sound_Seq1
Sound_Seq10
Sound_Seq11
Sound_Seq12
Sound_Seq13
Sound_Seq14
Sound_Seq2
Sound_Seq3
Sound_Seq4
Sound_Seq5
Sound_Seq6
Sound_Seq7
Sound_Seq8
Sound_Seq9
Sound_USDSPI

### Sound_ADKeyTime [References: 0] Defined? True

#define Sound_ADKeyTime(LED,InCh,ADKey1,ADKey2,Time) PatternT2( LED,28,InCh, \
2,0,255,0,PM_SEQUENZ_NO_RESTART,Time,10 ms,ADKey1,ADKey2,0,0)

`defined @` MobaLedLib.h#708

I depend on these macros:

Sound_ADKeyTime | PM_SEQUENZ_NO_RESTART
PatternT2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
ms

These macros depend on me:

Sound_ADKeyTime | Sound_DecVol
Sound_IncVol
Sound_New_DecVol
Sound_New_IncVol

### Sound_DecVol [References: 0] Defined? True

#define Sound_DecVol(LED,InCh,Steps) Sound_ADKeyTime(LED, InCh, SOUND_ADKEY5, 0, 850 ms - \
75 ms + (Steps-1) * 150 ms)

`defined @` MobaLedLib.h#721

I depend on these macros:

Sound_DecVol | SOUND_ADKEY5
Sound_ADKeyTime | PM_SEQUENZ_NO_RESTART
PatternT2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
ms
ms

### Sound_IncVol [References: 0] Defined? True

#define Sound_IncVol(LED,InCh,Steps) Sound_ADKeyTime(LED, InCh, SOUND_ADKEY6, 0, 850 ms - \
75 ms + (Steps-1) * 150 ms)

`defined @` MobaLedLib.h#722

I depend on these macros:

Sound_IncVol | SOUND_ADKEY6
Sound_ADKeyTime | PM_SEQUENZ_NO_RESTART
PatternT2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
ms
ms

### Sound_JQ6500_ADKey [References: 0] Defined? True

#define Sound_JQ6500_ADKey(LED,InCh,ADKey) PatternTE2(LED,28,InCh,SI_Enable_Sound,1,0,255,0,PM_SEQUENZ_NO_RESTART,400 \
ms,10 ms,ADKey,0)

`defined @` MobaLedLib.h#819

I depend on these macros:

Sound_JQ6500_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

These macros depend on me:

Sound_JQ6500_ADKey | Sound_JQ6500_BG_Next
Sound_JQ6500_BG_Prev
Sound_JQ6500_BG_Seq1
Sound_JQ6500_BG_Seq2
Sound_JQ6500_BG_Seq3
Sound_JQ6500_BG_Seq4
Sound_JQ6500_BG_Seq5
Sound_JQ6500_Next
Sound_JQ6500_Prev
Sound_JQ6500_Seq1
Sound_JQ6500_Seq2
Sound_JQ6500_Seq3
Sound_JQ6500_Seq4
Sound_JQ6500_Seq5

### Sound_JQ6500_ADKeyTime [References: 0] Defined? True

#define Sound_JQ6500_ADKeyTime(LED,InCh,ADKey,Time) PatternT2( LED,28,InCh, \
1,0,255,0,PM_SEQUENZ_NO_RESTART,Time,10 ms,ADKey,0)

`defined @` MobaLedLib.h#822

I depend on these macros:

Sound_JQ6500_ADKeyTime | PM_SEQUENZ_NO_RESTART
PatternT2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
ms

These macros depend on me:

Sound_JQ6500_ADKeyTime | Sound_JQ6500_BG_DecVol
Sound_JQ6500_BG_IncVol
Sound_JQ6500_DecVol
Sound_JQ6500_IncVol

### Sound_JQ6500_BG_DecVol [References: 0] Defined? True

#define Sound_JQ6500_BG_DecVol(LED,InCh,Steps) Sound_JQ6500_ADKeyTime(LED, InCh, \
SOUND_JQ6500_ADKEY6_BG, 1000 ms + (Steps-1) * 150 ms)

`defined @` MobaLedLib.h#857

I depend on these macros:

Sound_JQ6500_BG_DecVol | SOUND_JQ6500_ADKEY6_BG
Sound_JQ6500_ADKeyTime | PM_SEQUENZ_NO_RESTART
PatternT2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
ms
ms

### Sound_JQ6500_BG_IncVol [References: 0] Defined? True

#define Sound_JQ6500_BG_IncVol(LED,InCh,Steps) Sound_JQ6500_ADKeyTime(LED, InCh, \
SOUND_JQ6500_ADKEY7_BG, 1000 ms + (Steps-1) * 150 ms)

`defined @` MobaLedLib.h#858

I depend on these macros:

Sound_JQ6500_BG_IncVol | SOUND_JQ6500_ADKEY7_BG
Sound_JQ6500_ADKeyTime | PM_SEQUENZ_NO_RESTART
PatternT2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
ms
ms

### Sound_JQ6500_BG_Next [References: 0] Defined? True

#define Sound_JQ6500_BG_Next(LED,InCh) Sound_JQ6500_ADKey( LED, InCh, SOUND_JQ6500_ADKEY7_BG) \

`defined @` MobaLedLib.h#847

I depend on these macros:

Sound_JQ6500_BG_Next | SOUND_JQ6500_ADKEY7_BG
Sound_JQ6500_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_JQ6500_BG_Next_of_N [References: 0] Defined? True

#define Sound_JQ6500_BG_Next_of_N(LED,InCh,MaxSoundNr) Sound_JQ6500_BG_Next_of_N_Reset(LED, \
InCh, SI_0, MaxSoundNr)

`defined @` MobaLedLib.h#901

I depend on these macros:

Sound_JQ6500_BG_Next_of_N | SI_0
Sound_JQ6500_BG_Next_of_N_Reset | CF_INV_ENABLE
CF_ONLY_LOCALVAR | CF_LOCAL_VAR
_CF_NO_LEDOUTP
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
New_Local_Var | NEW_LOCAL_VAR_T
RAM2 | RAM1
Sec
_LocalVar_Sound_JQ6500_BG | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
SOUND_JQ6500_ADKEY1_BG
SOUND_JQ6500_ADKEY2_BG
SOUND_JQ6500_ADKEY3_BG
SOUND_JQ6500_ADKEY4_BG
SOUND_JQ6500_ADKEY5_BG
ms

### Sound_JQ6500_BG_Next_of_N_Reset [References: 0] Defined? True

#define Sound_JQ6500_BG_Next_of_N_Reset(LED,InCh,InReset,MaxSoundNr) New_Local_Var() \
Counter(CF_ONLY_LOCALVAR | CF_ROTATE | CF_SKIP0 | CF_INV_ENABLE, InCh, InReset, 0 \
Sec, MaxSoundNr+1) _LocalVar_Sound_JQ6500_BG(LED)

`defined @` MobaLedLib.h#896

I depend on these macros:

Sound_JQ6500_BG_Next_of_N_Reset | CF_INV_ENABLE
CF_ONLY_LOCALVAR | CF_LOCAL_VAR
_CF_NO_LEDOUTP
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
New_Local_Var | NEW_LOCAL_VAR_T
RAM2 | RAM1
Sec
_LocalVar_Sound_JQ6500_BG | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
SOUND_JQ6500_ADKEY1_BG
SOUND_JQ6500_ADKEY2_BG
SOUND_JQ6500_ADKEY3_BG
SOUND_JQ6500_ADKEY4_BG
SOUND_JQ6500_ADKEY5_BG
ms

These macros depend on me:

Sound_JQ6500_BG_Next_of_N_Reset | Sound_JQ6500_BG_Next_of_N

### Sound_JQ6500_BG_PlayRandom [References: 0] Defined? True

#define Sound_JQ6500_BG_PlayRandom(LED,InCh,MaxSoundNr) New_Local_Var() Counter(CF_ONLY_LOCALVAR \
| CF_RANDOM | CF_SKIP0, InCh, SI_1, 0 Sec, MaxSoundNr+1) _LocalVar_Sound_JQ6500_BG(LED) \

`defined @` MobaLedLib.h#891

I depend on these macros:

Sound_JQ6500_BG_PlayRandom | CF_ONLY_LOCALVAR | CF_LOCAL_VAR
_CF_NO_LEDOUTP
CF_RANDOM
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
New_Local_Var | NEW_LOCAL_VAR_T
RAM2 | RAM1
SI_1
Sec
_LocalVar_Sound_JQ6500_BG | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
SOUND_JQ6500_ADKEY1_BG
SOUND_JQ6500_ADKEY2_BG
SOUND_JQ6500_ADKEY3_BG
SOUND_JQ6500_ADKEY4_BG
SOUND_JQ6500_ADKEY5_BG
ms

### Sound_JQ6500_BG_Prev [References: 0] Defined? True

#define Sound_JQ6500_BG_Prev(LED,InCh) Sound_JQ6500_ADKey( LED, InCh, SOUND_JQ6500_ADKEY6_BG) \

`defined @` MobaLedLib.h#846

I depend on these macros:

Sound_JQ6500_BG_Prev | SOUND_JQ6500_ADKEY6_BG
Sound_JQ6500_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_JQ6500_BG_Seq1 [References: 0] Defined? True

#define Sound_JQ6500_BG_Seq1(LED,InCh) Sound_JQ6500_ADKey(LED, InCh, SOUND_JQ6500_ADKEY1_BG) \

`defined @` MobaLedLib.h#867

I depend on these macros:

Sound_JQ6500_BG_Seq1 | SOUND_JQ6500_ADKEY1_BG
Sound_JQ6500_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_JQ6500_BG_Seq2 [References: 0] Defined? True

#define Sound_JQ6500_BG_Seq2(LED,InCh) Sound_JQ6500_ADKey(LED, InCh, SOUND_JQ6500_ADKEY2_BG) \

`defined @` MobaLedLib.h#868

I depend on these macros:

Sound_JQ6500_BG_Seq2 | SOUND_JQ6500_ADKEY2_BG
Sound_JQ6500_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_JQ6500_BG_Seq3 [References: 0] Defined? True

#define Sound_JQ6500_BG_Seq3(LED,InCh) Sound_JQ6500_ADKey(LED, InCh, SOUND_JQ6500_ADKEY3_BG) \

`defined @` MobaLedLib.h#869

I depend on these macros:

Sound_JQ6500_BG_Seq3 | SOUND_JQ6500_ADKEY3_BG
Sound_JQ6500_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_JQ6500_BG_Seq4 [References: 0] Defined? True

#define Sound_JQ6500_BG_Seq4(LED,InCh) Sound_JQ6500_ADKey(LED, InCh, SOUND_JQ6500_ADKEY4_BG) \

`defined @` MobaLedLib.h#870

I depend on these macros:

Sound_JQ6500_BG_Seq4 | SOUND_JQ6500_ADKEY4_BG
Sound_JQ6500_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_JQ6500_BG_Seq5 [References: 0] Defined? True

#define Sound_JQ6500_BG_Seq5(LED,InCh) Sound_JQ6500_ADKey(LED, InCh, SOUND_JQ6500_ADKEY5_BG) \

`defined @` MobaLedLib.h#871

I depend on these macros:

Sound_JQ6500_BG_Seq5 | SOUND_JQ6500_ADKEY5_BG
Sound_JQ6500_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_JQ6500_DecVol [References: 0] Defined? True

#define Sound_JQ6500_DecVol(LED,InCh,Steps) Sound_JQ6500_ADKeyTime(LED, InCh, \
SOUND_JQ6500_ADKEY6_N, 1000 ms + (Steps-1) * 150 ms)

`defined @` MobaLedLib.h#854

I depend on these macros:

Sound_JQ6500_DecVol | SOUND_JQ6500_ADKEY6_N
Sound_JQ6500_ADKeyTime | PM_SEQUENZ_NO_RESTART
PatternT2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
ms
ms

### Sound_JQ6500_IncVol [References: 0] Defined? True

#define Sound_JQ6500_IncVol(LED,InCh,Steps) Sound_JQ6500_ADKeyTime(LED, InCh, \
SOUND_JQ6500_ADKEY7_N, 1000 ms + (Steps-1) * 150 ms)

`defined @` MobaLedLib.h#855

I depend on these macros:

Sound_JQ6500_IncVol | SOUND_JQ6500_ADKEY7_N
Sound_JQ6500_ADKeyTime | PM_SEQUENZ_NO_RESTART
PatternT2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
ms
ms

### Sound_JQ6500_Next [References: 0] Defined? True

#define Sound_JQ6500_Next(LED,InCh) Sound_JQ6500_ADKey( LED, InCh, SOUND_JQ6500_ADKEY7_N) \

`defined @` MobaLedLib.h#844

I depend on these macros:

Sound_JQ6500_Next | SOUND_JQ6500_ADKEY7_N
Sound_JQ6500_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_JQ6500_Next_of_N [References: 0] Defined? True

#define Sound_JQ6500_Next_of_N(LED,InCh,MaxSoundNr) Sound_JQ6500_Next_of_N_Reset(LED, InCh, \
SI_0, MaxSoundNr)

`defined @` MobaLedLib.h#887

I depend on these macros:

Sound_JQ6500_Next_of_N | SI_0
Sound_JQ6500_Next_of_N_Reset | CF_INV_ENABLE
CF_ONLY_LOCALVAR | CF_LOCAL_VAR
_CF_NO_LEDOUTP
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
New_Local_Var | NEW_LOCAL_VAR_T
RAM2 | RAM1
Sec
_LocalVar_Sound_JQ6500 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
SOUND_JQ6500_ADKEY1_N
SOUND_JQ6500_ADKEY2_N
SOUND_JQ6500_ADKEY3_N
SOUND_JQ6500_ADKEY4_N
SOUND_JQ6500_ADKEY5_N
ms

### Sound_JQ6500_Next_of_N_Reset [References: 0] Defined? True

#define Sound_JQ6500_Next_of_N_Reset(LED,InCh,InReset,MaxSoundNr) New_Local_Var() \
Counter(CF_ONLY_LOCALVAR | CF_ROTATE | CF_SKIP0 | CF_INV_ENABLE, InCh, InReset, 0 \
Sec, MaxSoundNr+1) _LocalVar_Sound_JQ6500(LED)

`defined @` MobaLedLib.h#882

I depend on these macros:

Sound_JQ6500_Next_of_N_Reset | CF_INV_ENABLE
CF_ONLY_LOCALVAR | CF_LOCAL_VAR
_CF_NO_LEDOUTP
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
New_Local_Var | NEW_LOCAL_VAR_T
RAM2 | RAM1
Sec
_LocalVar_Sound_JQ6500 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
SOUND_JQ6500_ADKEY1_N
SOUND_JQ6500_ADKEY2_N
SOUND_JQ6500_ADKEY3_N
SOUND_JQ6500_ADKEY4_N
SOUND_JQ6500_ADKEY5_N
ms

These macros depend on me:

Sound_JQ6500_Next_of_N_Reset | Sound_JQ6500_Next_of_N

### Sound_JQ6500_PlayRandom [References: 0] Defined? True

#define Sound_JQ6500_PlayRandom(LED,InCh,MaxSoundNr) New_Local_Var() Counter(CF_ONLY_LOCALVAR \
| CF_RANDOM | CF_SKIP0, InCh, SI_1, 0 Sec, MaxSoundNr+1) _LocalVar_Sound_JQ6500(LED) \

`defined @` MobaLedLib.h#877

I depend on these macros:

Sound_JQ6500_PlayRandom | CF_ONLY_LOCALVAR | CF_LOCAL_VAR
_CF_NO_LEDOUTP
CF_RANDOM
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
New_Local_Var | NEW_LOCAL_VAR_T
RAM2 | RAM1
SI_1
Sec
_LocalVar_Sound_JQ6500 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
SOUND_JQ6500_ADKEY1_N
SOUND_JQ6500_ADKEY2_N
SOUND_JQ6500_ADKEY3_N
SOUND_JQ6500_ADKEY4_N
SOUND_JQ6500_ADKEY5_N
ms

### Sound_JQ6500_Prev [References: 0] Defined? True

#define Sound_JQ6500_Prev(LED,InCh) Sound_JQ6500_ADKey( LED, InCh, SOUND_JQ6500_ADKEY6_N) \

`defined @` MobaLedLib.h#843

I depend on these macros:

Sound_JQ6500_Prev | SOUND_JQ6500_ADKEY6_N
Sound_JQ6500_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_JQ6500_Seq1 [References: 0] Defined? True

#define Sound_JQ6500_Seq1(LED,InCh) Sound_JQ6500_ADKey(LED, InCh, SOUND_JQ6500_ADKEY1_N)

`defined @` MobaLedLib.h#861

I depend on these macros:

Sound_JQ6500_Seq1 | SOUND_JQ6500_ADKEY1_N
Sound_JQ6500_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_JQ6500_Seq2 [References: 0] Defined? True

#define Sound_JQ6500_Seq2(LED,InCh) Sound_JQ6500_ADKey(LED, InCh, SOUND_JQ6500_ADKEY2_N)

`defined @` MobaLedLib.h#862

I depend on these macros:

Sound_JQ6500_Seq2 | SOUND_JQ6500_ADKEY2_N
Sound_JQ6500_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_JQ6500_Seq3 [References: 0] Defined? True

#define Sound_JQ6500_Seq3(LED,InCh) Sound_JQ6500_ADKey(LED, InCh, SOUND_JQ6500_ADKEY3_N)

`defined @` MobaLedLib.h#863

I depend on these macros:

Sound_JQ6500_Seq3 | SOUND_JQ6500_ADKEY3_N
Sound_JQ6500_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_JQ6500_Seq4 [References: 0] Defined? True

#define Sound_JQ6500_Seq4(LED,InCh) Sound_JQ6500_ADKey(LED, InCh, SOUND_JQ6500_ADKEY4_N)

`defined @` MobaLedLib.h#864

I depend on these macros:

Sound_JQ6500_Seq4 | SOUND_JQ6500_ADKEY4_N
Sound_JQ6500_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_JQ6500_Seq5 [References: 0] Defined? True

#define Sound_JQ6500_Seq5(LED,InCh) Sound_JQ6500_ADKey(LED, InCh, SOUND_JQ6500_ADKEY5_N)

`defined @` MobaLedLib.h#865

I depend on these macros:

Sound_JQ6500_Seq5 | SOUND_JQ6500_ADKEY5_N
Sound_JQ6500_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_Loop [References: 0] Defined? True

#define Sound_Loop(LED,InCh) Sound_ADKey(LED, InCh, SOUND_ADKEY8, 0)

`defined @` MobaLedLib.h#713

I depend on these macros:

Sound_Loop | SOUND_ADKEY8
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_New_DecVol [References: 0] Defined? True

#define Sound_New_DecVol(LED,InCh,Steps) Sound_ADKeyTime(LED, InCh, SOUND_New_ADKEY5, 0, \
950 ms - 75 ms + (Steps-1) * 150 ms)

`defined @` MobaLedLib.h#782

I depend on these macros:

Sound_New_DecVol | SOUND_New_ADKEY5
Sound_ADKeyTime | PM_SEQUENZ_NO_RESTART
PatternT2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
ms
ms

### Sound_New_IncVol [References: 0] Defined? True

#define Sound_New_IncVol(LED,InCh,Steps) Sound_ADKeyTime(LED, InCh, SOUND_New_ADKEY6, 0, \
950 ms - 75 ms + (Steps-1) * 150 ms)

`defined @` MobaLedLib.h#783

I depend on these macros:

Sound_New_IncVol | SOUND_New_ADKEY6
Sound_ADKeyTime | PM_SEQUENZ_NO_RESTART
PatternT2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
ms
ms

### Sound_New_Loop [References: 0] Defined? True

#define Sound_New_Loop(LED,InCh) Sound_ADKey(LED, InCh, SOUND_New_ADKEY8, 0)

`defined @` MobaLedLib.h#774

I depend on these macros:

Sound_New_Loop | SOUND_New_ADKEY8
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_New_Next [References: 0] Defined? True

#define Sound_New_Next(LED,InCh) Sound_ADKey(LED, InCh, SOUND_New_ADKEY6, 0)

`defined @` MobaLedLib.h#772

I depend on these macros:

Sound_New_Next | SOUND_New_ADKEY6
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_New_Next_of_N [References: 0] Defined? True

#define Sound_New_Next_of_N(LED,InCh,MaxSoundNr) Sound_New_Next_of_N_Reset(LED, InCh, SI_0, \
MaxSoundNr)

`defined @` MobaLedLib.h#812

I depend on these macros:

Sound_New_Next_of_N | SI_0
Sound_New_Next_of_N_Reset | CF_INV_ENABLE
CF_ONLY_LOCALVAR | CF_LOCAL_VAR
_CF_NO_LEDOUTP
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
New_Local_Var | NEW_LOCAL_VAR_T
RAM2 | RAM1
Sec
_LocalVar_New_Sound | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
SOUND_New_ADKEY1
SOUND_New_ADKEY10
SOUND_New_ADKEY2
SOUND_New_ADKEY3
SOUND_New_ADKEY4
SOUND_New_ADKEY5
SOUND_New_ADKEY6
SOUND_New_ADKEY7
SOUND_New_ADKEY8
SOUND_New_ADKEY9
ms

### Sound_New_Next_of_N_Reset [References: 0] Defined? True

#define Sound_New_Next_of_N_Reset(LED,InCh,InReset,MaxSoundNr) New_Local_Var() \
Counter(CF_ONLY_LOCALVAR | CF_ROTATE | CF_SKIP0 | CF_INV_ENABLE, InCh, InReset, 0 \
Sec, MaxSoundNr+1) _LocalVar_New_Sound(LED)

`defined @` MobaLedLib.h#807

I depend on these macros:

Sound_New_Next_of_N_Reset | CF_INV_ENABLE
CF_ONLY_LOCALVAR | CF_LOCAL_VAR
_CF_NO_LEDOUTP
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
New_Local_Var | NEW_LOCAL_VAR_T
RAM2 | RAM1
Sec
_LocalVar_New_Sound | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
SOUND_New_ADKEY1
SOUND_New_ADKEY10
SOUND_New_ADKEY2
SOUND_New_ADKEY3
SOUND_New_ADKEY4
SOUND_New_ADKEY5
SOUND_New_ADKEY6
SOUND_New_ADKEY7
SOUND_New_ADKEY8
SOUND_New_ADKEY9
ms

These macros depend on me:

Sound_New_Next_of_N_Reset | Sound_New_Next_of_N

### Sound_New_PausePlay [References: 0] Defined? True

#define Sound_New_PausePlay(LED,InCh) Sound_ADKey(LED, InCh, SOUND_New_ADKEY7, 0)

`defined @` MobaLedLib.h#773

I depend on these macros:

Sound_New_PausePlay | SOUND_New_ADKEY7
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_New_PlayMode [References: 0] Defined? True

#define Sound_New_PlayMode(LED,InCh) Sound_ADKey(LED, InCh, SOUND_New_ADKEY10, 0)

`defined @` MobaLedLib.h#776

I depend on these macros:

Sound_New_PlayMode | SOUND_New_ADKEY10
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_New_PlayRandom [References: 0] Defined? True

#define Sound_New_PlayRandom(LED,InCh,MaxSoundNr) New_Local_Var() Counter(CF_ONLY_LOCALVAR \
| CF_RANDOM | CF_SKIP0, InCh, SI_1, 0 Sec, MaxSoundNr+1) _LocalVar_New_Sound(LED) \

`defined @` MobaLedLib.h#802

I depend on these macros:

Sound_New_PlayRandom | CF_ONLY_LOCALVAR | CF_LOCAL_VAR
_CF_NO_LEDOUTP
CF_RANDOM
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
New_Local_Var | NEW_LOCAL_VAR_T
RAM2 | RAM1
SI_1
Sec
_LocalVar_New_Sound | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
SOUND_New_ADKEY1
SOUND_New_ADKEY10
SOUND_New_ADKEY2
SOUND_New_ADKEY3
SOUND_New_ADKEY4
SOUND_New_ADKEY5
SOUND_New_ADKEY6
SOUND_New_ADKEY7
SOUND_New_ADKEY8
SOUND_New_ADKEY9
ms

### Sound_New_Prev [References: 0] Defined? True

#define Sound_New_Prev(LED,InCh) Sound_ADKey(LED, InCh, SOUND_New_ADKEY5, 0)

`defined @` MobaLedLib.h#771

I depend on these macros:

Sound_New_Prev | SOUND_New_ADKEY5
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_New_Seq1 [References: 0] Defined? True

#define Sound_New_Seq1(LED,InCh) Sound_ADKey(LED, InCh, SOUND_New_ADKEY1, 0)

`defined @` MobaLedLib.h#785

I depend on these macros:

Sound_New_Seq1 | SOUND_New_ADKEY1
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_New_Seq10 [References: 0] Defined? True

#define Sound_New_Seq10(LED,InCh) Sound_ADKey(LED, InCh, 0, SOUND_New_ADKEY6)

`defined @` MobaLedLib.h#794

I depend on these macros:

Sound_New_Seq10 | SOUND_New_ADKEY6
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_New_Seq11 [References: 0] Defined? True

#define Sound_New_Seq11(LED,InCh) Sound_ADKey(LED, InCh, 0, SOUND_New_ADKEY7)

`defined @` MobaLedLib.h#795

I depend on these macros:

Sound_New_Seq11 | SOUND_New_ADKEY7
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_New_Seq12 [References: 0] Defined? True

#define Sound_New_Seq12(LED,InCh) Sound_ADKey(LED, InCh, 0, SOUND_New_ADKEY8)

`defined @` MobaLedLib.h#796

I depend on these macros:

Sound_New_Seq12 | SOUND_New_ADKEY8
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_New_Seq13 [References: 0] Defined? True

#define Sound_New_Seq13(LED,InCh) Sound_ADKey(LED, InCh, 0, SOUND_New_ADKEY9)

`defined @` MobaLedLib.h#797

I depend on these macros:

Sound_New_Seq13 | SOUND_New_ADKEY9
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_New_Seq14 [References: 0] Defined? True

#define Sound_New_Seq14(LED,InCh) Sound_ADKey(LED, InCh, 0, SOUND_New_ADKEY10)

`defined @` MobaLedLib.h#798

I depend on these macros:

Sound_New_Seq14 | SOUND_New_ADKEY10
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_New_Seq2 [References: 0] Defined? True

#define Sound_New_Seq2(LED,InCh) Sound_ADKey(LED, InCh, SOUND_New_ADKEY2, 0)

`defined @` MobaLedLib.h#786

I depend on these macros:

Sound_New_Seq2 | SOUND_New_ADKEY2
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_New_Seq3 [References: 0] Defined? True

#define Sound_New_Seq3(LED,InCh) Sound_ADKey(LED, InCh, SOUND_New_ADKEY3, 0)

`defined @` MobaLedLib.h#787

I depend on these macros:

Sound_New_Seq3 | SOUND_New_ADKEY3
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_New_Seq4 [References: 0] Defined? True

#define Sound_New_Seq4(LED,InCh) Sound_ADKey(LED, InCh, SOUND_New_ADKEY4, 0)

`defined @` MobaLedLib.h#788

I depend on these macros:

Sound_New_Seq4 | SOUND_New_ADKEY4
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_New_Seq5 [References: 0] Defined? True

#define Sound_New_Seq5(LED,InCh) Sound_ADKey(LED, InCh, 0, SOUND_New_ADKEY1)

`defined @` MobaLedLib.h#789

I depend on these macros:

Sound_New_Seq5 | SOUND_New_ADKEY1
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_New_Seq6 [References: 0] Defined? True

#define Sound_New_Seq6(LED,InCh) Sound_ADKey(LED, InCh, 0, SOUND_New_ADKEY2)

`defined @` MobaLedLib.h#790

I depend on these macros:

Sound_New_Seq6 | SOUND_New_ADKEY2
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_New_Seq7 [References: 0] Defined? True

#define Sound_New_Seq7(LED,InCh) Sound_ADKey(LED, InCh, 0, SOUND_New_ADKEY3)

`defined @` MobaLedLib.h#791

I depend on these macros:

Sound_New_Seq7 | SOUND_New_ADKEY3
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_New_Seq8 [References: 0] Defined? True

#define Sound_New_Seq8(LED,InCh) Sound_ADKey(LED, InCh, 0, SOUND_New_ADKEY4)

`defined @` MobaLedLib.h#792

I depend on these macros:

Sound_New_Seq8 | SOUND_New_ADKEY4
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_New_Seq9 [References: 0] Defined? True

#define Sound_New_Seq9(LED,InCh) Sound_ADKey(LED, InCh, 0, SOUND_New_ADKEY5)

`defined @` MobaLedLib.h#793

I depend on these macros:

Sound_New_Seq9 | SOUND_New_ADKEY5
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_New_USDSPI [References: 0] Defined? True

#define Sound_New_USDSPI(LED,InCh) Sound_ADKey(LED, InCh, SOUND_New_ADKEY9, 0)

`defined @` MobaLedLib.h#775

I depend on these macros:

Sound_New_USDSPI | SOUND_New_ADKEY9
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_Next [References: 0] Defined? True

#define Sound_Next(LED,InCh) Sound_ADKey(LED, InCh, SOUND_ADKEY6, 0)

`defined @` MobaLedLib.h#711

I depend on these macros:

Sound_Next | SOUND_ADKEY6
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_Next_of_N [References: 0] Defined? True

#define Sound_Next_of_N(LED,InCh,MaxSoundNr) Sound_Next_of_N_Reset(LED, InCh, SI_0, \
MaxSoundNr)

`defined @` MobaLedLib.h#751

I depend on these macros:

Sound_Next_of_N | SI_0
Sound_Next_of_N_Reset | CF_INV_ENABLE
CF_ONLY_LOCALVAR | CF_LOCAL_VAR
_CF_NO_LEDOUTP
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
New_Local_Var | NEW_LOCAL_VAR_T
RAM2 | RAM1
Sec
_LocalVar_Sound | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
SOUND_ADKEY1
SOUND_ADKEY10
SOUND_ADKEY2
SOUND_ADKEY3
SOUND_ADKEY4
SOUND_ADKEY5
SOUND_ADKEY6
SOUND_ADKEY7
SOUND_ADKEY8
SOUND_ADKEY9
ms

### Sound_Next_of_N_Reset [References: 0] Defined? True

#define Sound_Next_of_N_Reset(LED,InCh,InReset,MaxSoundNr) New_Local_Var() Counter(CF_ONLY_LOCALVAR \
| CF_ROTATE | CF_SKIP0 | CF_INV_ENABLE, InCh, InReset, 0 Sec, MaxSoundNr+1) \
_LocalVar_Sound(LED)

`defined @` MobaLedLib.h#746

I depend on these macros:

Sound_Next_of_N_Reset | CF_INV_ENABLE
CF_ONLY_LOCALVAR | CF_LOCAL_VAR
_CF_NO_LEDOUTP
CF_ROTATE
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
New_Local_Var | NEW_LOCAL_VAR_T
RAM2 | RAM1
Sec
_LocalVar_Sound | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
SOUND_ADKEY1
SOUND_ADKEY10
SOUND_ADKEY2
SOUND_ADKEY3
SOUND_ADKEY4
SOUND_ADKEY5
SOUND_ADKEY6
SOUND_ADKEY7
SOUND_ADKEY8
SOUND_ADKEY9
ms

These macros depend on me:

Sound_Next_of_N_Reset | Sound_Next_of_N

### Sound_PausePlay [References: 0] Defined? True

#define Sound_PausePlay(LED,InCh) Sound_ADKey(LED, InCh, SOUND_ADKEY7, 0)

`defined @` MobaLedLib.h#712

I depend on these macros:

Sound_PausePlay | SOUND_ADKEY7
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_PlayMode [References: 0] Defined? True

#define Sound_PlayMode(LED,InCh) Sound_ADKey(LED, InCh, SOUND_ADKEY10, 0)

`defined @` MobaLedLib.h#715

I depend on these macros:

Sound_PlayMode | SOUND_ADKEY10
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_PlayRandom [References: 0] Defined? True

#define Sound_PlayRandom(LED,InCh,MaxSoundNr) New_Local_Var() Counter(CF_ONLY_LOCALVAR | \
CF_RANDOM | CF_SKIP0, InCh, SI_1, 0 Sec, MaxSoundNr+1) _LocalVar_Sound(LED)

`defined @` MobaLedLib.h#741

I depend on these macros:

Sound_PlayRandom | CF_ONLY_LOCALVAR | CF_LOCAL_VAR
_CF_NO_LEDOUTP
CF_RANDOM
CF_SKIP0
Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
New_Local_Var | NEW_LOCAL_VAR_T
RAM2 | RAM1
SI_1
Sec
_LocalVar_Sound | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
SOUND_ADKEY1
SOUND_ADKEY10
SOUND_ADKEY2
SOUND_ADKEY3
SOUND_ADKEY4
SOUND_ADKEY5
SOUND_ADKEY6
SOUND_ADKEY7
SOUND_ADKEY8
SOUND_ADKEY9
ms

### Sound_Prev [References: 0] Defined? True

#define Sound_Prev(LED,InCh) Sound_ADKey(LED, InCh, SOUND_ADKEY5, 0)

`defined @` MobaLedLib.h#710

I depend on these macros:

Sound_Prev | SOUND_ADKEY5
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_Seq1 [References: 0] Defined? True

#define Sound_Seq1(LED,InCh) Sound_ADKey(LED, InCh, SOUND_ADKEY1, 0)

`defined @` MobaLedLib.h#724

I depend on these macros:

Sound_Seq1 | SOUND_ADKEY1
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_Seq10 [References: 0] Defined? True

#define Sound_Seq10(LED,InCh) Sound_ADKey(LED, InCh, 0, SOUND_ADKEY6)

`defined @` MobaLedLib.h#733

I depend on these macros:

Sound_Seq10 | SOUND_ADKEY6
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_Seq11 [References: 0] Defined? True

#define Sound_Seq11(LED,InCh) Sound_ADKey(LED, InCh, 0, SOUND_ADKEY7)

`defined @` MobaLedLib.h#734

I depend on these macros:

Sound_Seq11 | SOUND_ADKEY7
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_Seq12 [References: 0] Defined? True

#define Sound_Seq12(LED,InCh) Sound_ADKey(LED, InCh, 0, SOUND_ADKEY8)

`defined @` MobaLedLib.h#735

I depend on these macros:

Sound_Seq12 | SOUND_ADKEY8
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_Seq13 [References: 0] Defined? True

#define Sound_Seq13(LED,InCh) Sound_ADKey(LED, InCh, 0, SOUND_ADKEY9)

`defined @` MobaLedLib.h#736

I depend on these macros:

Sound_Seq13 | SOUND_ADKEY9
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_Seq14 [References: 0] Defined? True

#define Sound_Seq14(LED,InCh) Sound_ADKey(LED, InCh, 0, SOUND_ADKEY10)

`defined @` MobaLedLib.h#737

I depend on these macros:

Sound_Seq14 | SOUND_ADKEY10
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_Seq2 [References: 0] Defined? True

#define Sound_Seq2(LED,InCh) Sound_ADKey(LED, InCh, SOUND_ADKEY2, 0)

`defined @` MobaLedLib.h#725

I depend on these macros:

Sound_Seq2 | SOUND_ADKEY2
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_Seq3 [References: 0] Defined? True

#define Sound_Seq3(LED,InCh) Sound_ADKey(LED, InCh, SOUND_ADKEY3, 0)

`defined @` MobaLedLib.h#726

I depend on these macros:

Sound_Seq3 | SOUND_ADKEY3
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_Seq4 [References: 0] Defined? True

#define Sound_Seq4(LED,InCh) Sound_ADKey(LED, InCh, SOUND_ADKEY4, 0)

`defined @` MobaLedLib.h#727

I depend on these macros:

Sound_Seq4 | SOUND_ADKEY4
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_Seq5 [References: 0] Defined? True

#define Sound_Seq5(LED,InCh) Sound_ADKey(LED, InCh, 0, SOUND_ADKEY1)

`defined @` MobaLedLib.h#728

I depend on these macros:

Sound_Seq5 | SOUND_ADKEY1
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_Seq6 [References: 0] Defined? True

#define Sound_Seq6(LED,InCh) Sound_ADKey(LED, InCh, 0, SOUND_ADKEY2)

`defined @` MobaLedLib.h#729

I depend on these macros:

Sound_Seq6 | SOUND_ADKEY2
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_Seq7 [References: 0] Defined? True

#define Sound_Seq7(LED,InCh) Sound_ADKey(LED, InCh, 0, SOUND_ADKEY3)

`defined @` MobaLedLib.h#730

I depend on these macros:

Sound_Seq7 | SOUND_ADKEY3
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_Seq8 [References: 0] Defined? True

#define Sound_Seq8(LED,InCh) Sound_ADKey(LED, InCh, 0, SOUND_ADKEY4)

`defined @` MobaLedLib.h#731

I depend on these macros:

Sound_Seq8 | SOUND_ADKEY4
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_Seq9 [References: 0] Defined? True

#define Sound_Seq9(LED,InCh) Sound_ADKey(LED, InCh, 0, SOUND_ADKEY5)

`defined @` MobaLedLib.h#732

I depend on these macros:

Sound_Seq9 | SOUND_ADKEY5
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Sound_USDSPI [References: 0] Defined? True

#define Sound_USDSPI(LED,InCh) Sound_ADKey(LED, InCh, SOUND_ADKEY9, 0)

`defined @` MobaLedLib.h#714

I depend on these macros:

Sound_USDSPI | SOUND_ADKEY9
Sound_ADKey | PM_SEQUENZ_NO_RESTART
PatternTE2 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT2_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_Enable_Sound
ms

### Status_ButtonBL_0_1 [References: 0] Defined? True

#define Status_ButtonBL_0_1(LED,B_LED_Cx,Val1,BackLight) PatternT1(LED,28 \
+_Cx2StCh(B_LED_Cx),SI_LocalVar,1,0,255,0,0,0.4 Sec,BackLight,Val1,0,0,0 ,63,192,0,0,1) \

`defined @` MobaLedLib.h#420

I depend on these macros:

Status_ButtonBL_0_1 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec
_Cx2StCh

These macros depend on me:

Status_ButtonBL_0_1 | PushButton2I_w_LED_BL_0_1
PushButton_w_LED_BL_0_1

### Status_ButtonBL_0_2 [References: 0] Defined? True

#define Status_ButtonBL_0_2(LED,B_LED_Cx,Val1,BackLight) PatternT1(LED,28 \
+_Cx2StCh(B_LED_Cx),SI_LocalVar,1,0,255,0,0,0.4 Sec,BackLight,Val1,0,0,0,Val1,0,Val1,0,0,0 \
,63,192,0,0,1,192,0,0,0,0,2)

`defined @` MobaLedLib.h#421

I depend on these macros:

Status_ButtonBL_0_2 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec
_Cx2StCh

These macros depend on me:

Status_ButtonBL_0_2 | PushButton2I_w_LED_BL_0_2
PushButton_w_LED_BL_0_2

### Status_ButtonBL_0_3 [References: 0] Defined? True

#define Status_ButtonBL_0_3(LED,B_LED_Cx,Val1,BackLight) PatternT1(LED,28 \
+_Cx2StCh(B_LED_Cx),SI_LocalVar,1,0,255,0,0,0.4 \
Sec,BackLight,Val1,0,0,0,Val1,0,Val1,0,0,0,Val1,0,Val1,0,Val1,0,0,0 \
,63,192,0,0,1,192,0,0,0,0,2,192,0,0,0,0,0,0,3)

`defined @` MobaLedLib.h#422

I depend on these macros:

Status_ButtonBL_0_3 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec
_Cx2StCh

These macros depend on me:

Status_ButtonBL_0_3 | PushButton2I_w_LED_BL_0_3
PushButton_w_LED_BL_0_3

### Status_ButtonBL_0_4 [References: 0] Defined? True

#define Status_ButtonBL_0_4(LED,B_LED_Cx,Val1,BackLight) PatternT1(LED,28 \
+_Cx2StCh(B_LED_Cx),SI_LocalVar,1,0,255,0,0,0.4 \
Sec,BackLight,Val1,0,0,0,Val1,0,Val1,0,0,0,Val1,0,Val1,0,Val1,0,0,0,Val1,0,Val1,0,Val1,0,Val1,0,0,0 \
,63,192,0,0,1,192,0,0,0,0,2,192,0,0,0,0,0,0,3,192,0,0,0,0,0,0,0,0,4)

`defined @` MobaLedLib.h#423

I depend on these macros:

Status_ButtonBL_0_4 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec
_Cx2StCh

These macros depend on me:

Status_ButtonBL_0_4 | PushButton2I_w_LED_BL_0_4
PushButton_w_LED_BL_0_4

### Status_ButtonBL_0_5 [References: 0] Defined? True

#define Status_ButtonBL_0_5(LED,B_LED_Cx,Val1,BackLight) PatternT1(LED,28 \
+_Cx2StCh(B_LED_Cx),SI_LocalVar,1,0,255,0,0,0.4 \
Sec,BackLight,Val1,0,0,0,Val1,0,Val1,0,0,0,Val1,0,Val1,0,Val1,0,0,0,Val1,0,Val1,0,Val1,0,Val1,0,0,0,Val1,0,Val1,0,Val1,0,Val1,0,Val1\
,0,0,0 ,63,192,0,0,1,192,0,0,0,0,2,192,0,0,0,0,0,0,3,192,0,0,0,0,0,0,0,0,4,192,0,0,0,0,0,0,0,0,0,0,5) \

`defined @` MobaLedLib.h#424

I depend on these macros:

Status_ButtonBL_0_5 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec
_Cx2StCh

These macros depend on me:

Status_ButtonBL_0_5 | PushButton2I_w_LED_BL_0_5
PushButton_w_LED_BL_0_5

### Status_Button_0_1 [References: 0] Defined? True

#define Status_Button_0_1(LED,B_LED_Cx,Val1) PatternT1(LED,40 +_Cx2StCh(B_LED_Cx),SI_LocalVar,1,0,Val1,0,0,0.4 \
Sec,57,0 ,63,192,0,0,1)

`defined @` MobaLedLib.h#413

I depend on these macros:

Status_Button_0_1 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec
_Cx2StCh

These macros depend on me:

Status_Button_0_1 | PushButton_w_LED_0_1

### Status_Button_0_2 [References: 0] Defined? True

#define Status_Button_0_2(LED,B_LED_Cx,Val1) PatternT1(LED,232+_Cx2StCh(B_LED_Cx),SI_LocalVar,1,0,Val1,0,0,0.4 \
Sec,57,128,227,0,0 ,63,192,0,0,1,192,0,0,0,0,2)

`defined @` MobaLedLib.h#414

I depend on these macros:

Status_Button_0_2 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec
_Cx2StCh

These macros depend on me:

Status_Button_0_2 | PushButton_w_LED_0_2

### Status_Button_0_3 [References: 0] Defined? True

#define Status_Button_0_3(LED,B_LED_Cx,Val1) PatternT1(LED,232+_Cx2StCh(B_LED_Cx),SI_LocalVar,1,0,Val1,0,0,0.4 \
Sec,57,128,227,0,142,227,0,0 ,63,192,0,0,1,192,0,0,0,0,2,192,0,0,0,0,0,0,3)

`defined @` MobaLedLib.h#415

I depend on these macros:

Status_Button_0_3 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec
_Cx2StCh

These macros depend on me:

Status_Button_0_3 | PushButton_w_LED_0_3

### Status_Button_0_4 [References: 0] Defined? True

#define Status_Button_0_4(LED,B_LED_Cx,Val1) PatternT1(LED,40 +_Cx2StCh(B_LED_Cx),SI_LocalVar,1,0,Val1,0,0,0.4 \
Sec,57,128,227,0,142,227,0,142,227,56,0 ,63,192,0,0,1,192,0,0,0,0,2,192,0,0,0,0,0,0,3,192,0,0,0,0,0,0,0,0,4) \

`defined @` MobaLedLib.h#416

I depend on these macros:

Status_Button_0_4 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec
_Cx2StCh

These macros depend on me:

Status_Button_0_4 | PushButton_w_LED_0_4

### Status_Button_0_5 [References: 0] Defined? True

#define Status_Button_0_5(LED,B_LED_Cx,Val1) PatternT1(LED,168+_Cx2StCh(B_LED_Cx),SI_LocalVar,1,0,Val1,0,0,0.4 \
Sec,57,128,227,0,142,227,0,142,227,56,128,227,56,142,3,0 \
,63,192,0,0,1,192,0,0,0,0,2,192,0,0,0,0,0,0,3,192,0,0,0,0,0,0,0,0,4,192,0,0,0,0,0,0,0,0,0,0,5) \

`defined @` MobaLedLib.h#417

I depend on these macros:

Status_Button_0_5 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec
_Cx2StCh

These macros depend on me:

Status_Button_0_5 | PushButton_w_LED_0_5

### Status_Button_RGB_0_1 [References: 0] Defined? True

#define Status_Button_RGB_0_1(LED,R0,G0,B0,R10,G10,B10,R11,G11,B11) \
PatternT1(LED,28,SI_LocalVar,3,0,255,0,0,0.5 Sec,R0,G0,B0,R10,G10,B10,R11,G11,B11 \
,63,192,1)

`defined @` MobaLedLib.h#427

I depend on these macros:

Status_Button_RGB_0_1 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec

These macros depend on me:

Status_Button_RGB_0_1 | PushButton2I_RGB_0_1
PushButton_RGB_0_1

### Status_Button_RGB_0_2 [References: 0] Defined? True

#define Status_Button_RGB_0_2(LED,R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21) \
PatternT1(LED,28,SI_LocalVar,3,0,255,0,0,0.5 Sec,R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21 \
,63,192,1,192,2)

`defined @` MobaLedLib.h#428

I depend on these macros:

Status_Button_RGB_0_2 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec

These macros depend on me:

Status_Button_RGB_0_2 | PushButton2I_RGB_0_2
PushButton_RGB_0_2

### Status_Button_RGB_0_3 [References: 0] Defined? True

#define Status_Button_RGB_0_3(LED,R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21,R30,G30,B30,R31,G31,B31) \
PatternT1(LED,28,SI_LocalVar,3,0,255,0,0,0.5 \
Sec,R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21,R30,G30,B30,R31,G31,B31 \
,63,192,1,192,2,192,3)

`defined @` MobaLedLib.h#429

I depend on these macros:

Status_Button_RGB_0_3 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec

These macros depend on me:

Status_Button_RGB_0_3 | PushButton2I_RGB_0_3
PushButton_RGB_0_3

### Status_Button_RGB_0_4 [References: 0] Defined? True

#define Status_Button_RGB_0_4(LED,R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21,R30,G30,B30,R31,G31,B31,R40,G40,B40,R41,G41,B41) \
PatternT1(LED,28,SI_LocalVar,3,0,255,0,0,0.5 \
Sec,R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21,R30,G30,B30,R31,G31,B31,R40,G40,B40,R41,G41,B41 \
,63,192,1,192,2,192,3,192,4)

`defined @` MobaLedLib.h#430

I depend on these macros:

Status_Button_RGB_0_4 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec

These macros depend on me:

Status_Button_RGB_0_4 | PushButton2I_RGB_0_4
PushButton_RGB_0_4

### Status_Button_RGB_0_5 [References: 0] Defined? True

#define Status_Button_RGB_0_5(LED,R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21,R30,G30,B30,R31,G31,B31,R40,G40,B40,R41,G41,B41,R50,G50,B50,R51,G51,B51) 1,B51) PatternT1(LED,28,SI_LocalVar,3,0,255,0,0,0.5 \
Sec,R0,G0,B0,R10,G10,B10,R11,G11,B11,R20,G20,B20,R21,G21,B21,R30,G30,B30,R31,G31,B31,R40,G40,B40,R41,G41,B41,R50,G50,B50,R51,G51,B51 \
,63,192,1,192,2,192,3,192,4,192,5)

`defined @` MobaLedLib.h#431

I depend on these macros:

Status_Button_RGB_0_5 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
Sec

These macros depend on me:

Status_Button_RGB_0_5 | PushButton2I_RGB_0_5
PushButton_RGB_0_5

### TM_BUT_TEST [References: 0] Defined? True

#define TM_BUT_TEST 3

`defined @` MobaLedLib.h#1265

### TM_DISABLED [References: 0] Defined? True

#define TM_DISABLED 0

`defined @` MobaLedLib.h#1262

### TM_INP_TEST [References: 0] Defined? True

#define TM_INP_TEST 2

`defined @` MobaLedLib.h#1264

### TM_LED_TEST [References: 0] Defined? True

#define TM_LED_TEST 1

`defined @` MobaLedLib.h#1263

### TOTAL_SEND_INPUTS [References: 0] Defined? True

#define TOTAL_SEND_INPUTS 1

`defined @` leds_autoprog.h#70

### TOTAL_SWITCHES_A [References: 0] Defined? True

#define TOTAL_SWITCHES_A 0

`defined @` leds_autoprog.h#71

### TOTAL_SWITCHES_B [References: 0] Defined? True

#define TOTAL_SWITCHES_B 0

`defined @` leds_autoprog.h#72

### TOTAL_SWITCHES_C [References: 0] Defined? True

#define TOTAL_SWITCHES_C 0

`defined @` leds_autoprog.h#73

### TOTAL_SWITCHES_D [References: 0] Defined? True

#define TOTAL_SWITCHES_D 0

`defined @` leds_autoprog.h#74

### TOTAL_VARIABLES [References: 0] Defined? True

#define TOTAL_VARIABLES 1

`defined @` leds_autoprog.h#75

### TWO_BUTTONS_PER_ADDRESS [References: 0] Defined? True

#define TWO_BUTTONS_PER_ADDRESS 1

`defined @` leds_autoprog.h#14

### T_BIN_MASK [References: 0] Defined? True

#define T_BIN_MASK 4

`defined @` leds_autoprog.h#92

### T_EQUAL_THEN [References: 0] Defined? True

#define T_EQUAL_THEN 0

`defined @` leds_autoprog.h#88

### T_FlipFlop2Reset [References: 0] Defined? True

#define T_FlipFlop2Reset(DstVar0,DstVar1,T_InCh,R_InCh) Counter(_CM_T_FlipFlopReset2, \
T_InCh, R_InCh, 0, DstVar0, DstVar1)

`defined @` MobaLedLib.h#376

I depend on these macros:

T_FlipFlop2Reset | Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
_CM_T_FlipFlopReset2 | CF_INV_ENABLE
CF_ROTATE

### T_FlipFlop2ResetTimeout [References: 0] Defined? True

#define T_FlipFlop2ResetTimeout(DstVar0,DstVar1,T_InCh,R_InCh,Timeout) Counter(_CM_T_FlipFlopReset2, \
T_InCh, R_InCh, Timeout, DstVar0, DstVar1)

`defined @` MobaLedLib.h#377

I depend on these macros:

T_FlipFlop2ResetTimeout | Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
_CM_T_FlipFlopReset2 | CF_INV_ENABLE
CF_ROTATE

### T_FlipFlopInvReset [References: 0] Defined? True

#define T_FlipFlopInvReset(DstVar,T_InCh,R_InCh) Counter(_CM_T_FlipFlopReset2, T_InCh, \
R_InCh, 0, DstVar, DstVar)

`defined @` MobaLedLib.h#368

I depend on these macros:

T_FlipFlopInvReset | Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
_CM_T_FlipFlopReset2 | CF_INV_ENABLE
CF_ROTATE

### T_FlipFlopInvResetTimeout [References: 0] Defined? True

#define T_FlipFlopInvResetTimeout(DstVar,T_InCh,R_InCh,Timeout) Counter(_CM_T_FlipFlopReset2, \
T_InCh, R_InCh, Timeout, DstVar, DstVar)

`defined @` MobaLedLib.h#369

I depend on these macros:

T_FlipFlopInvResetTimeout | Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
_CM_T_FlipFlopReset2 | CF_INV_ENABLE
CF_ROTATE

### T_FlipFlopReset [References: 0] Defined? True

#define T_FlipFlopReset(DstVar,T_InCh,R_InCh) Counter(_CM_T_FlipFlop1, T_InCh, R_InCh, 0, \
DstVar)

`defined @` MobaLedLib.h#360

I depend on these macros:

T_FlipFlopReset | Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
_CM_T_FlipFlop1 | CF_BINARY
CF_INV_ENABLE
CF_ROTATE

### T_FlipFlopResetTimeout [References: 0] Defined? True

#define T_FlipFlopResetTimeout(DstVar,T_InCh,R_InCh,Timeout) Counter(_CM_T_FlipFlop1, \
T_InCh, R_InCh, Timeout, DstVar)

`defined @` MobaLedLib.h#361

I depend on these macros:

T_FlipFlopResetTimeout | Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
_CM_T_FlipFlop1 | CF_BINARY
CF_INV_ENABLE
CF_ROTATE

### T_LESS_THEN [References: 0] Defined? True

#define T_LESS_THEN 2

`defined @` leds_autoprog.h#90

### T_NOT_BIN_MASK [References: 0] Defined? True

#define T_NOT_BIN_MASK 5

`defined @` leds_autoprog.h#93

### T_NOT_EQUAL_THEN [References: 0] Defined? True

#define T_NOT_EQUAL_THEN 1

`defined @` leds_autoprog.h#89

### USE_EXT_ADDR [References: 0] Defined? True

#define USE_EXT_ADDR

`defined @` leds_autoprog.h#30

### USE_GLOBALVAR_T [References: 0] Defined? True

#define USE_GLOBALVAR_T 172

`defined @` Macros.h#662

These macros depend on me:

USE_GLOBALVAR_T | Use_GlobalVar

### USE_LED_TO_VAR [References: 0] Defined? True

#define USE_LED_TO_VAR

`defined @` leds_autoprog.h#86

### USE_PROTOCOL_DCC [References: 0] Defined? True

#define USE_PROTOCOL_DCC

`defined @` leds_autoprog.h#24

### USE_RS232_OR_SPI_AS_INPUT [References: 0] Defined? True

#define USE_RS232_OR_SPI_AS_INPUT

`defined @` leds_autoprog.h#31

### Use_GlobalVar [References: 0] Defined? True

#define Use_GlobalVar(GlobVarNr) USE_GLOBALVAR_T, GlobVarNr,

`defined @` MobaLedLib.h#133

I depend on these macros:

Use_GlobalVar | USE_GLOBALVAR_T

### VorsignalBin_RGB [References: 0] Defined? True

#define VorsignalBin_RGB(LED,InCh,MaxB16) Bin_InCh_to_TmpVar(InCh, 1) \
XPatternT1(LED,12,SI_LocalVar,12,0,MaxB16,0,0,500 ms,0,0,0,0,0,0,0,128,0,0,128,0,0,0,0,0,0,0,122,0,0,122,0,0 \
,0,63,128,63)

`defined @` MobaLedLib.h#334

I depend on these macros:

VorsignalBin_RGB | Bin_InCh_to_TmpVar | BIN_INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### Vorsignal_RGB [References: 0] Defined? True

#define Vorsignal_RGB(LED,InCh,MaxB16) InCh_to_TmpVar(InCh, 2) XPatternT1(LED,12,SI_LocalVar,12,0,MaxB16,0,0,500 \
ms,0,0,0,0,0,0,0,128,0,0,128,0,0,0,0,0,0,0,122,0,0,122,0,0 ,0,63,128,63)

`defined @` MobaLedLib.h#300

I depend on these macros:

Vorsignal_RGB | InCh_to_TmpVar | INCH_TO_TMPVAR_T
SI_LocalVar | SI_0
XPatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B
ms

### WELDING_CONT_T [References: 0] Defined? True

#define WELDING_CONT_T 141

`defined @` Macros.h#655

These macros depend on me:

WELDING_CONT_T | WeldingCont

### WELDING_T [References: 0] Defined? True

#define WELDING_T 142

`defined @` Macros.h#656

These macros depend on me:

WELDING_T | Welding | RandWelding

### WITHOUT_CHANNEL_MASK [References: 0] Defined? True

#define WITHOUT_CHANNEL_MASK HOUSE_T

`defined @` Macros.h#698

I depend on these macros:

WITHOUT_CHANNEL_MASK | HOUSE_T

### WITHOUT_INP_CH [References: 0] Defined? True

#define WITHOUT_INP_CH NEW_HSV_GROUP_T

`defined @` Macros.h#699

I depend on these macros:

WITHOUT_INP_CH | NEW_HSV_GROUP_T

### Welding [References: 0] Defined? True

#define Welding(LED,InCh) WELDING_T, _CHKL(LED)+RAM5, InCh,

`defined @` MobaLedLib.h#120

I depend on these macros:

Welding | RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
WELDING_T
_CHKL | NUM_LEDS
_ERR_LED_RANGE

These macros depend on me:

Welding | RandWelding

### WeldingCont [References: 0] Defined? True

#define WeldingCont(LED,InCh) WELDING_CONT_T, _CHKL(LED)+RAM5, InCh,

`defined @` MobaLedLib.h#119

I depend on these macros:

WeldingCont | RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
WELDING_CONT_T
_CHKL | NUM_LEDS
_ERR_LED_RANGE

### XPatternT1 [References: 0] Defined? True

#define XPatternT1(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,...) APATTERNT1_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#246

I depend on these macros:

XPatternT1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

These macros depend on me:

XPatternT1 | DepSignal4
DepSignal4Bin
DepSignal4Bin_RGB
DepSignal4_RGB
EntrySignal3
EntrySignal3Bin
EntrySignal3Bin_RGB
EntrySignal3_RGB_BT | EntrySignal3_RGB
EntrySignal3_RGB_B
EntrySignal3_RGB_T
GleissperrsignalBin_RGB
Gleissperrsignal_RGB
HP_2_2Bin_RGB
HP_2_2_RGB
HS_5_PlusBin_RGB
HS_5_Plus_RGB
HS_5lBin_RGB
HS_5l_RGB
HS_5rBin_RGB
HS_5r_RGB
HS_EinfachBin_RGB
HS_Einfach_RGB
SingleLedSignal
SingleLedSignalEx
VorsignalBin_RGB
Vorsignal_RGB

### XPatternT10 [References: 0] Defined? True

#define XPatternT10(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,...) \
APATTERNT10_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_W2B(CO\
UNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#255

I depend on these macros:

XPatternT10 | APATTERNT10_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT11 [References: 0] Defined? True

#define XPatternT11(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,...) \
APATTERNT11_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#256

I depend on these macros:

XPatternT11 | APATTERNT11_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

These macros depend on me:

XPatternT11 | KS_Hauptsignal_Zs3_Zs1
KS_Hauptsignal_Zs3_Zs1Bin
KS_Hauptsignal_Zs3_Zs1Bin_RGB
KS_Hauptsignal_Zs3_Zs1_RGB
KS_Hauptsignal_Zs3_Zs6_Zs1
KS_Hauptsignal_Zs3_Zs6_Zs1Bin
KS_Hauptsignal_Zs3_Zs6_Zs1Bin_RGB
KS_Hauptsignal_Zs3_Zs6_Zs1_RGB

### XPatternT12 [References: 0] Defined? True

#define XPatternT12(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,...) \
APATTERNT12_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#257

I depend on these macros:

XPatternT12 | APATTERNT12_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT13 [References: 0] Defined? True

#define XPatternT13(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,...) \
APATTERNT13_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#258

I depend on these macros:

XPatternT13 | APATTERNT13_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT14 [References: 0] Defined? True

#define XPatternT14(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,...) \
APATTERNT14_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#259

I depend on these macros:

XPatternT14 | APATTERNT14_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT15 [References: 0] Defined? True

#define XPatternT15(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,...) \
APATTERNT15_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#260

I depend on these macros:

XPatternT15 | APATTERNT15_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT16 [References: 0] Defined? True

#define XPatternT16(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,...) \
APATTERNT16_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#261

I depend on these macros:

XPatternT16 | APATTERNT16_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT17 [References: 0] Defined? True

#define XPatternT17(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,...) \
APATTERNT17_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#262

I depend on these macros:

XPatternT17 | APATTERNT17_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT18 [References: 0] Defined? True

#define XPatternT18(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,...) \
APATTERNT18_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#263

I depend on these macros:

XPatternT18 | APATTERNT18_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT19 [References: 0] Defined? True

#define XPatternT19(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,...) \
APATTERNT19_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#264

I depend on these macros:

XPatternT19 | APATTERNT19_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT2 [References: 0] Defined? True

#define XPatternT2(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,...) APATTERNT2_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#247

I depend on these macros:

XPatternT2 | APATTERNT2_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT20 [References: 0] Defined? True

#define XPatternT20(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,...) \
APATTERNT20_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#265

I depend on these macros:

XPatternT20 | APATTERNT20_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT21 [References: 0] Defined? True

#define XPatternT21(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,...) \
APATTERNT21_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_W2B(COUNT_VARARGS(__VA_ARGS_\
_)), __VA_ARGS__,

`defined @` Macros.h#266

I depend on these macros:

XPatternT21 | APATTERNT21_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT22 [References: 0] Defined? True

#define XPatternT22(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,...) .) APATTERNT22_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_W2B(COUNT_VARARGS(\
__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#267

I depend on these macros:

XPatternT22 | APATTERNT22_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT23 [References: 0] Defined? True

#define XPatternT23(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,...) 3,...) APATTERNT23_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_W2B(COUN\
T_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#268

I depend on these macros:

XPatternT23 | APATTERNT23_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT24 [References: 0] Defined? True

#define XPatternT24(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,...) 4,...) APATTERNT24_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#269

I depend on these macros:

XPatternT24 | APATTERNT24_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT25 [References: 0] Defined? True

#define XPatternT25(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,...) 5,...) APATTERNT25_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#270

I depend on these macros:

XPatternT25 | APATTERNT25_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT26 [References: 0] Defined? True

#define XPatternT26(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,...) 6,...) APATTERNT26_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#271

I depend on these macros:

XPatternT26 | APATTERNT26_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT27 [References: 0] Defined? True

#define XPatternT27(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,...) 7,...) APATTERNT27_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#272

I depend on these macros:

XPatternT27 | APATTERNT27_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT28 [References: 0] Defined? True

#define XPatternT28(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,...) 8,...) APATTERNT28_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#273

I depend on these macros:

XPatternT28 | APATTERNT28_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT29 [References: 0] Defined? True

#define XPatternT29(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,...) 9,...) APATTERNT29_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#274

I depend on these macros:

XPatternT29 | APATTERNT29_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT3 [References: 0] Defined? True

#define XPatternT3(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,...) APATTERNT3_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#248

I depend on these macros:

XPatternT3 | APATTERNT3_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT30 [References: 0] Defined? True

#define XPatternT30(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,...) 0,...) APATTERNT30_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#275

I depend on these macros:

XPatternT30 | APATTERNT30_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT31 [References: 0] Defined? True

#define XPatternT31(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,...) 1,...) APATTERNT31_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#276

I depend on these macros:

XPatternT31 | APATTERNT31_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT32 [References: 0] Defined? True

#define XPatternT32(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,...) 2,...) APATTERNT32_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#277

I depend on these macros:

XPatternT32 | APATTERNT32_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT33 [References: 0] Defined? True

#define XPatternT33(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,...) 3,...) APATTERNT33_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#278

I depend on these macros:

XPatternT33 | APATTERNT33_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT34 [References: 0] Defined? True

#define XPatternT34(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,...) 4,...) APATTERNT34_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_W2B(COUNT_VARARGS(__VA_ARGS__)\
), __VA_ARGS__,

`defined @` Macros.h#279

I depend on these macros:

XPatternT34 | APATTERNT34_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT35 [References: 0] Defined? True

#define XPatternT35(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,...) 5,...) APATTERNT35_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_W2B(COUNT_VARARGS(__\
VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#280

I depend on these macros:

XPatternT35 | APATTERNT35_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT36 [References: 0] Defined? True

#define XPatternT36(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,...) 6,...) APATTERNT36_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_W2B(COUNT_\
VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#281

I depend on these macros:

XPatternT36 | APATTERNT36_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT37 [References: 0] Defined? True

#define XPatternT37(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,...) 7,...) APATTERNT37_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_\
W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#282

I depend on these macros:

XPatternT37 | APATTERNT37_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT38 [References: 0] Defined? True

#define XPatternT38(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,...) 8,...) APATTERNT38_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_\
T2B(T38),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#283

I depend on these macros:

XPatternT38 | APATTERNT38_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT39 [References: 0] Defined? True

#define XPatternT39(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,...) 9,...) APATTERNT39_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_\
T2B(T38),_T2B(T39),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#284

I depend on these macros:

XPatternT39 | APATTERNT39_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT4 [References: 0] Defined? True

#define XPatternT4(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,...) APATTERNT4_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#249

I depend on these macros:

XPatternT4 | APATTERNT4_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT40 [References: 0] Defined? True

#define XPatternT40(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,...) 0,...) \
APATTERNT40_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_\
T2B(T38),_T2B(T39),_T2B(T40),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#285

I depend on these macros:

XPatternT40 | APATTERNT40_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT41 [References: 0] Defined? True

#define XPatternT41(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,...) 1,...) \
APATTERNT41_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_\
T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__, \

`defined @` Macros.h#286

I depend on these macros:

XPatternT41 | APATTERNT41_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT42 [References: 0] Defined? True

#define XPatternT42(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,...) 2,...) \
APATTERNT42_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_\
T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#287

I depend on these macros:

XPatternT42 | APATTERNT42_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT43 [References: 0] Defined? True

#define XPatternT43(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,...) 3,...) \
APATTERNT43_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_\
T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#288

I depend on these macros:

XPatternT43 | APATTERNT43_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT44 [References: 0] Defined? True

#define XPatternT44(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,...) 4,...) \
APATTERNT44_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_\
T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#289

I depend on these macros:

XPatternT44 | APATTERNT44_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT45 [References: 0] Defined? True

#define XPatternT45(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,...) 5,...) \
APATTERNT45_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_\
T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#290

I depend on these macros:

XPatternT45 | APATTERNT45_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT46 [References: 0] Defined? True

#define XPatternT46(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,...) 6,...) \
APATTERNT46_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_\
T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#291

I depend on these macros:

XPatternT46 | APATTERNT46_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT47 [References: 0] Defined? True

#define XPatternT47(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,...) 7,...) \
APATTERNT47_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_\
T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#292

I depend on these macros:

XPatternT47 | APATTERNT47_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT48 [References: 0] Defined? True

#define XPatternT48(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,...) 8,...) \
APATTERNT48_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_\
T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_W2B(COUNT_VARARGS(__VA\
_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#293

I depend on these macros:

XPatternT48 | APATTERNT48_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT49 [References: 0] Defined? True

#define XPatternT49(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,...) 9,...) \
APATTERNT49_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_\
T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_W2B(COUNT_VA\
RARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#294

I depend on these macros:

XPatternT49 | APATTERNT49_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT5 [References: 0] Defined? True

#define XPatternT5(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,...) APATTERNT5_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#250

I depend on these macros:

XPatternT5 | APATTERNT5_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT50 [References: 0] Defined? True

#define XPatternT50(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,...) 0,...) \
APATTERNT50_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_\
T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_W2\
B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#295

I depend on these macros:

XPatternT50 | APATTERNT50_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT51 [References: 0] Defined? True

#define XPatternT51(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,...) 1,...) \
APATTERNT51_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_\
T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2\
B(T51),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#296

I depend on these macros:

XPatternT51 | APATTERNT51_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT52 [References: 0] Defined? True

#define XPatternT52(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,...) 2,...) \
APATTERNT52_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_\
T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2\
B(T51),_T2B(T52),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#297

I depend on these macros:

XPatternT52 | APATTERNT52_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT53 [References: 0] Defined? True

#define XPatternT53(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,...) 3,...) \
APATTERNT53_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_\
T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2\
B(T51),_T2B(T52),_T2B(T53),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#298

I depend on these macros:

XPatternT53 | APATTERNT53_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT54 [References: 0] Defined? True

#define XPatternT54(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,...) 4,...) \
APATTERNT54_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_\
T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2\
B(T51),_T2B(T52),_T2B(T53),_T2B(T54),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__, \

`defined @` Macros.h#299

I depend on these macros:

XPatternT54 | APATTERNT54_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT55 [References: 0] Defined? True

#define XPatternT55(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,...) 5,..\
.) APATTERNT55_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_\
T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2\
B(T51),_T2B(T52),_T2B(T53),_T2B(T54),_T2B(T55),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#300

I depend on these macros:

XPatternT55 | APATTERNT55_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT56 [References: 0] Defined? True

#define XPatternT56(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,...) \
6,...) APATTERNT56_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_\
T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2\
B(T51),_T2B(T52),_T2B(T53),_T2B(T54),_T2B(T55),_T2B(T56),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#301

I depend on these macros:

XPatternT56 | APATTERNT56_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT57 [References: 0] Defined? True

#define XPatternT57(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,...) 6,T57,...) APATTERNT57_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_\
T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2\
B(T51),_T2B(T52),_T2B(T53),_T2B(T54),_T2B(T55),_T2B(T56),_T2B(T57),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#302

I depend on these macros:

XPatternT57 | APATTERNT57_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT58 [References: 0] Defined? True

#define XPatternT58(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,...) T57,T58,...) APATTERNT58_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_\
T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2\
B(T51),_T2B(T52),_T2B(T53),_T2B(T54),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#303

I depend on these macros:

XPatternT58 | APATTERNT58_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT59 [References: 0] Defined? True

#define XPatternT59(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,...) T58,T59,...) APATTERNT59_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_\
T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2\
B(T51),_T2B(T52),_T2B(T53),_T2B(T54),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_T2B(T59),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#304

I depend on these macros:

XPatternT59 | APATTERNT59_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT6 [References: 0] Defined? True

#define XPatternT6(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,...) APATTERNT6_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#251

I depend on these macros:

XPatternT6 | APATTERNT6_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT60 [References: 0] Defined? True

#define XPatternT60(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,...) T59,T60,...) APATTERNT60_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_\
T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2\
B(T51),_T2B(T52),_T2B(T53),_T2B(T54),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_T2B(T59),_T2B(T60),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#305

I depend on these macros:

XPatternT60 | APATTERNT60_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT61 [References: 0] Defined? True

#define XPatternT61(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,...) T60,T61,...) APATTERNT61_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_\
T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2\
B(T51),_T2B(T52),_T2B(T53),_T2B(T54),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_T2B(T59),_T2B(T60),_T2B(T61),_W2B(COUNT_VARARGS(__VA_A\
RGS__)), __VA_ARGS__,

`defined @` Macros.h#306

I depend on these macros:

XPatternT61 | APATTERNT61_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT62 [References: 0] Defined? True

#define XPatternT62(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,...) T61,T62,...) APATTERNT62_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_\
T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2\
B(T51),_T2B(T52),_T2B(T53),_T2B(T54),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_T2B(T59),_T2B(T60),_T2B(T61),_T2B(T62),_W2B(COUNT_VARA\
RGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#307

I depend on these macros:

XPatternT62 | APATTERNT62_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT63 [References: 0] Defined? True

#define XPatternT63(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,T63,...) T62,T63,...) APATTERNT63_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_\
T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2\
B(T51),_T2B(T52),_T2B(T53),_T2B(T54),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_T2B(T59),_T2B(T60),_T2B(T61),_T2B(T62),_T2B(T63),_W2B(\
COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#308

I depend on these macros:

XPatternT63 | APATTERNT63_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT64 [References: 0] Defined? True

#define XPatternT64(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,T63,T64,...) T63,T64,...) APATTERNT64_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T1\
1),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18),_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24)\
,_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_\
T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2\
B(T51),_T2B(T52),_T2B(T53),_T2B(T54),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(T58),_T2B(T59),_T2B(T60),_T2B(T61),_T2B(T62),_T2B(T63),_T2B(\
T64),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#309

I depend on these macros:

XPatternT64 | APATTERNT64_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT7 [References: 0] Defined? True

#define XPatternT7(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,...) \
APATTERNT7_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#252

I depend on these macros:

XPatternT7 | APATTERNT7_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT8 [References: 0] Defined? True

#define XPatternT8(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,...) \
APATTERNT8_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_W2B(COUNT_VARARGS(__VA_AR\
GS__)), __VA_ARGS__,

`defined @` Macros.h#253

I depend on these macros:

XPatternT8 | APATTERNT8_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternT9 [References: 0] Defined? True

#define XPatternT9(LED,NStru,InCh,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,...) \
APATTERNT9_T, _CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),SI_1, \
LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_W2B(COUNT_VARARG\
S(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#254

I depend on these macros:

XPatternT9 | APATTERNT9_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

These macros depend on me:

XPatternT9 | AndreaskrLT
AndreaskrLT3
AndreaskrLT3_RGB
AndreaskrLT_RGB
KS_Vorsignal_Zs3V
KS_Vorsignal_Zs3VBin
KS_Vorsignal_Zs3VBin_RGB
KS_Vorsignal_Zs3V_RGB

### XPatternTE1 [References: 0] Defined? True

#define XPatternTE1(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,...) APATTERNT1_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_W2B(COUNT_VARARGS(__VA_ARGS_\
_)), __VA_ARGS__,

`defined @` Macros.h#447

I depend on these macros:

XPatternTE1 | APATTERNT1_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE10 [References: 0] Defined? True

#define XPatternTE10(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,...) \
APATTERNT10_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#456

I depend on these macros:

XPatternTE10 | APATTERNT10_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE11 [References: 0] Defined? True

#define XPatternTE11(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,...) \
APATTERNT11_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#457

I depend on these macros:

XPatternTE11 | APATTERNT11_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE12 [References: 0] Defined? True

#define XPatternTE12(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,...) \
APATTERNT12_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#458

I depend on these macros:

XPatternTE12 | APATTERNT12_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE13 [References: 0] Defined? True

#define XPatternTE13(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,...) \
APATTERNT13_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#459

I depend on these macros:

XPatternTE13 | APATTERNT13_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE14 [References: 0] Defined? True

#define XPatternTE14(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,...) \
APATTERNT14_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#460

I depend on these macros:

XPatternTE14 | APATTERNT14_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE15 [References: 0] Defined? True

#define XPatternTE15(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,...) \
APATTERNT15_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_W2B(COUNT_VARARGS(__VA_ARGS_\
_)), __VA_ARGS__,

`defined @` Macros.h#461

I depend on these macros:

XPatternTE15 | APATTERNT15_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE16 [References: 0] Defined? True

#define XPatternTE16(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,...) \
APATTERNT16_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_W2B(COUNT_VARARGS(\
__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#462

I depend on these macros:

XPatternTE16 | APATTERNT16_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE17 [References: 0] Defined? True

#define XPatternTE17(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,...) \
APATTERNT17_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_W2B(COUN\
T_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#463

I depend on these macros:

XPatternTE17 | APATTERNT17_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE18 [References: 0] Defined? True

#define XPatternTE18(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,...) \
APATTERNT18_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#464

I depend on these macros:

XPatternTE18 | APATTERNT18_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE19 [References: 0] Defined? True

#define XPatternTE19(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,...) \
APATTERNT19_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#465

I depend on these macros:

XPatternTE19 | APATTERNT19_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE2 [References: 0] Defined? True

#define XPatternTE2(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,...) APATTERNT2_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_W2B(COUNT_VARARGS(_\
_VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#448

I depend on these macros:

XPatternTE2 | APATTERNT2_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE20 [References: 0] Defined? True

#define XPatternTE20(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,...) .) APATTERNT20_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#466

I depend on these macros:

XPatternTE20 | APATTERNT20_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE21 [References: 0] Defined? True

#define XPatternTE21(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,...) 1,...) APATTERNT21_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#467

I depend on these macros:

XPatternTE21 | APATTERNT21_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE22 [References: 0] Defined? True

#define XPatternTE22(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,...) 2,...) APATTERNT22_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#468

I depend on these macros:

XPatternTE22 | APATTERNT22_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE23 [References: 0] Defined? True

#define XPatternTE23(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,...) 3,...) APATTERNT23_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#469

I depend on these macros:

XPatternTE23 | APATTERNT23_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE24 [References: 0] Defined? True

#define XPatternTE24(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,...) 4,...) APATTERNT24_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#470

I depend on these macros:

XPatternTE24 | APATTERNT24_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE25 [References: 0] Defined? True

#define XPatternTE25(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,...) 5,...) APATTERNT25_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#471

I depend on these macros:

XPatternTE25 | APATTERNT25_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE26 [References: 0] Defined? True

#define XPatternTE26(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,...) 6,...) APATTERNT26_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#472

I depend on these macros:

XPatternTE26 | APATTERNT26_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE27 [References: 0] Defined? True

#define XPatternTE27(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,...) 7,...) APATTERNT27_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#473

I depend on these macros:

XPatternTE27 | APATTERNT27_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE28 [References: 0] Defined? True

#define XPatternTE28(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,...) 8,...) APATTERNT28_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_W2B(COUNT_VARARGS(__VA_ARGS__)\
), __VA_ARGS__,

`defined @` Macros.h#474

I depend on these macros:

XPatternTE28 | APATTERNT28_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE29 [References: 0] Defined? True

#define XPatternTE29(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,...) 9,...) APATTERNT29_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_W2B(COUNT_VARARGS(__\
VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#475

I depend on these macros:

XPatternTE29 | APATTERNT29_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE3 [References: 0] Defined? True

#define XPatternTE3(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,...) APATTERNT3_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_W2B(COUNT_\
VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#449

I depend on these macros:

XPatternTE3 | APATTERNT3_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE30 [References: 0] Defined? True

#define XPatternTE30(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,...) 0,...) APATTERNT30_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_W2B(COUNT_\
VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#476

I depend on these macros:

XPatternTE30 | APATTERNT30_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE31 [References: 0] Defined? True

#define XPatternTE31(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,...) 1,...) APATTERNT31_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#477

I depend on these macros:

XPatternTE31 | APATTERNT31_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE32 [References: 0] Defined? True

#define XPatternTE32(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,...) 2,...) APATTERNT32_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#478

I depend on these macros:

XPatternTE32 | APATTERNT32_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE33 [References: 0] Defined? True

#define XPatternTE33(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,...) 3,...) APATTERNT33_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#479

I depend on these macros:

XPatternTE33 | APATTERNT33_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE34 [References: 0] Defined? True

#define XPatternTE34(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,...) 4,...) APATTERNT34_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_T2B(T34),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#480

I depend on these macros:

XPatternTE34 | APATTERNT34_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE35 [References: 0] Defined? True

#define XPatternTE35(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,...) 5,...) APATTERNT35_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__, \

`defined @` Macros.h#481

I depend on these macros:

XPatternTE35 | APATTERNT35_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE36 [References: 0] Defined? True

#define XPatternTE36(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,...) 6,...) APATTERNT36_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#482

I depend on these macros:

XPatternTE36 | APATTERNT36_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE37 [References: 0] Defined? True

#define XPatternTE37(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,...) 7,...) APATTERNT37_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#483

I depend on these macros:

XPatternTE37 | APATTERNT37_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE38 [References: 0] Defined? True

#define XPatternTE38(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,...) 8,...) \
APATTERNT38_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#484

I depend on these macros:

XPatternTE38 | APATTERNT38_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE39 [References: 0] Defined? True

#define XPatternTE39(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,...) 9,...) \
APATTERNT39_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#485

I depend on these macros:

XPatternTE39 | APATTERNT39_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE4 [References: 0] Defined? True

#define XPatternTE4(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,...) \
APATTERNT4_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_W\
2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#450

I depend on these macros:

XPatternTE4 | APATTERNT4_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE40 [References: 0] Defined? True

#define XPatternTE40(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,...) 0,...) \
APATTERNT40_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#486

I depend on these macros:

XPatternTE40 | APATTERNT40_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE41 [References: 0] Defined? True

#define XPatternTE41(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,...) 1,...) \
APATTERNT41_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#487

I depend on these macros:

XPatternTE41 | APATTERNT41_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE42 [References: 0] Defined? True

#define XPatternTE42(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,...) 2,...) \
APATTERNT42_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_W2B(COUNT_VARARGS(__VA\
_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#488

I depend on these macros:

XPatternTE42 | APATTERNT42_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE43 [References: 0] Defined? True

#define XPatternTE43(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,...) 3,...) \
APATTERNT43_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_W2B(COUNT_VA\
RARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#489

I depend on these macros:

XPatternTE43 | APATTERNT43_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE44 [References: 0] Defined? True

#define XPatternTE44(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,...) 4,...) \
APATTERNT44_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_W2\
B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#490

I depend on these macros:

XPatternTE44 | APATTERNT44_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE45 [References: 0] Defined? True

#define XPatternTE45(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,...) 5,...) \
APATTERNT45_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2\
B(T45),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#491

I depend on these macros:

XPatternTE45 | APATTERNT45_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE46 [References: 0] Defined? True

#define XPatternTE46(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,...) 6,...) \
APATTERNT46_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2\
B(T45),_T2B(T46),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#492

I depend on these macros:

XPatternTE46 | APATTERNT46_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE47 [References: 0] Defined? True

#define XPatternTE47(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,...) 7,...) \
APATTERNT47_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2\
B(T45),_T2B(T46),_T2B(T47),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#493

I depend on these macros:

XPatternTE47 | APATTERNT47_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE48 [References: 0] Defined? True

#define XPatternTE48(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,...) 8,...) \
APATTERNT48_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2\
B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__, \

`defined @` Macros.h#494

I depend on these macros:

XPatternTE48 | APATTERNT48_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE49 [References: 0] Defined? True

#define XPatternTE49(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,...) 9,...) \
APATTERNT49_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2\
B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#495

I depend on these macros:

XPatternTE49 | APATTERNT49_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE5 [References: 0] Defined? True

#define XPatternTE5(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,...) \
APATTERNT5_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#451

I depend on these macros:

XPatternTE5 | APATTERNT5_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE50 [References: 0] Defined? True

#define XPatternTE50(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,...) 0,...) \
APATTERNT50_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2\
B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#496

I depend on these macros:

XPatternTE50 | APATTERNT50_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE51 [References: 0] Defined? True

#define XPatternTE51(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,...) 1,...) \
APATTERNT51_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2\
B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#497

I depend on these macros:

XPatternTE51 | APATTERNT51_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE52 [References: 0] Defined? True

#define XPatternTE52(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,...) 2,...) \
APATTERNT52_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2\
B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#498

I depend on these macros:

XPatternTE52 | APATTERNT52_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE53 [References: 0] Defined? True

#define XPatternTE53(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,...) 3,..\
.) APATTERNT53_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2\
B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#499

I depend on these macros:

XPatternTE53 | APATTERNT53_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE54 [References: 0] Defined? True

#define XPatternTE54(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,...) \
4,...) APATTERNT54_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2\
B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T54),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#500

I depend on these macros:

XPatternTE54 | APATTERNT54_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE55 [References: 0] Defined? True

#define XPatternTE55(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,...) 4,T55,...) APATTERNT55_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2\
B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T54),_T2B(T55),_W2B(COUNT_VARARGS(__VA_A\
RGS__)), __VA_ARGS__,

`defined @` Macros.h#501

I depend on these macros:

XPatternTE55 | APATTERNT55_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE56 [References: 0] Defined? True

#define XPatternTE56(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,...) T55,T56,...) APATTERNT56_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2\
B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T54),_T2B(T55),_T2B(T56),_W2B(COUNT_VARA\
RGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#502

I depend on these macros:

XPatternTE56 | APATTERNT56_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE57 [References: 0] Defined? True

#define XPatternTE57(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,...) T56,T57,...) APATTERNT57_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2\
B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T54),_T2B(T55),_T2B(T56),_T2B(T57),_W2B(\
COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#503

I depend on these macros:

XPatternTE57 | APATTERNT57_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE58 [References: 0] Defined? True

#define XPatternTE58(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,...) T57,T58,...) APATTERNT58_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2\
B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T54),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(\
T58),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#504

I depend on these macros:

XPatternTE58 | APATTERNT58_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE59 [References: 0] Defined? True

#define XPatternTE59(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,...) T58,T59,...) APATTERNT59_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2\
B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T54),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(\
T58),_T2B(T59),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#505

I depend on these macros:

XPatternTE59 | APATTERNT59_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE6 [References: 0] Defined? True

#define XPatternTE6(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,...) \
APATTERNT6_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#452

I depend on these macros:

XPatternTE6 | APATTERNT6_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE60 [References: 0] Defined? True

#define XPatternTE60(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,...) T59,T60,...) APATTERNT60_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2\
B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T54),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(\
T58),_T2B(T59),_T2B(T60),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#506

I depend on these macros:

XPatternTE60 | APATTERNT60_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE61 [References: 0] Defined? True

#define XPatternTE61(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,...) T60,T61,...) APATTERNT61_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2\
B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T54),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(\
T58),_T2B(T59),_T2B(T60),_T2B(T61),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__, \

`defined @` Macros.h#507

I depend on these macros:

XPatternTE61 | APATTERNT61_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE62 [References: 0] Defined? True

#define XPatternTE62(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,...) T61,T62,...) APATTERNT62_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2\
B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T54),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(\
T58),_T2B(T59),_T2B(T60),_T2B(T61),_T2B(T62),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#508

I depend on these macros:

XPatternTE62 | APATTERNT62_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE63 [References: 0] Defined? True

#define XPatternTE63(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,T63,...) T62,T63,...) APATTERNT63_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2\
B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T54),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(\
T58),_T2B(T59),_T2B(T60),_T2B(T61),_T2B(T62),_T2B(T63),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#509

I depend on these macros:

XPatternTE63 | APATTERNT63_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE64 [References: 0] Defined? True

#define XPatternTE64(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,T10,T11,T12,T13,T14,T15,T16,T17,T18,T19,T20,T21,T22,T23,T24,T25,T26,T27,T28,T29,T30,T31,T32,T33,T34,T35,T36,T37,T38,T39,T40,T41,T42,T43,T44,T45,T46,T47,T48,T49,T50,T51,T52,T53,T54,T55,T56,T57,T58,T59,T60,T61,T62,T63,T64,...) T63,T64,...) APATTERNT64_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_T2B(T10),_T2B(T11),_T2B(T12),_T2B(T13),_T2B(T14),_T2B(T15),_T2B(T16),_T2B(T17),_T2B(T18)\
,_T2B(T19),_T2B(T20),_T2B(T21),_T2B(T22),_T2B(T23),_T2B(T24),_T2B(T25),_T2B(T26),_T2B(T27),_T2B(T28),_T2B(T29),_T2B(T30),_T2B(T31),_\
T2B(T32),_T2B(T33),_T2B(T34),_T2B(T35),_T2B(T36),_T2B(T37),_T2B(T38),_T2B(T39),_T2B(T40),_T2B(T41),_T2B(T42),_T2B(T43),_T2B(T44),_T2\
B(T45),_T2B(T46),_T2B(T47),_T2B(T48),_T2B(T49),_T2B(T50),_T2B(T51),_T2B(T52),_T2B(T53),_T2B(T54),_T2B(T55),_T2B(T56),_T2B(T57),_T2B(\
T58),_T2B(T59),_T2B(T60),_T2B(T61),_T2B(T62),_T2B(T63),_T2B(T64),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#510

I depend on these macros:

XPatternTE64 | APATTERNT64_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE7 [References: 0] Defined? True

#define XPatternTE7(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,...) \
APATTERNT7_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#453

I depend on these macros:

XPatternTE7 | APATTERNT7_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE8 [References: 0] Defined? True

#define XPatternTE8(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,...) \
APATTERNT8_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_W2B(COUNT_VARARGS(__VA_ARGS__)), __VA_ARGS__,

`defined @` Macros.h#454

I depend on these macros:

XPatternTE8 | APATTERNT8_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### XPatternTE9 [References: 0] Defined? True

#define XPatternTE9(LED,NStru,InCh,Enable,LEDs,Val0,Val1,Off,Mode,T1,T2,T3,T4,T5,T6,T7,T8,T9,...) \
APATTERNT9_T, \
_CHKL(LED)+RAM7+RAMN(LEDs),(NStru)&0xFF,_ChkIn(InCh),Enable,LEDs,Val0,Val1,Off,Mode|_PF_XFADE,_T2B(T1),_T2B(T2),_T2B(T3),_T2B(T4),_T\
2B(T5),_T2B(T6),_T2B(T7),_T2B(T8),_T2B(T9),_W2B(COUNT_VARARGS(__VA_ARGS__)), \
__VA_ARGS__,

`defined @` Macros.h#455

I depend on these macros:

XPatternTE9 | APATTERNT9_T
COUNT_VARARGS | _GET_NTH_ARG
RAM7 | RAM1
RAM6 | RAM1
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
RAMN
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_PF_XFADE
_T2B | _W2B
_W2B

### _ALL_LT_MX2 [References: 0] Defined? True

#define _ALL_LT_MX2(MinTime,MaxTime) ((_LT_MX(MinTime) * _LT_MX(MaxTime) * \
_LT_MX((MinTime)+(MaxTime))))

`defined @` Macros.h#45

I depend on these macros:

_ALL_LT_MX2 | _LT_MX | _MAX_TIMER_VAL

These macros depend on me:

_ALL_LT_MX2 | _ALL_LT_MX4 | _RAND_DIV4 | _Tx2B4 | Random | ButtonFunc
Def_Neon_Misha
Flash
RandWelding
_RAND_MODE4 | Random | ButtonFunc
Def_Neon_Misha
Flash
RandWelding
_RAND_DIV2 | _Tx2B2 | RandMux | RandCntMux
_RAND_MODE2 | RandMux | RandCntMux

### _ALL_LT_MX4 [References: 0] Defined? True

#define _ALL_LT_MX4(MinTime1,MaxTime1,MinTime2,MaxTime2) (_ALL_LT_MX2((MinTime1), (MaxTime1)) \
* _ALL_LT_MX2((MinTime2), (MaxTime2)))

`defined @` Macros.h#46

I depend on these macros:

_ALL_LT_MX4 | _ALL_LT_MX2 | _LT_MX | _MAX_TIMER_VAL

These macros depend on me:

_ALL_LT_MX4 | _RAND_DIV4 | _Tx2B4 | Random | ButtonFunc
Def_Neon_Misha
Flash
RandWelding
_RAND_MODE4 | Random | ButtonFunc
Def_Neon_Misha
Flash
RandWelding

### _ALL_NEW_BITS [References: 0] Defined? True

#define _ALL_NEW_BITS 0b01010101

`defined @` MobaLedLib.h#1192

### _ALL_OLD_BITS [References: 0] Defined? True

#define _ALL_OLD_BITS 0b10101010

`defined @` MobaLedLib.h#1191

### _BIT_NEW [References: 0] Defined? True

#define _BIT_NEW 0b00000001

`defined @` MobaLedLib.h#1188

These macros depend on me:

_BIT_NEW | _NEW_AND_OLD

### _BIT_OLD [References: 0] Defined? True

#define _BIT_OLD 0b00000010

`defined @` MobaLedLib.h#1187

These macros depend on me:

_BIT_OLD | _NEW_AND_OLD

### _CF_NO_LEDOUTP [References: 0] Defined? True

#define _CF_NO_LEDOUTP (0b00000100<<8)

`defined @` MobaLedLib.h#1064

These macros depend on me:

_CF_NO_LEDOUTP | CF_ONLY_LOCALVAR | Sound_JQ6500_BG_Next_of_N_Reset | Sound_JQ6500_BG_Next_of_N
Sound_JQ6500_BG_PlayRandom
Sound_JQ6500_Next_of_N_Reset | Sound_JQ6500_Next_of_N
Sound_JQ6500_PlayRandom
Sound_New_Next_of_N_Reset | Sound_New_Next_of_N
Sound_New_PlayRandom
Sound_Next_of_N_Reset | Sound_Next_of_N
Sound_PlayRandom

### _CF_P_P_SKIP0 [References: 0] Defined? True

#define _CF_P_P_SKIP0 (CF_PINGPONG | CF_SKIP0)

`defined @` MobaLedLib.h#1075

I depend on these macros:

_CF_P_P_SKIP0 | CF_PINGPONG
CF_SKIP0

### _CF_ROT_SKIP0 [References: 0] Defined? True

#define _CF_ROT_SKIP0 (CF_ROTATE | CF_SKIP0)

`defined @` MobaLedLib.h#1074

I depend on these macros:

_CF_ROT_SKIP0 | CF_ROTATE
CF_SKIP0

### _CHECK_MODE_RF_NOT_SAME [References: 0] Defined? True

#define _CHECK_MODE_RF_NOT_SAME(Mode,DstVar1,DstVarN) (((Mode)&RF_NOT_SAME) && (DstVarN) \
- (DstVar1) == 0) ? ((Mode) & ~RF_NOT_SAME) : (Mode)

`defined @` MobaLedLib.h#112

I depend on these macros:

_CHECK_MODE_RF_NOT_SAME | RF_NOT_SAME

These macros depend on me:

_CHECK_MODE_RF_NOT_SAME | RandMux | RandCntMux

### _CM_RS_FlipFlop1 [References: 0] Defined? True

#define _CM_RS_FlipFlop1 (CF_BINARY|CF_UP_DOWN)

`defined @` MobaLedLib.h#1068

I depend on these macros:

_CM_RS_FlipFlop1 | CF_BINARY
CF_UP_DOWN

These macros depend on me:

_CM_RS_FlipFlop1 | MonoFlop
MonoFlopLongReset
MonoFlopReset
RS_FlipFlop | _Herz_MoRelais_RS | Herz_MoRelais
Herz_MoRelais_I
RS_FlipFlopTimeout | _Herz_MoRelais_RS | Herz_MoRelais
Herz_MoRelais_I

### _CM_RS_FlipFlop2 [References: 0] Defined? True

#define _CM_RS_FlipFlop2 (CF_UP_DOWN)

`defined @` MobaLedLib.h#1070

I depend on these macros:

_CM_RS_FlipFlop2 | CF_UP_DOWN

These macros depend on me:

_CM_RS_FlipFlop2 | MonoFlop2
MonoFlop2LongReset
MonoFlopInv
MonoFlopInvLongReset
RS_FlipFlop2
RS_FlipFlop2Timeout
RS_FlipFlopInv
RS_FlipFlopInvTimeout

### _CM_T_FlipFlop1 [References: 0] Defined? True

#define _CM_T_FlipFlop1 (CF_BINARY|CF_INV_ENABLE|CF_ROTATE)

`defined @` MobaLedLib.h#1069

I depend on these macros:

_CM_T_FlipFlop1 | CF_BINARY
CF_INV_ENABLE
CF_ROTATE

These macros depend on me:

_CM_T_FlipFlop1 | T_FlipFlopReset
T_FlipFlopResetTimeout

### _CM_T_FlipFlopEnable2 [References: 0] Defined? True

#define _CM_T_FlipFlopEnable2 (CF_ROTATE)

`defined @` MobaLedLib.h#1071

I depend on these macros:

_CM_T_FlipFlopEnable2 | CF_ROTATE

### _CM_T_FlipFlopReset2 [References: 0] Defined? True

#define _CM_T_FlipFlopReset2 (CF_ROTATE | CF_INV_ENABLE)

`defined @` MobaLedLib.h#1072

I depend on these macros:

_CM_T_FlipFlopReset2 | CF_INV_ENABLE
CF_ROTATE

These macros depend on me:

_CM_T_FlipFlopReset2 | T_FlipFlop2Reset
T_FlipFlop2ResetTimeout
T_FlipFlopInvReset
T_FlipFlopInvResetTimeout

### _C_ALL_not_supported [References: 0] Defined? True

#define _C_ALL_not_supported 33877u

`defined @` MobaLedLib.h#1003

These macros depend on me:

_C_ALL_not_supported | _PAT_DBLFL | _Cx2P_DBLFL | BlueLight1
BlueLight2
Leuchtfeuer

### _ConvChannelNr2Byte [References: 0] Defined? True

#define _ConvChannelNr2Byte(ChannelNr) (ChannelNr%4 == 0 ? (ChannelNr)/4 : 512 + (ChannelNr)/4) \

`defined @` MobaLedLib.h#957

These macros depend on me:

_ConvChannelNr2Byte | MobaLedLib_Copy_to_InpStruct

### _Cx2P_DBLFL [References: 0] Defined? True

#define _Cx2P_DBLFL(Cx) (_PAT_DBLFL(_Cx2LedCnt(Cx)))

`defined @` MobaLedLib.h#1010

I depend on these macros:

_Cx2P_DBLFL | _Cx2LedCnt
_PAT_DBLFL | _C_ALL_not_supported

These macros depend on me:

_Cx2P_DBLFL | BlueLight1
BlueLight2
Leuchtfeuer

### _GET_BIN_SIZE [References: 0] Defined? True

#define _GET_BIN_SIZE(n) (n<=1?0:(n<=2?1:(n<=4)?2:(n<=8?3:(n<=16?4:999))))

`defined @` MobaLedLib.h#231

These macros depend on me:

_GET_BIN_SIZE | Charlie_Binary

### _Herz_MoRelais_RS [References: 0] Defined? True

#define _Herz_MoRelais_RS(LED,InCh,Single_Cx,DelayHerz1,TmpNr,Inv) RS_FlipFlopTimeout(TmpNr+0, \
InCh, InCh+1, DelayHerz1 + 200 ms) RS_FlipFlopTimeout(TmpNr+1, InCh, InCh+1, \
DelayHerz1) RS_FlipFlopTimeout(TmpNr+2, InCh+1, InCh, DelayHerz1 + 200 ms) \
RS_FlipFlopTimeout(TmpNr+3, InCh+1, InCh, DelayHerz1) Logic(TmpNr+4, TmpNr+0 AND \
NOT TmpNr+1) Logic(TmpNr+5, TmpNr+2 AND NOT TmpNr+3) RS_FlipFlop(TmpNr+6, TmpNr+5-Inv, \
TmpNr+4+Inv) Const(LED, Single_Cx, TmpNr+6, 0, 255)

`defined @` MobaLedLib.h#645

I depend on these macros:

_Herz_MoRelais_RS | AND
Const | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
Sec
_Cx2LedCnt
_Cx2P_BLINK | _Cx2LedCnt
_PAT_BLINK
_NStru | _Cx2LedCnt
_Cx2StCh
_FreeBits
Logic | COUNT_VARARGS | _GET_NTH_ARG
LOGIC_T
NOT | _NOT_NR | SI_1
RS_FlipFlop | Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
_CM_RS_FlipFlop1 | CF_BINARY
CF_UP_DOWN
RS_FlipFlopTimeout | Counter | COUNTER_T
COUNT_VARARGS | _GET_NTH_ARG
RAM3 | RAM1
RAM2 | RAM1
_T2B | _W2B
_W2B
_CM_RS_FlipFlop1 | CF_BINARY
CF_UP_DOWN
ms

These macros depend on me:

_Herz_MoRelais_RS | Herz_MoRelais
Herz_MoRelais_I

### _LT_MX [References: 0] Defined? True

#define _LT_MX(MaxTime) (((MaxTime)<_MAX_TIMER_VAL)?1:0)

`defined @` Macros.h#44

I depend on these macros:

_LT_MX | _MAX_TIMER_VAL

These macros depend on me:

_LT_MX | _ALL_LT_MX2 | _ALL_LT_MX4 | _RAND_DIV4 | _Tx2B4 | Random | ButtonFunc
Def_Neon_Misha
Flash
RandWelding
_RAND_MODE4 | Random | ButtonFunc
Def_Neon_Misha
Flash
RandWelding
_RAND_DIV2 | _Tx2B2 | RandMux | RandCntMux
_RAND_MODE2 | RandMux | RandCntMux

### _LocalVar_New_Sound [References: 0] Defined? True

#define _LocalVar_New_Sound(LED) PatternT1(LED,28,SI_LocalVar,2,0,255,0,0,200 \
ms,0,0,SOUND_New_ADKEY1,0,SOUND_New_ADKEY2,0,SOUND_New_ADKEY3,0,SOUND_New_ADKEY4,0,0,SOUND_New_ADKEY1,0,SOUND_New_ADKEY2,0,SOUND_New\
_ADKEY3,0,SOUND_New_ADKEY4,0,SOUND_New_ADKEY5,0,SOUND_New_ADKEY6,0,SOUND_New_ADKEY7,0,SOUND_New_ADKEY8,0,SOUND_New_ADKEY9,0,SOUND_Ne\
w_ADKEY10,0,0 ,1,129,129,129,129,129,129,129,129,129,129,129,129,129,129,127)

`defined @` MobaLedLib.h#800

I depend on these macros:

_LocalVar_New_Sound | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
SOUND_New_ADKEY1
SOUND_New_ADKEY10
SOUND_New_ADKEY2
SOUND_New_ADKEY3
SOUND_New_ADKEY4
SOUND_New_ADKEY5
SOUND_New_ADKEY6
SOUND_New_ADKEY7
SOUND_New_ADKEY8
SOUND_New_ADKEY9
ms

These macros depend on me:

_LocalVar_New_Sound | Sound_New_Next_of_N_Reset | Sound_New_Next_of_N
Sound_New_PlayRandom

### _LocalVar_Sound [References: 0] Defined? True

#define _LocalVar_Sound(LED) PatternT1(LED,28,SI_LocalVar,2,0,255,0,0,200 \
ms,0,0,SOUND_ADKEY1,0,SOUND_ADKEY2,0,SOUND_ADKEY3,0,SOUND_ADKEY4,0,0,SOUND_ADKEY1,0,SOUND_ADKEY2,0,SOUND_ADKEY3,0,SOUND_ADKEY4,0,SOU\
ND_ADKEY5,0,SOUND_ADKEY6,0,SOUND_ADKEY7,0,SOUND_ADKEY8,0,SOUND_ADKEY9,0,SOUND_ADKEY10,0,0 \
,1,129,129,129,129,129,129,129,129,129,129,129,129,129,129,127)

`defined @` MobaLedLib.h#739

I depend on these macros:

_LocalVar_Sound | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
SOUND_ADKEY1
SOUND_ADKEY10
SOUND_ADKEY2
SOUND_ADKEY3
SOUND_ADKEY4
SOUND_ADKEY5
SOUND_ADKEY6
SOUND_ADKEY7
SOUND_ADKEY8
SOUND_ADKEY9
ms

These macros depend on me:

_LocalVar_Sound | Sound_Next_of_N_Reset | Sound_Next_of_N
Sound_PlayRandom

### _LocalVar_Sound_JQ6500 [References: 0] Defined? True

#define _LocalVar_Sound_JQ6500(LED) PatternT1(LED,28,SI_LocalVar,1,0,255,0,0,400 \
ms,0,SOUND_JQ6500_ADKEY1_N, SOUND_JQ6500_ADKEY2_N, SOUND_JQ6500_ADKEY3_N, \
SOUND_JQ6500_ADKEY4_N, SOUND_JQ6500_ADKEY5_N, 0,1,129,129,129,129,129,127)

`defined @` MobaLedLib.h#873

I depend on these macros:

_LocalVar_Sound_JQ6500 | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
SOUND_JQ6500_ADKEY1_N
SOUND_JQ6500_ADKEY2_N
SOUND_JQ6500_ADKEY3_N
SOUND_JQ6500_ADKEY4_N
SOUND_JQ6500_ADKEY5_N
ms

These macros depend on me:

_LocalVar_Sound_JQ6500 | Sound_JQ6500_Next_of_N_Reset | Sound_JQ6500_Next_of_N
Sound_JQ6500_PlayRandom

### _LocalVar_Sound_JQ6500_BG [References: 0] Defined? True

#define _LocalVar_Sound_JQ6500_BG(LED) PatternT1(LED,28,SI_LocalVar,1,0,255,0,0,400 \
ms,0,SOUND_JQ6500_ADKEY1_BG,SOUND_JQ6500_ADKEY2_BG,SOUND_JQ6500_ADKEY3_BG,SOUND_JQ6500_ADKEY4_BG,SOUND_JQ6500_ADKEY5_BG,0,1,129,129,\
129,129,129,127)

`defined @` MobaLedLib.h#874

I depend on these macros:

_LocalVar_Sound_JQ6500_BG | PatternT1 | COUNT_VARARGS | _GET_NTH_ARG
PATTERNT1_T
RAM5 | RAM1
RAM4 | RAM1
RAM3 | RAM1
RAM2 | RAM1
SI_1
_CHKL | NUM_LEDS
_ERR_LED_RANGE
_ChkIn | _ERR_INPUT_RANGE
_INP_STRUCT_ARRAY_SIZE
_T2B | _W2B
_W2B
SI_LocalVar | SI_0
SOUND_JQ6500_ADKEY1_BG
SOUND_JQ6500_ADKEY2_BG
SOUND_JQ6500_ADKEY3_BG
SOUND_JQ6500_ADKEY4_BG
SOUND_JQ6500_ADKEY5_BG
ms

These macros depend on me:

_LocalVar_Sound_JQ6500_BG | Sound_JQ6500_BG_Next_of_N_Reset | Sound_JQ6500_BG_Next_of_N
Sound_JQ6500_BG_PlayRandom

### _MAX_INP_CHANNEL [References: 0] Defined? True

#define _MAX_INP_CHANNEL (_INP_STRUCT_ARRAY_SIZE*4-1)

`defined @` Macros.h#14

I depend on these macros:

_MAX_INP_CHANNEL | _INP_STRUCT_ARRAY_SIZE

### _MAX_TIMER_VAL [References: 0] Defined? True

#define _MAX_TIMER_VAL 65536

`defined @` Macros.h#43

These macros depend on me:

_MAX_TIMER_VAL | _LT_MX | _ALL_LT_MX2 | _ALL_LT_MX4 | _RAND_DIV4 | _Tx2B4 | Random | ButtonFunc
Def_Neon_Misha
Flash
RandWelding
_RAND_MODE4 | Random | ButtonFunc
Def_Neon_Misha
Flash
RandWelding
_RAND_DIV2 | _Tx2B2 | RandMux | RandCntMux
_RAND_MODE2 | RandMux | RandCntMux

### _MOBALEDLIB_H_ [References: 0] Defined? True

#define _MOBALEDLIB_H_

`defined @` MobaLedLib.h#31

### _NEW_AND_OLD [References: 0] Defined? True

#define _NEW_AND_OLD (_BIT_NEW + _BIT_OLD)

`defined @` MobaLedLib.h#1189

I depend on these macros:

_NEW_AND_OLD | _BIT_NEW
_BIT_OLD

### _NOT_NR [References: 0] Defined? True

#define _NOT_NR SI_1

`defined @` MobaLedLib.h#1176

I depend on these macros:

_NOT_NR | SI_1

These macros depend on me:

_NOT_NR | NOT | DISABLE
_Herz_MoRelais_RS | Herz_MoRelais
Herz_MoRelais_I

### _OR_NR [References: 0] Defined? True

#define _OR_NR SI_0

`defined @` MobaLedLib.h#1175

I depend on these macros:

_OR_NR | SI_0

These macros depend on me:

_OR_NR | DISABLE
ENABLE
OR | PushButton2I_0_1 | PushButton2I_RGB_0_1
PushButton2I_w_LED_BL_0_1
PushButton2I_0_2 | PushButton2I_RGB_0_2
PushButton2I_w_LED_BL_0_2
PushButton2I_0_3 | PushButton2I_RGB_0_3
PushButton2I_w_LED_BL_0_3
PushButton2I_0_4 | PushButton2I_RGB_0_4
PushButton2I_w_LED_BL_0_4
PushButton2I_0_5 | PushButton2I_RGB_0_5
PushButton2I_w_LED_BL_0_5

### _PAT_DBLFL [References: 0] Defined? True

#define _PAT_DBLFL(LedCnt) ((LedCnt)==1?0b00000101: ((LedCnt)==2?0b00110011:_C_ALL_not_supported)) \

`defined @` MobaLedLib.h#1007

I depend on these macros:

_PAT_DBLFL | _C_ALL_not_supported

These macros depend on me:

_PAT_DBLFL | _Cx2P_DBLFL | BlueLight1
BlueLight2
Leuchtfeuer

### _PF_XFADE [References: 0] Defined? True

#define _PF_XFADE 0x08

`defined @` MobaLedLib.h#1038

These macros depend on me:

_PF_XFADE | XPatternT1 | DepSignal4
DepSignal4Bin
DepSignal4Bin_RGB
DepSignal4_RGB
EntrySignal3
EntrySignal3Bin
EntrySignal3Bin_RGB
EntrySignal3_RGB_BT | EntrySignal3_RGB
EntrySignal3_RGB_B
EntrySignal3_RGB_T
GleissperrsignalBin_RGB
Gleissperrsignal_RGB
HP_2_2Bin_RGB
HP_2_2_RGB
HS_5_PlusBin_RGB
HS_5_Plus_RGB
HS_5lBin_RGB
HS_5l_RGB
HS_5rBin_RGB
HS_5r_RGB
HS_EinfachBin_RGB
HS_Einfach_RGB
SingleLedSignal
SingleLedSignalEx
VorsignalBin_RGB
Vorsignal_RGB
XPatternT10
XPatternT11 | KS_Hauptsignal_Zs3_Zs1
KS_Hauptsignal_Zs3_Zs1Bin
KS_Hauptsignal_Zs3_Zs1Bin_RGB
KS_Hauptsignal_Zs3_Zs1_RGB
KS_Hauptsignal_Zs3_Zs6_Zs1
KS_Hauptsignal_Zs3_Zs6_Zs1Bin
KS_Hauptsignal_Zs3_Zs6_Zs1Bin_RGB
KS_Hauptsignal_Zs3_Zs6_Zs1_RGB
XPatternT12
XPatternT13
XPatternT14
XPatternT15
XPatternT16
XPatternT17
XPatternT18
XPatternT19
XPatternT2
XPatternT20
XPatternT21
XPatternT22
XPatternT23
XPatternT24
XPatternT25
XPatternT26
XPatternT27
XPatternT28
XPatternT29
XPatternT3
XPatternT30
XPatternT31
XPatternT32
XPatternT33
XPatternT34
XPatternT35
XPatternT36
XPatternT37
XPatternT38
XPatternT39
XPatternT4
XPatternT40
XPatternT41
XPatternT42
XPatternT43
XPatternT44
XPatternT45
XPatternT46
XPatternT47
XPatternT48
XPatternT49
XPatternT5
XPatternT50
XPatternT51
XPatternT52
XPatternT53
XPatternT54
XPatternT55
XPatternT56
XPatternT57
XPatternT58
XPatternT59
XPatternT6
XPatternT60
XPatternT61
XPatternT62
XPatternT63
XPatternT64
XPatternT7
XPatternT8
XPatternT9 | AndreaskrLT
AndreaskrLT3
AndreaskrLT3_RGB
AndreaskrLT_RGB
KS_Vorsignal_Zs3V
KS_Vorsignal_Zs3VBin
KS_Vorsignal_Zs3VBin_RGB
KS_Vorsignal_Zs3V_RGB
XPatternTE1
XPatternTE10
XPatternTE11
XPatternTE12
XPatternTE13
XPatternTE14
XPatternTE15
XPatternTE16
XPatternTE17
XPatternTE18
XPatternTE19
XPatternTE2
XPatternTE20
XPatternTE21
XPatternTE22
XPatternTE23
XPatternTE24
XPatternTE25
XPatternTE26
XPatternTE27
XPatternTE28
XPatternTE29
XPatternTE3
XPatternTE30
XPatternTE31
XPatternTE32
XPatternTE33
XPatternTE34
XPatternTE35
XPatternTE36
XPatternTE37
XPatternTE38
XPatternTE39
XPatternTE4
XPatternTE40
XPatternTE41
XPatternTE42
XPatternTE43
XPatternTE44
XPatternTE45
XPatternTE46
XPatternTE47
XPatternTE48
XPatternTE49
XPatternTE5
XPatternTE50
XPatternTE51
XPatternTE52
XPatternTE53
XPatternTE54
XPatternTE55
XPatternTE56
XPatternTE57
XPatternTE58
XPatternTE59
XPatternTE6
XPatternTE60
XPatternTE61
XPatternTE62
XPatternTE63
XPatternTE64
XPatternTE7
XPatternTE8
XPatternTE9

### _RAND_DIV2 [References: 0] Defined? True

#define _RAND_DIV2(MinTime,MaxTime) (_ALL_LT_MX2((MinTime), (MaxTime) )?1L:16L)

`defined @` Macros.h#49

I depend on these macros:

_RAND_DIV2 | _ALL_LT_MX2 | _LT_MX | _MAX_TIMER_VAL

These macros depend on me:

_RAND_DIV2 | _Tx2B2 | RandMux | RandCntMux

### _RAND_DIV4 [References: 0] Defined? True

#define _RAND_DIV4(MinTime1,MaxTime1,MinTime2,MaxTime2) (_ALL_LT_MX4((MinTime1),(MaxTime1), \
(MinTime2), (MaxTime2) )?1L:16L)

`defined @` Macros.h#50

I depend on these macros:

_RAND_DIV4 | _ALL_LT_MX4 | _ALL_LT_MX2 | _LT_MX | _MAX_TIMER_VAL

These macros depend on me:

_RAND_DIV4 | _Tx2B4 | Random | ButtonFunc
Def_Neon_Misha
Flash
RandWelding

### _RAND_MODE2 [References: 0] Defined? True

#define _RAND_MODE2(MinTime,MaxTime) (_ALL_LT_MX2((MinTime ), (MaxTime ) )?0:RF_SLOW)

`defined @` Macros.h#47

I depend on these macros:

_RAND_MODE2 | RF_SLOW
_ALL_LT_MX2 | _LT_MX | _MAX_TIMER_VAL

These macros depend on me:

_RAND_MODE2 | RandMux | RandCntMux

### _RAND_MODE4 [References: 0] Defined? True

#define _RAND_MODE4(MinTime1,MaxTime1,MinTime2,MaxTime2) (_ALL_LT_MX4((MinTime1), (MaxTime1), \
MinTime2, MaxTime2)?0:RF_SLOW)

`defined @` Macros.h#48

I depend on these macros:

_RAND_MODE4 | RF_SLOW
_ALL_LT_MX4 | _ALL_LT_MX2 | _LT_MX | _MAX_TIMER_VAL

These macros depend on me:

_RAND_MODE4 | Random | ButtonFunc
Def_Neon_Misha
Flash
RandWelding

### _Tx2B2 [References: 0] Defined? True

#define _Tx2B2(Time,OtherTime) _T2B((Time)/_RAND_DIV2((Time), (OtherTime)))

`defined @` Macros.h#51

I depend on these macros:

_Tx2B2 | _RAND_DIV2 | _ALL_LT_MX2 | _LT_MX | _MAX_TIMER_VAL
_T2B | _W2B

These macros depend on me:

_Tx2B2 | RandMux | RandCntMux

### _Tx2B4 [References: 0] Defined? True

#define _Tx2B4(Time,OtherTime1,OtherTime2,OtherTime3) _T2B((Time)/_RAND_DIV4((Time), \
(OtherTime1), (OtherTime2), (OtherTime3)))

`defined @` Macros.h#52

I depend on these macros:

_Tx2B4 | _RAND_DIV4 | _ALL_LT_MX4 | _ALL_LT_MX2 | _LT_MX | _MAX_TIMER_VAL
_T2B | _W2B

These macros depend on me:

_Tx2B4 | Random | ButtonFunc
Def_Neon_Misha
Flash
RandWelding

### __DATE__ [References: 0] Defined? True

#define __DATE__ May 4 2025

`defined @` #1

### __LEDS_AUTOPROG_H__ [References: 0] Defined? True

#define __LEDS_AUTOPROG_H__

`defined @` leds_autoprog.h#8

### __MACROS_H__ [References: 0] Defined? True

#define __MACROS_H__

`defined @` Macros.h#2

### __TIME__ [References: 0] Defined? True

#define __TIME__ 13:29:26

`defined @` #1

### sec [References: 0] Defined? True

#define sec Sec

`defined @` MobaLedLib.h#1018

I depend on these macros:

sec | Sec

These macros depend on me:

sec | Def_Neon_Misha
RGB_AmpelX_A

### sek [References: 0] Defined? True

#define sek Sec

`defined @` MobaLedLib.h#1017

I depend on these macros:

sek | Sec

## Macros Tested When Not Defined

### ARDUINO_RASPBERRY_PI_PICO [References: 1]

MobaLedLib.h: 39-1

### CONFIG_ONLY [References: 5]

MobaLedLib.h: 38-1 916-1
leds_autoprog.h: 51-1 104-3 175-1

### COPYLED_OFF [References: 1]

leds_autoprog.h: 138-1

### COPYLED_OFF_ONCE [References: 1]

leds_autoprog.h: 142-1

### LONG_LED_ADDR [References: 2]

Macros.h: 6-1 56-1

### NUM_LEDS [References: 1]

leds_autoprog.h: 16-3

### _HOUSE_STATISTIC [References: 1]

MobaLedLib.h: 60-3

### _MOBALEDLIB_H_ [References: 1]

MobaLedLib.h: 31-1

### _NEW_ROOM_COL [References: 5]

Macros.h: 675-2
MobaLedLib.h: 94-2 1417-3 1443-4 1475-4

### _USE_LOCAL_TX [References: 2]

MobaLedLib.h: 1250-3 1343-2

### _USE_SEP_CONST [References: 1]

MobaLedLib.h: 78-2

### __LEDS_AUTOPROG_H__ [References: 1]

leds_autoprog.h: 8-1

### __MACROS_H__ [References: 1]

Macros.h: 2-1

Return to Index